Region 24 700 MHz Plan Amended Dec 28, 2007

Main Section Page 1

December 28, 2007

Federal Communications Commission

Wireless Telecommunications Bureau

Chief, Public Safety and Private Wireless Division

445 12th Street, SW

Washington, DC 20554

Subject: PSHSB Docket No. 07-132, Region 24 – 700 MHz Regional Plan Revisions

Dear Sirs:

Attached is the Region 24 700 MHz Regional Plan for your review. This document is the result of the FCC decision of July 31, 2007, Report and Order released August 10, 2007, 07-132. Region 24 has modified the plan to adhere to the changes by deletion of the wideband data channels and replacement of the General Category narrowband channels.

There are four significant changes to the plan. The first change involves deletion of section 3.5, the wideband portion of the plan. The second is the revision of channel allocations to meet the new FCC band plan. No new channels were added to any county, only the frequencies changed to conform to the FCC Band Plan Public Notice, FCC 07-4163, released October 4, 2007. The third involves an administrative update to reflect changes in the individuals holding the positions of chair and vice chair. These administrative updates are reflected in section 1.1 and 1.2 of the attached plan.

Notification of this change had been provided to the Commission on August 31, 2007. The fourth removes the chart of the prior layout of the 700 MHz band in Appendix I and replaces it with the chart provided in the FCC Second Report and Order 07-132 so that it correctly reflects the revised band plan. The verbiage subsequent paragraph has been adjusted to correspond with the chart.

It is our hope that this plan will meet with your approval and allow public safety agencies in Missouri the continued access to 700 MHz spectrum. Feel free to contact me if there are any questions.

Respectfully,

/S/

Steven J. Makky, Sr.

Chairman, Region 24 RPC

by electronic submission

Region 24 700 MHz

Regional Planning Committee

Steven J. Makky, Sr.

Chairperson

St. Charles County Sheriff’s Department

Special Enforcement Bureau

Division of Emergency Management

301 N Second St., Rm. 280

St. Charles, Mo. 63301-5424

636-949-3031

smakky@sccmo.org

**Table of Contents**

**1 Declaration of Region 24 700 MHz Regional Plan**

* 1. **Regional Chairperson**
	2. **Other Regional Planning Committee Officers**

**2 Region 24 description**

**2.1 Notification Process**

**2.2 Operations of the Regional Planning Committee**

**3 Regional Plan Administration**

**3.1 Procedure for Requesting Spectrum Allotments**

**3.2 Procedure for Frequency Coordination**

**3.3 Allocation of Narrowband “General Use”**

**Spectrum**

**3.4 Low Power Channels**

**3.5 Wideband Data**

**3.6 Dispute Resolution Intra-Region**

**3.7 Priority Matrix**

**4 Process for Handling Unformed Regions**

**5 Coordination with Adjacent Regions**

**6 System Design/Efficiency Requirements**

**6.1 Interference Protection**

**6.2 Spectrum Efficiency Standards**

**6.3 “Orphaned” channels**

**6.4 System Implementation**

**7 Interoperability Channels**

**7.1 Introduction**

**7.2 Tactical Channels**

**7.3 Deployable Systems**

**7.4 Monitoring of Calling Channels**

**8 Future Planning**

**8.1 Procedures for Plan Modifications and Alterations**

**8.2 Inter-Regional Dispute Resolution Process**

**9 Certification of Region 24 700 MHz Regional Plan**

**Appendices**

**Appendix A Bylaws**

**Appendix B Region 24 Members, Agencies, Contact Information and**

**Voting Status**

**Appendix C Region 24 (Missouri) Counties**

**Appendix D List of Meetings, summaries of minutes, agendas**

**Appendix E 700 MHz Interoperability channel nomenclature**

**Appendix F NCC 700 MHz Pre-Assignment Rules/Recommendations**

**Appendix G Region 24 Channel allotments**

**Appendix H Inter Regional Dispute Resolution Agreement**

**Appendix I DTV Protection and Incumbency**

**Appendix J Meeting Announcements, Notes etc**

**1 769-775/799-805 MHz Regional Plan for Region 24 (Missouri)**

This document is the Regional Plan for Region 24 (Missouri) describing how the 769-775/799-

805 MHz General Use frequencies will be allocated and implemented in the Region.

**1.1 Regional Chair**

The Chairperson of Region 24 is Steven J. Makky, Sr. His information is below:

Steven J. Makky, Sr.

St. Charles County Sheriff’s Department

301 N Second St., Rm. 280

St. Charles, Missouri 63301-5424

Phone 636-949-3031

FAX 636-949-3021

Email smakky@sccmo.org

**1.2 Other RPC Officers and full RPC Membership**

The Vice Chairman/Secretary of Region 24 is Stephen T. Devine. His contact information is below:

Mr. Stephen T. Devine

1018 Fairmount Blvd.

Jefferson City, Missouri 65101

Email stephendevine@mchsi.com

Phone 314-223-2191

The duties of Treasurer within Region 24 are assigned to Stephen T. Devine, Regional Vice Chairman.

Membership in the Region 24 Regional Planning Committee is open to any interested party. Committee Officer requirements, voting procedures and membership attendance requirements are listed in the Region 24 Planning Committee bylaws. Appendix A contains the Region 24 bylaws. Appendix B is a list of Region 24’s initial members, their agency/affiliation and voting status. Voting and operating procedures are described in Section 2.2 of this plan.

**2 Region 24 Description**

Region 24 encompasses the entire state of Missouri, consisting of 114 counties and the City of

St Louis, which does not reside within a Missouri county. An alphabetical list of the individual

counties can be found listed in **Appendix C**.

The State of Missouri has diverse geography along with a varied population base. Ground

elevations in Missouri vary from 70 meters AMSL in the Mississippi Delta of extreme southeast

Missouri to 500 meters AMSL in the Missouri Ozarks along the Arkansas border. The terrain

of northern Missouri is relatively flat with sparsely populated areas, allowing for effective radio

propagation. Throughout southern Missouri, however, varying ground elevations along with

some of the worlds largest concentrations of lead, iron and other mineral deposits create a

challenge to agencies in the Region attempting to develop efficient radio networks in any

frequency band.

Missouri’s roadways are some of the most frequently traveled in the country. The number of

vehicles traveling Missouri roadways in 2002 amounted to well over seven (7) times its existing

population of 5.8 million. These itinerant travelers take a heavy toll on all Missouri public

safety agencies.

The population of Missouri is 5.8 million people (Census January 2001). Over 80 percent of

this population is concentrated in the St Louis and Kansas City Metropolitan areas. These two

large metropolitan areas are made up in part or all of 35 counties. These areas are adjacent to

both Region 13 and Region 16 (Southern Illinois and the State of Kansas, respectively) and

require Missouri to obtain inter-state frequency coordination with both Regions when

attempting any frequency assignments in these densely populated areas.

Other areas in Missouri consist of small concentrated pockets of population surrounded by areas

of sparse population or with large amounts of unpopulated U.S. federal forest. These diverse

demographics, combined with the RF propagation difficulties stated above, make for

challenging frequency allotments. Previously, frequency allotments in areas of Region 24

adjacent to Regional areas other than those listed above have been successful primarily due to

the sparse population near each Regional border. Region 24 (State of Missouri) has eight (8)

adjacent Regions. They are as follows:

Region 13 Southern Illinois

Region 17 State of Kentucky

Region 39 State of Tennessee

Region 4 State of Arkansas

Region 34 State of Oklahoma

Region 16 State of Kansas

Region 26 State of Nebraska

Region 15 State of Iowa

In previous NPSPAC 821 MHz frequency allotments, spectrum amounts disproportionate to

population densities were allocated due to differing methodologies used in adjacent NPSPAC

Regions and the timing of adjacent regions plan approval. This resulted in a minimum number

of channels available for Region 24, particularly in the Kansas City and St. Louis areas. In the

700 MHz band, county allotments for both narrowband and wideband channels have been

developed based on population densities relative to adjacent Regions. Due to the Region’s

diverse population densities and the scarce spectrum resources in Missouri’s populated areas, it

is anticipated the majority of requests for voice/data spectrum will be from the Kansas City and

St Louis metropolitan areas, which both currently operate existing 800 MHz radio networks.

It is anticipated that other areas within Region 24, including areas in the Southwestern parts of

Missouri, may request 700 MHz channels from established county pool allotments to either expand

existing 800 MHz systems or develop new 700 MHz systems

***2.1 Notification Process***

821 MHz Region 24 Chairperson, Stephen T. Devine, appointed Ron Shook of Greene County

700 MHz Convenor on July 1, 2000. A 700 MHz Regional Planning Committee meeting date

was set for October 5, 2000. Interested parties were given 90 days notice prior to the first

meeting. Announcements indicating the date, time and location of the first meeting were sent

by mail to the FCC Wireless Telecommunications Bureau and, posted in the following

industry periodicals: MRT Magazine, Radio Resource Magazine and the Association of Public

Safety Communications Officials, Inc. magazine. The meeting information was also posted

on the Missouri Uniform Law Enforcement System (MULES) Teletype network and received

by all law enforcement agencies in both Missouri and the surrounding Regions. The Missouri

State Highway Patrol also issued a press release regarding the convening of the committee and

including the first meeting information. This awareness allowed for the dissemination of

meeting information to hundreds of law enforcement agencies, public safety agencies and

news media throughout Missouri and the eight (8) adjacent states to Missouri. The Missouri

State Emergency Management Agency, along with the Missouri National Guard was

contacted and notified of the convening of the 700 MHz Regional Planning Committee. The

convener also contacted several agencies via email that expressed interest in the planning

process prior to the meeting. There are no Native American tribal reservations located within

Region 24. Copies of the announcements sent to the FCC, any Public Notices released

relating to Region 24’s meeting, the ads placed in the industry periodicals, the Missouri SHP

press release, and emails sent to interested agencies are included in Appendix D. The 700

MHz first meeting convened on October 5, 2000 by Ron Shook. Stephen T. Devine was

elected the Chairperson of the Region 24 700 MHz Regional Planning Committee. Mr. Steve

Makky, Sr. of the St Charles County Emergency Management Agency was elected to the

position of Vice Chairperson/Secretary of the Region 24 700 MHz Regional Planning

Committee. The FCC did not issue a Public notice for this meeting.

*2.2 Operations of the Regional Plan Committee*

This committee will use Robert’s Rules of Order to conduct meetings. All decisions will be

by clear consensus vote with each Public Safety Agency in attendance having one (1) vote.

Additional voting member considerations are listed in the Region 24 Bylaws, Appendix A.

The meetings are open to all interested persons and public input time is provided for anyone

to express a viewpoint or to have input to the Regional Planning process.

Subcommittees have been formed as needed to work on specific issues. For the initial

planning of Region 24, three subcommittees were formed:

**Implementation, Interoperability, and Technology Subcommittees**: These

subcommittees are intended to work on the details of specific issues and make

recommendations to the full committee for the development of the Region 24 Regional plan.

Any changes to the Regional plan must be voted and approved by the full Regional Planning

Committee. Participation in subcommittees is open to any member. The Chair of the

Regional Planning Committee appoints each Subcommittee Chair. The Region 24

subcommittees are listed below. Subcommittee participation is open to the entire

membership, with the Chairpersons responsible for ensuring the content and atmosphere of

the plan best represents the region as a whole.

**Technology** Steve Makky, Sr. St Charles County Emergency Management,

**Chairperson**

Charles Gastler, St Louis City Police Department, Member

Thomas Kearns, Tyco/MA-Com, Commercial Member

Roger Strope, Missouri State Highway Patrol, Member

Jon Martin, Motorola Commercial Member

**Interoperability** William Cade, Jasper County 911, **Former Chairperson** (Moved from

Region 24 in Spring 2002 to the State of Florida and Ron Shook, Greene

County Emergency Management was appointed Interoperability

Subcommittee Chairperson by the Regional Chair).

Ron Shook, Greene County Emergency Management **(Chairperson)**

Stephen T. Devine, Missouri State Highway Patrol

**Implementation** Stephen T. Devine, **Chairperson**

Roger D. Strope, Missouri State Highway Patrol

A minimum of two (2) full committee meetings will be held every twelve months. When

possible, meetings will be held in the months of April and October. The Region 24

Chairperson has the authority to call an additional meeting at a time when he/she deems

necessary or when he/she deems it in the best interest of the Region to convene**.** In an

attempt to offer as many people as possible the opportunity to contribute to the Regional 700

MHz Planning Committee, one (1) of the two meetings will be held in various locations

within Region 24 and due to its central location, the remaining meeting will be held in

Jefferson City, Missouri.

The Region 24 700 MHz list-serve, http://groups.yahoo.com/group/RPC24/ was created in

July of 2001. The Region 24/Missouri public safety communications list serves,

**http://groups.yahoo.com/group/NPSPACRegion24/,**

**http:**//**groups.yahoo.com/group/rpc24**

**http://groups.yahoo.com/group/region24siec**

**http://groups.yahoo.com/group/moapco911**

All were created in 2000 to exchange information as well as disseminate original meeting

times, dates and agendas throughout the Regional Planning process for the initial 700 MHz

meeting and subsequent Region 24 (Missouri) SIEC meetings. These list serves are utilized

to disseminate messages on regional planning progress and meeting agendas and serves as

an excellent historical resource for regional planning development.

Beginning two years after Federal Communications Commission approval of this Regional

Plan, the Chairperson shall call a meeting of the Regional Planning Committee to elect a

Chair, Vice Chair and Secretary to serve for a two-year term. There is no limit to the

number of terms that may be served by officers of the 700 MHz Regional Planning

Committee.

If the Chair is unable to serve a complete term, the Vice Chair will serve as Chair until the next

700 MHz Regional meeting. If both the Chair and Vice Chair are unable to serve their full

terms, one or the other should make an effort to call a special meeting of the Committee to

elect replacements. If for some reason, neither the Chair nor the Vice Chair can call the

special meeting; the State or any County within the Region may call for a special meeting,

giving at least 5 days notice, to elect replacements.

A chronological list of meetings, summary of minutes, meeting announcements and agendas

outlining Region 24 progress in 700 MHz development is located in **Appendix D** of this

document.

**3 Regional Plan Administration**

*3.1 Procedure for Requesting Spectrum Allotments*

A. Upon FCC approval of this Plan, Region 24 will announce to the region that 700 MHz

public safety channels are available in the Region and that channels have been assigned to

pool allotments to counties within the Region. All available methods will be used to notify

public safety entities of channel availability in the Region (see Section 2.1). All requests will

be considered on a first come, first served basis. Region 24 supports the National

Coordination Committee Pre-Assignment Rules and Recommendations listed in Appendix F,

and will use these guidelines as a template to determine if an application submitted to the

Regional Planning Committee meets Regional Planning standards. It is recommended that

applicants familiarize themselves with these recommendations prior to submitting

applications for Region 24 700 MHz public safety system implementation. In order to

maintain accurate records in the CAPRAD database, applicants will provide Region 24 with

physical copies of their application along with associated documentation for Regional

Planning Committee review. The Regional Planning Committee will enter the FCC 601 form

into the CAPRAD database before the application is forwarded to the FCC certified

coordinators.

In general and unless otherwise noted, the Region 24 Regional Planning Committee will

adhere to the published National Coordination Committee Implementation Guidelines for 700

MHz Public Safety Regional Planning Committees.

B. When applying for new 700 MHz channels, the Regional Planning Committee looks forward

to 700 MHz applicants working with neighboring agencies to promote and continue the

establishment of interoperability within their community and allow for the equitable

distribution of existing spectrum allocations to promote efficient frequency use when applying

for 700 MHz spectrum. Region 24 expects applicants to be cognizant of the fact that moving to

the 700 MHz band may create a degree of isolation between themselves and neighboring

agencies, and Region 24 looks forward to working with these applicants on a case-by-case

basis on how to maintain spectrum availability in their area, while continuing to promote

interoperable communications.

C. To request channels from Region 24, a full application package must be submitted to the

Regional Planning Committee in physical written form for entry by Region 24 personnel in

the CAPRAD database http://caprad.nlectc.du.edu/login/home. The application must include:

An FCC Form 601,

A short description of the proposed system,

A justification for the additional spectrum,

An interference prediction map using the current version of TIA/EIA TSB 88 guidelines,

Maps showing all interference predicted in the proposed system,

Documents indicating agency-funding commitments sufficient to fund the development of the

proposed system(s) and an indication as to when they will migrate from their existing system

to the new system.

D. The Chair will distribute the request to all other agencies with allotments in the plan for

review and approval electronically. Absent a protest, the Regional Planning Committee will

approve the application and (if applicable), upon receipt of a ‘cancellation consent letter’

(See Section 3.1 B. above), submit it, through the CAPRAD database, to the applicant’s

preferred FCC-certified frequency coordinator for processing. This process meets the

requirements of Rule 90.176 (c).

The CAPRAD database will reflect the approved application and place the channels for the

proposed system in “pre-license” status.

E. Allocation Disputes: An agency may protest a proposed system within 30 calendar days

of the original distribution. Protests will only be considered if the allocation does not

conform to plan criteria or objecting agency or the Chairperson can show harmful

interference is likely based on the information submitted by the agency requesting the new

allocation. If an agency with pre-licensed/Region approved co-channel or adjacent channel

allocations objects to a proposed allocation due to concerns about potential interference, the

objecting agency may request field tests be done to confirm or refute interference potential.

The completion of these field tests will be required for Regional application approval.

Coverage area service/interference contours of the proposed system(s) should meet values

designated in Section 6.1 of this document. Any costs associated with field tests or any other

requirement to obtain Region 24 plan approval are the responsibility of the agency

submitting application to Region 24.

The parties involved must resolve the allocation dispute and notify the Region Chair within

14 calendar days. If the parties involved cannot resolve the allocation dispute within that

timeframe, then a special full Committee meeting will be scheduled to consider and vote on

the protest. If approved, the application will be submitted through the CAPRAD database to

the applicant’s chosen FCC-certified frequency coordinator for processing

F. **Lower Power "Campus Eligible" General Use Channels**: In the implementation of

700 MHz public safety spectrum throughout Region 24, there may be opportunities for

increased channel reuse when developing radio systems for "campus" type operations.

Examples of those who may capitalize on this opportunity include hospitals, stadiums, malls

or places of public gathering, public universities, transit systems and ports. While these

channels have been designated in county pool allotments with proper designations, they do

not enjoy the benefits of countywide channels in that they are not cleared for usage over a

wide area. In many instances, facilities require a smaller or more specific geographical

coverage area than assumed in the initial channel packing plan and may be able to be reused

more efficiently. These "campus" type systems also, in many cases, require in-building or

confined space/ tunnel radio coverage or communications along a linear pathway, such as a

maintenance or right of way. Public safety channels can be allotted to this type operation in

a region and can lead to effective system development, along with increased spectral

efficiency, if power levels and Area of Protection (AOP) of the area are taken into account

in system planning. These parameters must be established appropriate to the area of

coverage. In order to facilitate this effective method of system implementation, channels

have been identified in certain areas of Region 24 that may be utilized in a smaller service

area. These channels are NOT eligible to be utilized throughout the county they are allotted

to and the following criteria must be adhered to when requesting channels from Region 24

for operations of this type:

The 50dBu service contour of the proposed system must not exceed an area more

than 2 miles from the proposed service area. When this 2-mile distance extends to an

adjacent region, the applicant must obtain concurrence from the adjacent region. Reduced

external antenna height, along with reduced ERP, directional antennae,

distributed antenna systems, radiating "leaky coax," are all tools that should be utilized in

the development of these type systems. Region 24 will ensure the development of these

type of systems will in no way interfere with co-channel or adjacent channel users within

Region 24 or Region 24's adjacent regions. The Chairperson, or a majority of the members

of the region, has the authority to request and require engineering studies from the

applicant that indicate no harmful interference will be introduced to any co-channel or

adjacent channel existing user prior to application approval. For 12.5/25 kHz co-channel

assignments, the 50dBu service contour of the proposed stations will be allowed to extend

beyond the defined service area for a distance no greater than 2 miles. An

adjacent/alternate 12.5/25 kHz channel shall be allowed to have its 60 dBμ (50,50) contour

touch, but not overlap the 40dBμ service (50,50) contour of an adjacent/alternate system

being protected. Evaluations should be made in both directions to ensure

compliance. The approval of systems utilizing county allotment channels labeled

“Campus”, are subject to approval of the Region 24 700 MHz regional planning

committee. They are the final authority on parameters associated with “campus” type

operations.

If Region 24 receives an application for low power fixed use and the proposed service

contour encroaches onto an adjacent region prior to the channel allotted to the region

being implemented in a specific system, the application must be modified so the service

contour does not encroach into the adjacent region **or** the applicant must supply the Region

24 700 MHz Regional Planning Committee with written concurrence from the adjacent

region permitting the original design.

*3.2 Procedure for Frequency Coordination*

The Region 24 Planning Committee will adhere to the National Public Safety

Telecommunications Council’s (NPSTC) 700 MHz General Use channel sort as shown on

the CAPRAD database for narrowband General Use channels. The Region created its own

sort for the wideband data channels. (See Appendix G). Region 24 will participate in the

CAPRAD database and keep the Regional Plan and current frequency allotment/allocation

information on the database. The Region 24 Regional Planning Committee has both the

ability to accept recommendations from the committee and, if approved, the authority to

change the original frequency allotment. In order to keep the most current frequency

allotments within Region 24, an annual review of the allotments will be made at one of the

scheduled meetings by the full committee and recommended changes to the plan will be

voted on. The majority of members in attendance at a meeting of the full Regional Planning

Committee must approve any changes to the Regional allotments. If at any time a system is

allocated channels within Region 24 and the system cannot be developed within the agreed

upon guidelines (slow growth), the channels will be returned to the county pool allotments

they originated from and again be available to other agencies in the region. If plan

modifications are approved, the Chairperson will, if necessary, obtain adjacent Region

approval and file a plan amendment indicating the approved changes with the Federal

Communications Commission.

*3.3 Allocation of Narrowband “General Use” Spectrum*

The Region 24 Technology Subcommittee recommends that allotments be made on the basis

of one 25 KHz channel for every two (2) voice channel requests and one 12.5 KHz channel for

each narrowband data channel request. This recommendation is approved by the full

Committee and is part of this plan. Allotments will be made in 25 KHz groups to allow for

various digital technologies, at various bandwidths, to be implemented. All agencies

requesting spectrum during the initial filing window (see Section 3.1) will be allocated

channels if plan requirements are met. Agencies using Frequency Division Multiplexing

(FDMA) will be expected to maintain 12.5 KHz equivalency when developing systems and

will be required to utilize BOTH 12.5 KHz portions of the 25 KHz block. In most cases, this

will require the geographic separation of each 12.5 KHz adjacent channel. In order to

promote spectrum efficiency, Region 24 will ensure that systems allocated 25 KHz channel

blocks will utilize all of the channel and not “orphan” any portions of a system designated

channel. (See Section 6.3)

The Region 24 700 MHz Regional Planning Committee will be the final authority on the

approval of applications for 700 MHz General Use channel allocations.

***3.4 Low power Channels***

The FCC in the 700 MHz band plan set aside channels 1 - 8 paired with 961 – 968 and 949 –

958 paired with 1909 – 1918 for low power use for on-scene incident response purposes using

mobiles and portables subject to Commission-approved Regional Planning Committee

Regional Plans. Transmitter power must not exceed 2 watts (ERP).

Channels 9 –12 paired with 969 – 972 and 959 – 960 paired with 1919 – 1920 are licensed

nationwide for itinerant operation. Transmitter power must not exceed 2 watts (ERP).

These channels may operate using analog operation. To facilitate analog modulation, this

plan will allow aggregation of two 6.25 KHz channels for 12.5 kHz bandwidth. On scene

temporary base and mobile relay stations are allowed (to the extent FCC rules allow) antenna

height limit of 6.1 meter (20 feet) AGL (Above Ground Level). However, users are

encouraged to operate in simplex mode with the least practicable amount of power to reliably

maintain communications whenever possible. This plan does not limit use to analog only

operations and channels are intended for use in a wide variety of applications that may require

digital modulation types as well. The use of EIA/ TIA-102, Project 25 Common Air Interface

is required when using a digital mode of operation.

In its dialog leading up to CFR §90.531 allocating the twenty-four low power 6.25 kHz

frequency pairs (of which eighteen fall under RPC jurisdiction)1, the Federal Communications

Commission (FCC) suggested that there is a potential for multiple low power applications, and

absent a compelling showing, a sharing approach be employed rather than making exclusive

assignments for each specific application as low power operations can co-exist [in relatively

close proximity] on the same frequencies with minimal potential for interference due to the 2

watt power restriction.

1 See paragraphs 35 through 39 in FCC’s Third Memorandum Opinion and Order for WT Docket No. 96-86 adopted

September 18, 2000.

Whereas advantages exist in not making assignments, the reverse is also true. If, for example,

firefighters operate on a specific frequency or set of frequencies in one area, there is some

logic in replicating that template throughout the Region for firefighter equipment. If there are

no assignments, such a replication is unlikely.

In seeking the middle ground with positive attributes showing up both for assignments and no

assignments, we recommend the following regarding assignments associated with the eighteen

(18) low power channels for which the Regional Planning Committee has responsibility:

• Generic - Channel #’s 1-4 and 949-952 are set aside as generic 2 watt channels for use by

public safety agencies operating within Region 24, and the complementary mobile channels

# 961-964 and 1909-1912 are set aside as 2 watt generic mobile channels also for use by

public safety agencies likewise operating within Region 24.

• Fire/ EMS/ Consequence Management - Channel #’s 5-8 are designated as Fire Protection/

Emergency Medical and Consequence Management 2 watt channels for licensing and

exclusive use by the Fire/Emergency Medical disciplines, and the complementary mobile

channel #’s 965-968 are set aside as Fire/Emergency Medical and Consequence

Management 2 watt mobile channels also for licensing and exclusive use by the

Fire/Emergency Medical disciplines.

• Law/ Crisis Management - Channel #’s 953-956 are set aside as Law Enforcement/Crisis

Management 2 watt channels for licensing and exclusive use by the Law Enforcement

discipline, and the complementary 2 watt mobile channel #’s 1913-1916 are set aside as Law

Enforcement/Crisis Management mobile channels also for licensing and exclusive use by the

Law Enforcement discipline.

Multidisciplinary Joint Public Safety Operations - Channel #’s 957-958 are set aside as

Multidisciplinary Joint Public Safety Operations 2 watt channels for licensing and the

complementary 2 watt mobile channel #’s 1917-1918 are also set aside as Multidisciplinary

Joint Public Safety Operations Channels for use by political subdivisions and public safety

agencies operating under a unified command at a common incident for the express mission of

safety of life, property or environment.

Simplex operations may occur on either the base or mobile channels. Users are cautioned to

coordinate on scene use among all agencies involved, particularly when the use of

repeaterized modes is possible at or in proximity to a common incident. Users should license

multiple channels and be prepared to operate on alternate channels at any given operational

area. Again, Region 24 Regional Planning Committee will recommend to the Missouri SIEC

that all 700 MHz users and applicants to have **the capability to access** ALL of the thirty-two

(32) NCC approved interoperability channels in both duplex and simplex modes. Under no

circumstances may a user claim a channel as exclusively theirs; all 700 MHz interoperability

channels are under the administration of the Missouri Statewide Interoperability Executive

Committee.

*3.5 Wideband Data*

This section was deleted due to the FCC Second Report and Order, 07-132 released August

10, 2007.

However, if any entity desires to implement either a wideband (50 kHz – 150 kHz) or

broadband data system, they may contact the Public Safety Broadband Trust as set forth in

FCC 07-132 Second Report and Order and subsequent information released by the FCC and

PSBT.

Four General Use 6.25 kHz channels may still be combined to form one 25 kHz data channel.

*3.6 Dispute Resolution – Intra-Regional*

In the event an agency disputes the implementation of this plan or the Federal

Communications Commission approval of this plan or parts of this plan, the agency must

notify the Chair of the dispute in writing. This section does not apply to protests over new

spectrum allocations (see Section 3.1). The Chair will attempt to resolve the dispute on an

informal basis. If a party to the dispute employs the Chair, then the Vice Chair will attempt

resolution. In such cases, the Chair shall be deemed to have a conflict of interest and will be

precluded from voting on such matters. If after 30 days the dispute is not resolved, the Chair

(or Vice Chair) will appoint a Dispute Resolution Committee consisting of a member from the

State of Missouri and at least five members from the Counties in Region 24. That committee

will select a Chair to head the committee.

The Regional Plan Chair (or Vice Chair) will represent the Region in presentations to the

Dispute Resolution Committee. The Committee will hear input from the disputing agency,

any effected agencies and the Region Chair. The Committee will then meet in executive

session to prepare a recommendation to resolve the dispute. Should this recommendation not

be acceptable to the disputing agency/agencies, the dispute and all written documentation

from the dispute will be forwarded to the National Association of Regional Planning

Committee for dispute resolution. As a last resort, the dispute will be forwarded to the Federal

Communications Commission for final resolution.

3.7 *Priority Matrix*

In the event that spectrum allocation requests conflict and cannot all be accommodated, the

following matrix will be used to determine priority for allotment. This matrix will only be used if

two requests are received in the same time frame for the same number of channels. Otherwise, the

first come first served procedure of Section 3.1 will be used.

• Priority is given to users fundamentally involved with the protection of Life and

Property (15 points)

• Priority is given to multi-agency systems that promote multiple jurisdictional, multiagency,

inter-discipline interoperable communications within a sub-regional area.

These systems can be either a group of separate departments within a large agency or

groups of agencies operating together under a large blanket agency, or a combination

of both. (25 points)

• Documentation of proposed funding to construct the system using these 700 MHz

frequencies must be available and accompany the original spectrum request. (25

points)

• The submission of some form of proof of financial commitment, accompanied by a

RFP (Request for Proposal) outlining the design of the proposed system and

detailing the development of the requested channels will be required to be submitted

to the Regional Planning Committee prior to approval. (35 points)

If there are more applicants than frequencies available for a given area, the above criteria will be

used to grade each application before the committee.

This process, if required, will be treated as a dispute and the procedures outlined in Section 3.6

using the above criteria will be used to allocate the frequencies.

**4 PROCESS FOR HANDLING UNFORMED REGIONS**

The Implementation Subcommittee recommends that all Regions use the following pre-planning

methodology to facilitate coordination with adjacent Regions. This procedure will provide a

spectrum allotment for adjacent Regions that do not immediately form a Committee.

Counties or other geographic subdivisions within 70 miles of the Regional border need to share

spectrum with the adjacent Region(s). The sharing indicated is inherent in the NPSTC Packing

Program, as it views all counties nationwide as separate entities while ignoring state borders. With

all criteria being equal, this ensures all counties are provided sufficient spectrum in accordance with

their surrounding counties. The appropriate ratio of channels shall be allotted to counties in

adjacent Regions based upon each county’s population. A 25 kHz building block will be used to

distribute spectrum between the Regions. A description of the demographics of the affected border

areas shall be included.

The requirements for adjacent Region concurrence will require a waiver if the adjacent Region has

not yet formed. The Region filing the Plan must use the pre-planning procedure outlined above.

The waiver request must be filed concurrently with the Plan and contained in the cover letter.

**5. Coordination with Adjacent Regions**

The Regions adjacent to Region 24 are listed below:

Region 13, **Southern Illinois**

Region 17, **Kentucky**

Region 39, **Tennessee**

Region 4, **Arkansas**

Region 34, **Oklahoma**

Region 16, **Kansas**

Region 26, **Nebraska**

Region 15, **Iowa**

Region 24 has coordinated channel allocations and received concurrence with all its bordering

Regions by providing copies of the Region 24 plan (including channel allotments) to each

adjacent Region using the CAPRAD database and by mailing hard copies of the Plan to the

adjacent Region’s Chairperson or Convener.

Region 24’s borders with Region 4 and Region 34 are sparsely populated and generally, the

existing NPSPAC 821/866 MHz band frequencies are not built out on either side of these

regional border areas with Region 24. The east central and west central Region 24 borders,

with Region 13 and Region 16 respectively, are some of the most urban densely populated

areas of Missouri, while Region 24’s borders with Region 34 (Oklahoma), Region 26

(Nebraska), Region 39 (Tennessee), Region 4 (Arkansas), Region 15 (Iowa) and Region 17

(Kentucky) are some of the most rural, sparsely populated areas in the Midwest. The

CAPRAD database and its associated packing plan will provide minimum channel

allotments for all of Region 24’s bordering regions. This method was recommended by the

NCC Implementation Subcommittee as a way to assure that adjacent Regions, which did not

enter the Regional Planning process immediately, would not find all frequencies assigned in

their borders.

Therefore, adjacent Regions 4, 34, 16, 15, 26, 13, 17,and 39 should all be able to satisfy

voice and narrowband data requests along their border areas with Region 24. However, if

an adjacent Region has difficulties satisfying intra-regional requests due to channel

allocation within Missouri, this committee pledges to work with that adjacent Region to

resolve any issues that might hinder interoperability or reduce any benefit to public safety

communications.

**6. System Design/Efficiency Requirements**

*6.1 Interference Protection*

The frequency allotment list in Missouri’s counties result from the fact that the original

frequency sort did not anticipate high site system development that placed a priority on few

sites all operating at high ground elevations providing weak signal strength at the edge of a

jurisdictions coverage area. Rather, the sort utilized contours to maximize frequency re-use

across the country. This is based on an assumption that systems will be engineered on an

interference-limited basis, not a noise floor-limited basis. Agencies are expected to design

their systems for maximum signal levels within their coverage area and minimum levels in the

coverage area of other co-channel users. Quality system engineering, the use of directional

antennae and the advocacy of multi-agency/multi-discipline systems that promote

interoperability can accomplish this goal. A jurisdictions coverage area is normally the

geographical boundaries of the Agency(s) served plus a three to five mile area beyond.

Systems should be designed for minimum signal strength of 40 dBμ in the system coverage

area while minimizing signal power out of the coverage area. TIA/EIA TSB88-A (or latest

version) will be used to determine harmful interference assuming 40 dBμ, or greater, signal in

all systems coverage areas. This may require patterned antennas and extra sites compared to a

design that assumes noise limited coverage. Region 24 complies with National Coordination

Committee recommendations listed in Appendix K of the Regional Planning Committee

Guidelines published by the National Coordination Committee (NCC).

6.2 *Spectrum Efficiency Standards*

Initial allotments will be made on the basis of 25 kHz channels. To maximize spectrum

utilization, prudent engineering practices and receivers of the highest quality must be used in

all systems. Given a choice of radios to choose from in a given technology family, agencies

should use the units with the best specifications. This plan will not protect agencies from

interference if their systems are under-constructed (ie; areas with the established service area

having minimum signal strength below 40 dBu), or the systems utilize low quality receivers.

The applicants implementation of prudent engineering practices will be encouraged by the

Regional Planning Committee at all times.

It is the eventual goal of the FCC and the public safety community for radio equipment to

meet the requirement of one voice channel per 6.25 KHz of spectrum. When applying for

channels within Region 24, the applicants should acknowledge the deadline for converting all

equipment to 6.25 kHz or 6.25 kHz equivalent technology is 12/31/2016. For narrowband

mobile data requests, one mobile data channel will consist of two (2) 6.25 KHz channels/one

(1) 12.5 KHz channel. Narrowband 6.25 KHz channels can be aggregated for data use to a

maximum bandwidth of 25 KHz. As 6.25 KHz migration evolves, an agency that creates any

“orphaned” 6.25 KHz channels should realize that these channels would be allocated to nearby

agencies requesting channels to maintain consistent grouping and utilization of 25 KHz blocks

within the region. (See Section 6.3)

Region 24 encourages small agencies to partner with other agencies in multi-agency or

regional systems as they promote spectrum efficiency and both small and large agency

capacity needs can be met. Loading criteria can also be achieved in multi-agency systems that

will allow greater throughput for all agencies involved than that which could be achieved

individually.

*6.3 Orphaned Channels*

The narrowband pool allotments with Region 24 will have a channel bandwidth of 25 kHz.

These 25 kHz allotments have been characterized as “Technology Neutral” and flexible

enough to accommodate multiple technologies utilizing multiple bandwidths. If agencies

choose a technology that requires less than 25 kHz channel bandwidth for their system, there

is the potential for residual, “orphaned channels” of 6.25 kHz or 12.5 kHz bandwidth

immediately adjacent to the assigned channel within a given county area.

An orphan channel may be used at another location within the county area where it was

originally approved, if it meets co- and adjacent channel interference criteria. Region 24

will utilize **“county areas”** as guidelines for channel implementation with the area of

Region 24. The definition of **“county area”** in this plan is the geographical/political

boundaries of a given county, plus a distance of up to 15 miles outside of the county.

If the channel, or a portion of a channel, is being moved into a “county area” that is within

30 miles of an adjacent region, Region 24 will receive concurrence from the affected region.

By extending the “county area” by a designated distance, it is anticipated this will increase

the possibility that orphaned channel remainders will still be able to be utilized within the

“county area” , and reduce the potential for channel remainders to be forced to lay dormant

and used with a county channel allotment. These movements will be documented on the

National Public Safety Telecommunications Council CAPRAD database.

If the “orphaned channel” remainder does not meet co-channel and adjacent channel

interference criteria by moving it within the “county area” as listed above, and it is

determined by the region that the “orphaned channel” cannot be utilized in the region

without exceeding the distance described in the “county area” listed above, Region 24 will

submit a plan amendment to the FCC to repack the channel to a location where its potential

use will maintain maximum spectral efficiency. This FCC plan amendment will require

affected region concurrence.

When in the best interest of public safety communications and efficient spectrum use within

the Region, the Region 24 Regional Planning Committee shall have the authority to move

orphan channel allotments, and/or co-/adjacent-channel allotments affected by the

movement of orphan channels, within its “county areas”, which are defined above. This is to

retain spectrum efficiency and/or minimize co-channel or adjacent channel interference

between existing allotments within the region utilizing disparate bandwidths and

technologies.

***6.4 System Implementation***

TV station KSMO, located in Kansas City, Missouri utilizes analog TV channel 62. Channel

62 is adjacent to 700 MHz public safety allocations and the frequency sort in the Kansas City

area of Region 24 will include channels that can co-exist with TV channel 62 and channels

that cannot to prepare for implementation when the KSMO has left the band. The Region 24

Regional Planning Committee will utilize NCC Implementation Subcommittee documentation

titled **Appendix L “DTV Transition**” that will provide the criteria which will be used, per

FCC rules, to protect existing TV stations from land mobile use on 700 MHz public safety

channels. All other areas in Region 24 (State of Missouri) are capable of immediately

implementing systems using any 700 MHz public safety channels. With no restrictions in

implementation due to incumbent co-channel broadcasters in the region, implementation of

systems will adhere to guidelines in FCC rule 90.529 (b) and (c). An Agency may file a

request with the Regional Chairperson for an extension of time to implement. The request

should include all details describing why the agency has not implemented and a new

implementation schedule. If necessary, the Regional Chairperson will call a special meeting

to determine if the allotment should be extended or if the agency should reapply to the

committee for another allotment.

**7. Interoperability Channels**

***7.1 Introduction***

The ability for agencies to effectively respond to mutual aid requests directly depends on their

ability to communicate with each other. Missouri is subject to many natural disasters and

contains regions and facilities, which may be susceptible to a man-made disaster or weapons

of mass destruction attack. Mutual aid should be encouraged among agencies. This Plan

seeks to facilitate the communications necessary for effective mutual aid.

The State of Missouri will administer the Missouri Statewide Interoperability Executive

Committee; and the Missouri Statewide Interoperability Executive Committee (SIEC) under

National Coordination Committee’s (NCC) guidelines will administer the 700 MHz

interoperability channels. The Region 24 700 MHz Regional Planning Committee will work

with the Missouri State Interoperability Executive Committee and three (3) members of the

Region 24 700 MHz Regional Planning Committee will participate in the Missouri State

Interoperability Executive Committee (SIEC) representing Region 24. If at any time the State

SIEC is unable to function in the role of administering the interoperability channels in the 700

MHz band, then this committee will assume this role and notify the FCC in writing of the

change in administrative duties. See the NCC Implementation Subcommittees **Table of**

**Interoperability Channels in Appendix “E”**

***7.2 Tactical Channels***

Due to the immediate availability of 700 MHz public safety channels in Missouri, Region 24

will not set aside additional channels for interoperability use within the region. It is

anticipated the sixty-four FCC designated interoperability channels (6.25 KHz) will be

sufficient to provide interoperability (voice and data) within Region 24.

All mobile and portable units operating under this Plan and utilizing 700 MHz channels must

be programmed with the minimum number of channels called for either in NCC guidelines or

as the Missouri State interoperability Executive Committee specifies. The channel display in

these radios will be in accordance with the NCC guidelines that have common alphanumeric

nomenclature to avoid any misinterpretation of use within Region 24. The Missouri SIEC is

the final authority, in Missouri, on the interpretation of the distribution of the 700 MHz

interoperability channels.

***7.3 Deployable Systems***

In this Plan, Region 24 strongly supports use of deployable systems, both conventional and

trunked. Deployable systems are prepackaged systems that can deploy by ground or air to an

incident to provide additional coverage and capacity on designated 700 MHz interoperability

channels and/or agency specific General Use Channels. This will minimize the expense of

installing extensive fixed infrastructure in areas while still providing mission critical

functionalities as the Region recognizes the difficulty of providing complete coverage in all

areas due to financial, demographic and geographical constraints.

Agencies should have conventional deployable systems capable of being tuned to any of the

FCC designated/NCC recommended interoperability tactical channels. Those agencies that

are part of a multi-agency trunked system and commonly provide mutual aid to each other are

encouraged to have trunked deployable systems that operate on the tactical channels

designated by the FCC for this use. The SIEC will develop the operational details for

deploying these systems.

It is expected that the tactical channels set aside for trunked operation will be heavily used by

deployable systems. Therefore, the tactical channels cannot be assigned to augment general

use trunked systems.

***7.4 Monitoring of Calling Channels***

700 MHz General Use channel licensees will be responsible for monitoring interoperable

calling channels. The SIEC will develop operational guidelines for this function. **Appendix**

**E** will include NCC documents that display required Interoperability guidelines.

**8. Future Planning**

The CAPRAD pre-coordination database has developed channel allotments in each county area

within Missouri, including the City of St Louis using criteria such as current population, 2010

Census data, height above average terrain (HAAT) and public safety use curves generated by the

Public Safety Wireless Advisory Committee (PSWAC) to provide spectrally efficient frequency

allotments.

***8.1*** *Inter-Regional Dispute Resolution Process*

In the event that a dispute arises between Region 24 and an adjacent Region or Regions, regarding

spectrum allocations or implementation, that cannot be resolved within 60 days, the parties to the

dispute will request a hearing by the National Regional Planning Oversight Committee. **See**

**Appendix H for details and Inter-Regional Dispute Resolution Agreements signed by adjacent**

**Regions 4,13,15,16,17,26,34, and 39.**

**9.0 Certification**

I hereby certify that all planning committee meetings, including subcommittee or executive

committee meetings were open to the public. A summary of the deliberations of the

Committee pursuant to adopting this Plan can be found in Appendix D, in the minutes of the

January 14, 2003 Regional Planning meeting.

Stephen T. Devine

Chairman, Region 24

**Appendices**

**Appendix A Bylaws**

**Appendix B Region 24 Members, Agencies, Contact Information and**

**Voting Status**

**Appendix C Region 24 (Missouri) Counties**

**Appendix D List of Meetings, summaries of minutes, agendas**

**Appendix E 700 MHz Interoperability channel nomenclature**

**Appendix F NCC 700 MHz Pre-Assignment Rules/Recommendations**

**Appendix G Region 24 Channel allotments**

**Appendix H Inter Regional Dispute Resolution Agreement**

**Appendix I DTV Protection and Incumbency**

**Appendix J Meeting Announcements**

**Appendix A**

**Bylaws of the 700 MHz Regional Planning Committee-**

**Region 24 (State of Missouri)**

**Revised September 16, 2002**

**BYLAWS OF REGION 24**

**NAME & PURPOSE**

**1.1 Name and purpose**. The name of this Region shall be Region 24-Regional Planning

Committee. Its primary purpose is to foster and promote cooperation, planning, development

and evolution of Regional Plans and the implementation of these plans in the 700 MHz Public

Safety Band within the State of Missouri.

**MEMBERS**

For purposes of this document, the term “member,” unless otherwise specified, refers to both voting

and non-voting members.

**2.1 Numbers, Election and Qualification**. The Regional 24 700 MHz Regional Planning

Committee shall have two classes of members, “voting members” and “non-voting members.”

New members may be added at annual, special, or regular meetings. Tools to promote

participation and involvement in the Region 24 700 MHz Committee in the form of a list-serve

and/or regional newsletters will be researched by the committee. The newsletter may be

distributed both electronically and in print form.

**Voting Members**. Voting members shall consist of one (1) representative from any single

agency engaged in public safety eligible to hold a license under 47 CFR 90.20, 47 CFR 90.523

or 47 CFR 2.103. Except that a single agency shall be allowed no more than one vote for each

distinct eligibility category (e.g. police, fire, EMS, highway) within the agency’s organization or

political jurisdiction. In voting on any issue, the individual must identify himself/herself and the

agency and eligibility category in which he or she represents. **Voting members may not vote**

**on issues involving their entity. To become a member of Region 24 700 MHz Regional**

**Planning Committee to represent their agency, a representative simply has to attend a**

**meeting. See attendance and voting rights procedures below.**

**Non-Voting Members**. Non-voting members are all other non-public safety personnel

interested in furthering the goals of public safety communications.

**2.2 Tenure**. In general, each member shall hold MEMBERSHIP from the date of acceptance until

resignation or removal.

**2.3 Powers and Rights.** In addition to such powers and rights as are vested in them by law, or

these bylaws, the members shall have such other powers and rights as the membership may

determine.

**2.4 Suspensions and Removal.** A representative may be suspended or removed with cause by

vote of a majority of members after reasonable notice and opportunity to be heard. Region 24

will hold at least two (2) meetings in a calendar year. To retain consistent voting rights,

members should attend one (1) meeting in a 24-month period**. After the date of approval of**

**this Regional Plan by the Federal Communications Commission, all previous attendees are**

**voting members, with the exception of non-voting commercial members. After the**

**acceptance of this Regional Plan, voting members that do not attend one meeting in a 24-**

**month period that starts on the date of plan acceptance, will lose Region 24 voting rights**

**for either a 6 month period or when the member attends the next Regional Planning**

**Committee meeting, whichever comes first. Attending a meeting is all that is required to**

**immediately reinstate voting members voting rights**. The loss of voting rights does not

remove a member from active status; it simply requires attendance at a meeting (Special or

Regular) to reinstate voting privileges. The voting limitations of an individual have no effect on

the voting ability of a public safety entity. The public safety entity reserves the right to send

another representative to vote on issues regarding 700 MHz implementation, or send the original

voting representative to the next special or regular meeting.

A vote of the committee is the final determining factor regarding removal a member from

Region 24. A period of 6 months from the first day of removal is required before a removed

member is eligible for reinstatement for membership in the Regional Planning Committee.

**2.5 Resignation**. A member may resign by delivering written resignation to the chairman, vicechairman,

treasurer or secretary of the Regional Committee or to a meeting of the members. A

resigning member is eligible for reinstatement to the Regional Planning Committee after a

period of six months has lapsed, beginning on the first day of resignation.

**2.6 Meetings.** After Regional Plan approval, the Region 24 700 MHz Planning Committee will

meet no less than two (2) times every twelve (12) months. **One meeting in each calendar year**

**may be held in Jefferson City, Missouri. This is centrally located within Region 24 and**

**will provide the maximum opportunity for regional participation. The remaining**

**meeting(s) are to be located in a different city or town within the Region to attract and**

**promote involvement in the committee decided on by members of the committee.**

Committee meetings will not be held on holidays or weekend days, unless called by the Region

24 Chairperson. At any time and when deemed necessary by the Chairperson, an additional

meeting of the Region 24 Regional Planning Committee may be called. Video and/or Audio

Teleconferencing may be conducted at meetings to include as many people as possible in the

700 MHz allocation process. The use of electronic E-mail and the Region 24 list-servers

(**RPC24@yahoogroups.com, region24siec@yahoogroups.com and**

**NPSPACregion24@yahoogrous.com**) will be utilized by members and officers of Region 24

as needed to convey regional issues at hand. **It should be noted the use of E-mail and/or**

**video-audio teleconferencing does not remove the voting eligibility requirement of the**

**member to attend at least one (1) of the Region 24 annual meetings.**

**2.7 Special Meetings**. **The Chairperson has the authority to call a meeting of the Regional**

**Planning Committee when he deems it in the best interest of the Region and will provide**

**notice of the special meeting to existing members of the Region (and the public) at least 5**

**days prior to the meeting.** Special meetings of the members may be held at any time and at any

place within the Regional Committee area. Special meetings of the members may be called by

the chairman or by the vice-chairman, or in case of death, absence, incapacity, by any other

officer or, upon written application of two or more members.

**2.8 Call and Notice.**

A. Semi Annual meetings. Reasonable notice of the time and place of scheduled

meetings of the members, not being less than 60 days, shall be given to each member.

Such notice may specify the purposes of a meeting, but will specify meeting content if

required by law or these bylaws or unless there is to be considered at the meeting (i)

amendments to these bylaws or (ii) removal or suspension of a member who is an

officer. Announcements of meetings, stating the time and place where the meeting is to

be held, may be published in newspapers and land mobile radio periodicals. **In**

**addition, a press release may be issued, urging parties interested in public safety**

**communications to attend**. **Region 24 is will notify the Federal Communications**

**Commission, Chief of the Wireless Telecommunications Bureau, when a meeting**

**time and place has been established for the Region 24 700 MHz Regional Planning**

**Committee**.

B. **Reasonable and sufficient notice**. Except as otherwise expressly provided, it

shall be reasonable and sufficient notice to a member to send notice by mail at least five

days or by e-mail/facsimile at least three days before any special meetings, addressed to

such member at his or her usual or last known business address, or, to give notice to such

member in person or by telephone at least three days before the meeting.

**2.9 Quorum**. **At any meeting of the members, a majority of the officers and a minimum of at**

**least three (3) voting members shall constitute a quorum**. Any meeting may be adjourned to

such date or dates not more than ninety days after the first session of the meeting by a majority

of the votes cast upon the question, whether or not a quorum is present, and the meeting may be

held as adjourned without further notice.

**2.10 Action by Vote**. Each voting member, representing a particular agency (one vote per agency)

shall have one vote; non-voting members have no voting rights. When a quorum is present at

any meeting, a majority of the votes properly cast by voting members present shall decide any

question, including election to any office, unless otherwise provided by law or these bylaws.

**2.11 Action by Writing**. Any action required or permitted to be taken at any meeting of the

members may be taken without a meeting if all members entitled to vote on the matter consent

to the action in writing and the written consents are filed with the records of the meetings of the

members. **Such consents shall be treated for all purposes as a vote at a meeting.**

**2.12 Proxies**. Voting members may vote either in person or by written proxy dated not more than

one month before the meeting named therein, which proxies shall be filed before being noted

with the secretary or other person responsible for recording the proceedings of the meeting. **A**

**RPC member present via teleconference (audio or video) shall have voting status parallel**

**to a member present at the meeting**. **If the facility is unable to accommodate**

**teleconferencing (audio or video), or for any other reason teleconferencing cannot be**

**accommodated in the meeting place, it is the responsibility of the member to attend the**

**meeting in person or to vote by written proxy to have full voting rights.** Unless otherwise

specifically limited by their terms, such proxies shall entitle the holders thereof to vote at any

adjournment of the meeting for which the proxy exists and the proxy shall terminate after the

final adjournment of such meeting.

**2.13 Voting on One’s Own Application. At no time can a voting member vote on his/her**

**application**.

**2.14 Special Interest Voting**. A voting member **cannot** have a commercial interest in any of

his/her Region and/or adjacent Region’s application(s) on which he/she is reviewing, approving

and/or voting.

**OFFICERS AND AGENTS**

**3.1 Number and qualification. The officers of the Region 24 700 MHz Regional Planning**

**Committee shall consist of a chairman, a vice-chairman and a secretary. All officers must be**

**voting members of the Regional Committee.**

**3.2 Election**. The officers shall be elected by the voting members at their first meeting and,

thereafter, at a meeting determined by the membership. The terms of the officers in the Region

24 700 MHz RPC will be for two (2) years. In order to allow for consistency in the plan

creation and initialization process, the terms of elected officers will begin on the date of the

FCC’s approval of the Region 24 plan.

**3.3 Tenure.** The officers shall each hold office until the biannual election meeting of the members

held within two years from the adoption of these bylaws, or until their successor, if any, is

chosen, or in each case until he or she sooner dies, resigns, is removed or becomes disqualified.

**3.4 Chairman and Vice Chairman**. The chairman shall be the chief executive officer of the

Regional Committee and, subject to the control of the voting members, shall have general

charge and supervision of the affairs of the Regional Committee. The chairman shall preside at

all meetings of the Regional Committee. The Vice Chairman, if any, shall have such duties and

powers, as the voting members shall determine. The Vice-Chairman shall have and may

exercise all the powers and duties of the chairman during the absence of the chairman or in the

event of his or her inability to act.

**3.5 Treasurer.** The treasurer shall be the chief financial officer and the chief accounting officer of

the Regional Committee. The treasurer shall be in charge of its financial affairs, funds, and

valuable papers and shall keep full and accurate records thereof. **In the absence of a treasurer**

**within the Region 24 700 MHz Planning Committee, the Chairperson shall assign Region**

**24 treasurer duties as deemed necessary.**

**3.6 Secretary.** The secretary shall record and maintain records of all proceedings of the members

in a file or series of files kept for that purpose, which file or files shall be kept within the Region

and shall be open at all reasonable times to the inspection of any member. Such file or files

shall also contain records of all meetings and the original, or attested copies, of bylaws and

names of all members and the address (including e-mail address, if available) of each. If the

secretary is absent from any meeting of members, a temporary secretary chosen at the meeting

shall exercise the duties of the secretary at the meeting. In the absence of a secretary within the

Region 24 700 MHz Planning Committee, the Chairperson shall assign Region 24 Secretary

duties as deemed necessary.

**3.7 Suspensions or Removal**. An officer of the Region 24 Regional Planning Committee may be

suspended with cause by vote of a majority of the voting members in attendance.

**3.8 Resignation.** An officer may resign by delivering his or her written resignation to the chairman,

vice-chairman, treasurer, or secretary of the Regional Committee. Such resignation shall be

effective upon receipt (unless specified to be effective at some other time), and acceptance

thereof shall not be necessary to make it effective unless it so states.

**3.9 Vacancies**. If the office of any officer becomes vacant, the voting members may elect a

successor. Each such successor shall hold office for the remainder terms, and in the case of the

chairman, vice chairman, treasurer and clerk until his or her successor is elected and qualified,

or in each case until he or she sooner dies, resigns, is removed or become disqualified.

**AMENDMENTS**

These bylaws may be altered, amended or repealed in whole or in part by vote. The voting

members may by a two-thirds vote of a quorum, alter, amend, or repeal any bylaws adopted by the

Regional Committee members or otherwise adopt, alter, amend or repeal any provision which FCC

regulation or these bylaws requires action by the voting members.

**DISSOLUTION**

This Regional Committee may be dissolved by the consent of two-thirds plus one of an assembled

quorum of the membership at a special meeting called for such purpose. The FCC shall be notified.

**RULES OF PROCEDURES**

The Conduct of Regional Meetings including without limitation, debate and voting, shall be

governed by Robert’s Rules of Order, newly revised 1990 edition, ninth edition, Sarah Corbin

Robert, Henry M. Robert III, and William J. Evans.

**Appendix B**

**Region 24 member list and Contact information**

Peter Albera

Motorola C&E, Inc.

1129 SW Sunflower Dr.

Lee's Summit MO 64081

816-246-1350

peter.albera@motorola.com

(Commercial/ Non-voting)

William Bauer

North Central Fire Alarm

101 E Maple St.

Wentzville MO 63385

Tim Bechler

Central County E9-1-1

22 Weis Av

Ellisville MO 63011

636-207-7911

tim@cce911.org

Rick Bennett

Missouri Department of Transportation

2211 St. Mary's Blvd

Jefferson City MO 65102

573-526-4842

richard.bennett@modot.mo.gov

James C. Biggerstaff, Director

Missouri State Highway Patrol

1510 East Elm St.

Jefferson City MO 65101

573-526-6100

Scott Bigham

Missouri State Highway Patrol

P.O. Box 3756

Kirkwood MO 63122

Ed Brundage

Kansas City Police Department

1125 Locust St

Kansas City MO 64106

816-234-5000

ebrunadge@kcpd.org

Norman Buehre

Clayton Fire Department

10 N Bemiston Av

Clayton MO 63105

nbuehre@ci.clayton.mo.us

Terry Buhr

Motorola C&E, Inc.

5691 Sunnywood Drive

Cedar Hill MO 63106

636-274-4986

(Commercial/ Non-voting)

William Cade

Jasper County 911

13870 Dispatch Lane

Carthage MO 64836

417-358-7000

417-359-9116

911@jasco.org

Rex Capen

City of Joplin

303 East Third St

Joplin MO 64801

417-624-0820

rcapen@joplin.mo.org

David Cerqua

M/A-Com

8105 N Beltline Rd., Ste. 170

Irving TX 75063

972-550-2323

972-550-2364

(Commercial/ Non-voting)

Jonathan Chaney

Missouri State Highway Patrol

P.O. Box 3756

Kirkwood MO 63122

314-340-4000

Fax 314 340 4010

Michael Clinard

St. Peters Police Department

1020 Kimberley Dr.

St. Peters MO 63376

636-477-6600

Chuck Collins

Springfield/ Greene County Emergency Communications Department

319 East Chestnut Expressway

Springfield MO 65802

417-864-1708

417-864-1824

Tom Dailey

Kansas City Police Department

1125 Locust St

Kansas City MO 64106

816-234-5000

tadiley@kcpd.org

Stephen T. Devine, Chair

Missouri State Highway Patrol

1510 East Elm St.

Jefferson City MO 65101

573-526-6105

573-526-1112

steve.devine@mshp.dps.mo.gov

John Diggs

Missouri Department of Transportation

105 W Capitol Av

Jefferson City MO 65102

573-526-0125

john.diggs@modot.mo.gov

Tom Dollus

Missouri Department of Transportation

105 W Capitol Av

Jefferson City MO 65102

Kent Forde

Valle Ambulance District

P.O. Box 460

DeSoto MO 63020

636-586-2312

636-337-0808

David Funk

NLECTC

2050 E. Iliff Ave

Denver, Colorado 80208

dafunk@du.edu

303 871 2439

Charles Gastler

St. Louis Metropolitan Police Department

1200 Clark Av

St. Louis MO 63103

314-444-5993

314-444-2919

cdgastler@slmpd.org

David Gelyana

RCC Consulting

515 Newtown Drive

Buffalo Grove IL 60089

dgelyana@rcc.com

(Commercial/ Non-voting)

Pam Gilligan

Jefferson City Police Department

401 Monroe

Jefferson City MO 65101

573 634 6400

leadop@jeffcitymo.org

William Harlan

St. Louis County Police Department

7900 Forsyth Blvd.

Clayton MO 63105

314 6t15 3562

Bill Holcomb

Commenco

4901 Bristol Av

Kansas City MO 64129

816-753-2166

billh@commenco.com

(Commercial/ Non-voting)

Drew Juden

City of Sikeston

215 N New Madrid

Sikeston MO 63801

573-471-6200

drewj@sikeston.org

Thomas Kearns

M/A-Com

15511 W 89th Terrace

Lenexa KS 66291

913-541-8146

tkearns@discoverynet.com

(Commercial/ Non-voting)

Doug Keeney

Jefferson City Police Department

401 Monroe

Jefferson City MO 65101

573 634 6400

dkeeney@jeffcitymo.org

Keith Kemmerline

Motorola C&E, Inc.

2995 Telber Ct.

Stow OH 44224

330-678-0960

(Commercial/ Non-voting)

Ronald Kronenberger, Nextel

One City Place Drive, Suite # 100

St Louis, MO 63141

314 568 4550

Fax 314 787 3501

ronald.kronenberger@nextel.com

(Commercial/ Non-voting)

Robert Lawery

Kansas City Police Department

1125 Locust St

Kansas City MO 64106

816-234-5000

rlawrey@kcpd.org

James A. Lundsted

Missouri State Highway Patrol

1510 East Elm St.

Jefferson City MO 65101

573-526-6104

Paul Luttrell

City of Joplin

303 East Third St

Joplin MO 64801

417-624-0820

pluttrell@joplin.mo.org

Steven J. Makky, Sr., Vice-Chair

St. Charles County Government

301 N Second St., Rm. 280

St. Charles MO 63301-5410

636-949-3031

636-949-3021

smakky@saintcharlescounty.org

Jon Martin

Motorola C&E, Inc.

1292 Poseidon Ct

St. Peters MO 63367

636-970-7904

636-279-3309

jon.martin@motorola.com

(Commercial/ Non-voting)

Tony Martinez

Communications Associates

3343 S Scenic

Springfield MO 65807

417 882 1401

tony@commassocradio.com

(Commercial/ Non-voting)

Pat McKenzie

Kansas City Police Department

1125 Locust St

Kansas City MO 64106

816-234-5000

pmckenzie@kcpd.org

Joe Moncado

M/A-Com

15745 W Beckett Lane

Olathe KS 66062

913-764-0026

913-599-6280

(Commercial/ Non-voting)

Sharon Murray

Republic Police Department

540 Civic Blvd

Republic MO 65738

417-732-2642

Jim Nesselrode

Commenco

4901 Bristol Av

Kansas City MO 64129

816-753-2166

ness@commenco.com

(Commercial/ Non-voting)

Chad Powelson

Commenco

4901 Bristol Av

Kansas City MO 64129

816-753-2166

chad@commenco.com

(Commercial/ Non-voting)

Karen Raines

Federal Communications Commission-Kansas city Field Office

520 NE Colbern Rd, 2 FL

Lee's Summit MO 64086

816-316-1256

kraines@fcc.gov

(Honorary/ Non-Voting)

Tim Raymer

Missouri Department of Health & Senior Services

P.O. Box 570

Jefferson City MO 65102

573-526-7387

raymet@dss.mo.gov

Michael Redman

St. Louis County Police Department

7900 Forsyth Blvd.

Clayton MO 63105

314 615 5362

Region 24 700 MHz Plan Amended Dec 28, 2007

Main Section Page 38

Kurt Rellergert, Motorola C&E,

4 Gills Inn Drive

O'Fallon MO 63366

636-240-9315

kurtis.rellergert@motorola.com

Stephen Richey

St. Joseph Fire Department

401 S 7th St.

St. Joseph MO 64501

816-271-4603

srichey@ci-st-joseph.mo.us

Bette Rinehart

Motorola C&E, Inc.

28 Twin Lakes Drive

Gettysburg PA 17325

c18923@email.mot.com

(Commercial/ Non-voting)

Daniel Rowden

St. Charles County Department of Dispatch & Alarm

1605 Wentzville Parkway

Wentzville MO 63385

636-949-3018

636-949-7328

drowden@saintcharlescounty.org

Steve Ruskin

M/A-Com

9100 East Panorama Dr., Ste. 200

Englewood CO 80112

303-980-3022

303-980-3039

sruskin@tycoelectronics.com

(Commercial/ Non-voting)

Ron Shook-Retired

Greene County

833 Boonville

Springfield MO 65802

417-869-6040

rshook@greenecounty.org

Steve Sloan

Missouri State Emergency Management Agency

2302 Militia Drive

Jefferson City MO 65102

573-526-9144

steve.sloan@sema.dps.mo.gov

Robert Speidel

M/A-Com

P.O. Box 2000;

221 Jefferson Ridge Pkwy

Lynchburg VA 24501

434-455-9465

434-455-6764

speidelbo@tycoelectronics.com

(Commercial/ Non-voting)

Roger Strope, Chief Projects Engineer

Missouri State Highway Patrol

1510 East Elm St.

Jefferson City MO 65101

573-526-6104

Richard Stump, Communications Officer

Missouri State Emergency Management Agency

2302 Militia Drive

Jefferson City MO 65102

573-526-9201

richard.stump@sema.dps.mo.gov

Reg Swan

Johnson Communications Service/ Tel-Link

1606 North Kingshighway

Cape Girardeau MO 63701

573-335-5555

regswan@jcstel.com

(Commercial/ Non-voting)

Chris Teel

Springfield/ Greene County 9-1-1

319 East Chestnut Expressway

Springfield MO 65802

417-864-1708

417-864-1824

Michael Turner

Central County E9-1-1

22 Weis Av

Ellisville MO 63011

636-207-7911

mturner@cce911.org

T.J. Ward

State of Illinois

531 Sangamon Av

Springfield IL 62702

217-782-5742

217-524-4396

wardt@apco911.org

(Honorary/ Non-Voting)

J.R.Webb

Springfield/ Greene County 9-1-1

319 East Chestnut Expressway

Springfield MO 65802

417-874-1222

417-864-1572

jrwebb@ci.springfield.mo.us

Tom White, Director

Cooper County Emergency Management

200 Main Street

Boonville MO 65233

660-882-2614

660-882-2610

ema@undata.com

David Wunderlin

Radio Communications Specialists

1122 Illinois, Ste. 104

Joplin MO 64801

417-781-3797

417-781-8631

rcs@rcsonline.net

(Commercial/ Non-voting)

Chuck Zang

Kansas City Fire Department

635 Woodland Av, Suite 2100

Kansas City MO 64106

816-784-9200

816-784-9230

chuck\_zang@kcmo.org

Rodney Zerr

St. Charles County Emergency Management Agency

301 N Second St., Rm. 280

St. Charles MO 63301-5410

636-949-3023

636-949-3021

rzerr@saintcharlescounty.org

**Meeting attendees by meeting**

June 7, 2000 Jefferson City, Missouri

Attendees

Stephen T. Devine, Patrol Frequency Coordinator, Missouri State Highway Patrol, 800 MHz

NPSPAC Chairperson

Michael Redman, Communications Coordinator, St Louis County Police

Ron Shook, Emergency Management Agency, Greene County Missouri

William Cade, Jasper County 911, Jasper County Missouri

Chris Teel, Springfield/Greene County 911, Springfield, Missouri

J.R. Webb, Greene County Missouri Sheriff’s Office

James C. Biggerstaff, Director of Radio, Missouri State Highway Patrol

James A. Lundsted, Chief Projects Engineer, Missouri State Highway Patrol

Charles Gastler, Communications Manager, St Louis Metropolitan Police Department

October 5, 2000 Jefferson City, Missouri

Ron Shook, Convenor, Greene County Emergency Management

Stephen T. Devine, (Elected Chairperson at meeting)

J.R. Webb, Greene County Sheriff’s Office

Chuck Collins, Springfield/Greene County Emergency Communications Department

Charles Gastler, St Louis Metropolitan Police Department

James C. Biggerstaff, Director of Radio, Missouri State Highway Patrol

Michael Redman, Communications Coordinator, St Louis police

Steve Makky Sr. St Charles County Government

William Cade, Jasper County 911, Jasper County Missouri

Chris Teel, Springfield/Greene County 911

James A. Lundsted, Chief Projects Engineer, Missouri State Highway Patrol

January 11, 2001(St Louis County, Missouri)

Stephen Devine, Missouri State Highway Patrol-Chairperson

Jonathan Chaney, Missouri State Highway Patrol-St Louis

Scott Bigham, Missouri State Highway Patrol-St Louis

Rodney Zerr, St Charles County Emergency Management

Steven Makky Sr. St Charles County Emergency Management

Tom Dollus, Missouri Department of Transportation

Tim Bechler, Central St Louis County Fire Alarm/911

Roger Strope, Chief Projects Engineer, Missouri State Highway Patrol

Richard Stump, Communications Officer, Missouri State Emergency Management Agency

Dan Rowden, Director, St Charles County Department of Dispatch

Sgt. Mike Clinnard, St Peters Police Department

**David Wunderlin, Radio Communications Specialists, Joplin, Missouri**

William Cade, Jasper County 911, Jasper County, Missouri

**Terry Buhr, Motorola**

**Jon Martin, Motorola**

**Keith Kemmerline, Motorola**

Drew Juden, City of Sikeston, Missouri

Michael Redman, Communications Coordinator, St Louis County Police Department

William Bauer, North St Louis County Fire Alarm,

**Tom Kearns, Com-Net Ericsson**

Tom Ward, State of Illinois

Kent Forde, Valle Ambulance District, Jefferson County, Missouri

Lt William Harlan, St Louis County Police

Charles Gastler, St Louis Metropolitan Police Department

March 29, 2001 (Springfield, Missouri)

Ron Shook, Greene Co. EMA

J.R. Webb, Greene Co. Sheriff's Dep't.

Stephen T. Devine, Chairperson, Missouri State Highway Patrol

**Pete Albera, Motorola C&E, Inc**.

Bill Cade, Jasper County E9-1-1

Sharon Murray, Republic Police Department

Steve Sloan, Missouri State Emergency Management Agency

Steve Makky, Sr., St. Charles County Emergency Management

Mike Turner, Central County E9-1-1 (St. Louis Co.)

June 28, 2001 Jefferson City, Missouri

Stephen T. Devine, Chairperson, Missouri State Highway Patrol

Charles Gastler, St Louis Metropolitan Police Department

**Tom Kearns, MA/COM Wireless**

**Kurt Rellagert, Motorola**

**Pete Albera, Motorola**

J.R. Webb, Greene County Sheriff’s Department, Greene County, Missouri

Ron Shook, Greene County Emergency Management

James C. Biggerstaff, Director of Radio, Missouri State Highway Patrol

September 18, 2001, Branson, Missouri

Stephen T. Devine - MSHP - RPC Chairperson/ Chair Implementation Subcommittee

Steve Makky, Sr. - SCCG/ EMA - RPC Secretary/ Chair Technology Subcommittee

Mike Turner - Central [St. Louis] County E9-1-1

**Terry Buhr - Motorola**

Charles Gastler - St. Louis Metropolitan Police Department

**Tom Kearns - M/A Com Wireless**

J.R. Webb - Greene Co. Sheriff's Office

Roger Strope - Missouri State Highway Patrol

**Peter Albera - Motorola**

Ed Brundage - Kansas City, Mo. Police Department

Chuck Zang - Kansas City, Mo. Fire Department

**David Cerqua - M/A Com Wireless**

January 10, 2002 Jefferson City, Missouri

**Tom Kearns - M/A Com - kearnsth@tycoelectronics.com**

**Joe Mancato - M/A Com - e-mail not given**

**Pete Albera - Motorola - peter.albera@motorola.com**

**Jon Martin - Motorola - jon.martin@motorola.com**

Roger Strope - MSHP - stropr@mshp.state.mo.us

Stephen T. Devine - Chairperson, MSHP - devins@mshp.state.mo.us

Ed Brundage - Kansas City Police Department - ebrundage@kcpd.org

Chuck Zang - Kansas City Fire Department - chuck\_zang@kcmo.org

Bob Lawrey - Kansas City Police Department - rlawrey@kcpd.org

Chuck Gastler - St. Louis Metropolitan Police Department - cdgastler@slmpd.org

Jim Lundsted - Missouri Department of Conservation - jlundste@mail.state.mo.us

Steve Makky, Sr. - St. Charles County - smakky@pipeline.com

April 11, 2002 Kansas City, Missouri

Those in attendance:

Stephen T. Devine, MSHP sdevine@mail.state.mo.us

Steven J. Makky, Sr., St. Charles County, Mo smakky@pipeline.com

Stephen Richey, Fire Chief, St. Joseph, Mo srichey@ci.st-joseph.mo.us

**Jon Martin, Motorola** jon.martin@motorola.com

**Bob Speidel, Tyco M/A Com** speidelbo@tycoelectronics.com

**Tom Kearns, Tyco M/A Com** kearnsth@tycoelectronics.com

Chuck Zang, Kansas City Fire Dept. chuck\_zang@kcmo.org

Robert Lawrey, Kansas City Police rlawrey@kcpd.org

Tom Dailey, Kansas City Police tdailey@kcpd.org

Ed Brundage, Kansas City Police ebrundage@kcpd.org

Pat McKenzie, Kansas City Police pmckenzie@kcpd.org

**Jim Nesselrobe, Commenco, Inc**. ness@commenco.com

**Chad Powelson, Commenco, Inc**. chad@commenco.com

September 24, 2002 Jefferson City

Stephen Devine, Chairperson, MSHP sdevine@mail.state.mo.us

Steve Makky, Sr. St Charles County EMA smakky@pipeline.com

Richard Stump, MO SEMA rstump@mail.state.mo.us

Karen Raines, FCC kraines@fcc.gov

Ron Shook, Greene County rshook@greencounty.org

Tom Kearns, MA/COM kearnsth@tycoelectronics.com

**Robert Speidel, MA/COM** speidelbo@tycoelectronics.com

J.R. Webb jrwebb@ci.springfield.mo.us

Paul Luttrell, Joplin, Mo pluttrel@joplinmo.org

**David Gleyana, RCC Consultants** dgelyana@rcc.com

Ed Brundage, KCPD ebrundage@kcpd.org

Bob Lowery rlawrey@kcpd.org

**Pete Albera, Motorola** peter.albera@motorola.com

January 14, 2003 Jefferson City, Missouri

Stephen Devine sdevine@mail.state.mo.us MSHP

Steve Makky, Sr. smakky@pipeline.com St Charles County EMA

Roger Strope stropr@mshp.state.mo.us MSHP

Norman Buehre nbuehre@ci.clayton.mo.us City of Clayton

Rick Bennett benner1@mail.modot.state.mo.us Missouri DOT

John Diggs diggsj@mail.modot.state.mo.us Missouri DOT

Richard Stump rstump@mail.state.mo.us State Emergency Management

J.R. Webb jrwebb@ci.springfield.mo.us City of Springfield, Missouri

Dan Rowden drowden@win.org St Charles County Fire Alarm

**Tom Kearns** kearnsth@tycoelectronics.com MA/COM

**Steve Ruskin** ruskinst@tycoelectronics.com MA/COM

Ed Brundage ebrundage@kcpd.org Kansas City Police Dept

Karen Raines kraines@fcc.gov FCC Enforcement Bureau-KC

Drew Juden drewj@sikeston.org City of Sikeston

**Reg Swan** regswan@jcstel.com JCS Tel Link

**Peter Albera** peter.albera@motorola.com Motorola

**Kurt Rellergert** kurtis.rellergert@motorola.com Motorola

**Jon Martin** jon.martin@motorola.com Motorola

Paul Luttrell pluttrel@joplinmo.org City of Joplin

Rex Capen rcapen@joplinmo.org City of Joplin

**Bette Rinehart** c18923@email.mot.com Motorola

Tom White ema@undata.com Cooper County, Missouri

Ron Shook rshook@greencounty.org Greene County EMA

July 1, 2003, Jefferson City, Missouri

Stephen T. Devine, Chair devins@mshp.state.mo.us MSHP

Roger Strope stropr@mshp.state.mo.us MSHP

Tim Raymer raymet@dhss.state.mo.us MO Div of Health-Human Services

J.R. Webb jrwebb@ci.springfield.mo.us Springfield-Greene County 911

**Bill Holcomb billh@commenco.com Commenco**

**Peter Albera peter.albera@motorola.com Motorola**

**Jon Martin jon.martin@motorola.com Motorola**

Richard Stump rstump@mail.state.mo.us MO State Emergency Management

Karen Raines kraines@fcc.gov FCC Kansas City Field Office

Steve Makky, Sr, Secretary/Vice Chair smakky@ka2otd.org St Charles County

December 8, 2004 St Louis City Police Department

Jon Martin jon.martin@motorola.com **Motorola**

Ron Kronenberger ronald.kronenberger@nextel.com **Nextel**

Pam Gilligan leadop@jeffcitymo.org Jefferson City Police Dept

Roger Strope roger.strope@mshp.dps.mo.gov Missouri State Highway Patrol

Charles Gastler cdgastler@slmpd.org St Louis City Police Department

David Funk dafunk@du.edu NLECTC

Steve Devine steve.devine@mshp.dps.mo.gov Missouri State Highway Patrol

Steve Ruskin ruskinst@tycoelectronics.com **MA/COM**

Tony Martinez tony@commassocradio.com **Communications Associates**

Douglas Keeney dkeeney@jeffcitymo.org Jefferson City Police Dept

.

**Appendix C**

**List of counties areas within Region 24:**

Note: The City of St Louis is the only city in the State of Missouri that is not located within a

Missouri county and it has an individual allotment. **Pool channel allotments are allotted by**

**“County Areas” in Region 24. County areas and their definitions are listed in Section 6.3**

Adair

Andrew

Atchison

Audrain

Barry

Barton

Bates

Benton

Bollinger

Boone

Buchanan

Butler

Caldwell

Callaway

Camden

Cape Girardeau

Carroll

Carter

Cass

Cedar

Chariton

Christian

Clark

Clay

Clinton

Cole

Cooper

Crawford

Dade

Dallas

Daviess

Dekalb

Dent

Douglas

Dunklin

Franklin

Gasconade

Gentry

Greene

Grundy

Harrison

Henry

Hickory

Holt

Howard

Howell

Iron

Jackson

Jasper

Jefferson

Johnson

Knox

Laclede

Lafayette

Lawrence

Lewis

Lincoln

Linn

Livingston

Macon

Madison

Maries

Marion

McDonald

Mercer

Miller

Mississippi

Moniteau

Monroe

Montgomery

Morgan

New Madrid

Newton

Nodaway

Oregon

Osage

Ozark

Pemiscot

Perry

Pettis

Phelps

Pike

Platte

Polk

Pulaski

Putnam

Ralls

Randolph

Ray

Reynolds

Ripley

Saline

Schuyler

Scotland

Scott

Shannon

Shelby

St. Charles

St. Louis

St. Francois

St. Clair

Ste. Genevieve

Stoddard

Stone

Sullivan

Taney

Texas

Vernon

Warren

Washington

Wayne

Webster

Worth

Wright

**Appendix D**

Meeting attendance, agendas and other events where 700MHz information was disseminated.

June 7, 2000 800 MHz NPSPAC Regional Planning Committee meeting in Jefferson City,

Missouri

Called by Acting Chairperson of 800 MHz NPSPAC Region Stephen Devine,

who is standing in for Mr. John Gerke, as he withdrew from the 800 MHz

Chair due to ill health, elected Chairperson of 800 MHz Committee. FCC

Wireless Bureau notified.

Meeting topics included discussion of Region 24’s status, the appointment of

a new Regional Chairperson and a review of national planning requirements.

A discussion of the upcoming 700 MHz public safety spectrum was

introduced and the Chairperson advised the committee he would be

appointing a convener. Letter from Chairperson Stephen T. Devine to Chief

of the Wireless Telecommunications Bureau dated June 12, 2000 prematurely

stated that Stephen Devine was named convener of the 700 MHz Region 24

Planning Committee. This did not allow for enough notice between meeting

announcement and initial meeting per FCC issued guidelines.

July 1, 2000 800 MHz Region 24 Chairperson Stephen T. Devine appoints Ron

Shook of Emergency Management, Greene County, Missouri Convener of

the 700 MHz Regional Planning Committee and sets first meeting date for

October 5, thereby allowing 90 days notice of first meeting. FCC Wireless

Bureau notified of the appointment of Convener in letter to Chief dated

October 6, 2000.

Convener Ron Shook, Greene County, Missouri Emergency Management

940 Booneville Road, Springfield, Missouri 65802

Work phone 417 829 6209

E-mail rshook@greenecountymo.org

August 28, 2000 Missouri State Highway Patrol issues Press release for meeting dated August

28, 2000.

APCO notified of meeting announcement

FCC Wireless Bureau notified of announcement

Missouri State Highway Patrol issues Statewide teletype message announcing

700 MHz committee formation on October 5, 2000.

October 5, 2000 700 MHz Region 24 Planning Committee convened by Ron Shook of Greene

County Emergency Management. 700 MHz Meeting began at 1145 hrs CDT.

Stephen T. Devine, Missouri State Highway Patrol Frequency Coordinator

was elected Chairperson of the 700 MHz Region 24 Planning Committee.

The list of attendees were as follows:

**Stephen T. Devine**, Chairperson Region 24 800 MHz and Frequency

Coordinator-Missouri State Highway Patrol

**Michael Redman**, St Louis County Police

**Ron Shook**, Convener, Greene County Emergency Management Agency

**William Cade**, Jasper County 911

**Chris Teel**, Springfield/Greene County 911

**J.R. Webb**, Greene County Sheriff’s Office

**James C. Biggerstaff**, Director of Radio, Missouri State Highway Patrol

**James A. Lundsted**, Chief Projects Engineer, Missouri State Highway Patrol

**Charles A. Gastler**-Communications-St Louis Metropolitan Police

**Steve Makky Sr**. St Charles County Emergency Management

Meeting topics included election of 700 MHz Chairperson and approaching

NCC to ask if meeting in the Midwest (St Louis or Kansas City, preferably)

See letter to NCC DFO Michael Wilhelm dated June 12, 2000.

January 11, 2001 700 MHz Region 24 meeting schedule for January 11, 2001 in St Louis

County Missouri at the St Louis County Emergency Operations Center,

14847 Olive Street Road, Chesterfield, Missouri beginning called to order at

11:30 by Chairperson Devine.

Missouri State Highway Patrol issues news release indicating date, time and

meeting agenda of January 11 meeting to news media throughout Missouri

and surrounding areas dated November 7, 2000. Copies of news release

faxed to all APCO Frequency Coordinators in Missouri’s eight (8) adjacent

states on December 13, 2000.

MRT, Radio Resource magazine and the APCO magazine are all notified of

the meeting date time and agenda. FCC Wireless Bureau also notified. A list

of fire agencies within the St Louis area is obtained and 70 copies of the

MSHP news release are faxed to the fire agencies making them aware of the

meeting on November 14, 2000

A letter is sent to Region 13 (Southern Illinois) convener T.J. Ward to invite

his participation in the meeting as they have begun the convening process and

have areas of interest in southern Illinois adjacent to the area of the meeting.

Meeting attendee list on file.

Meeting topics include updating NCC information, presentation on 700 MHz

band and frequency allotments (Interoperability, State license and General

Use) and Regional Plan requirements.

February 2-3, 2001 700 MHz Chairperson Stephen T. Devine gives two presentations at the

Missouri State Emergency Management Agency Annual Communications

Conference at the Inn at the Grand Glaize Hotel in Lake Ozark, Missouri.

Information regarding the 700 MHz Regional Planning Committee in Region

24 was discussed and attendees were invited to the meeting in Springfield,

Missouri set for March 29, 2001 and to participate in Region 24 700 MHz

meetings.

March 29, 2001 700 MHz Regional Planning Committee Meeting convenes on March 29 in

Springfield, Missouri at the Greene County Emergency Management

Agency. Attendee list is on file.

Missouri State Highway Patrol issues Tele-type message statewide

announced meeting date, time, location and agenda on March 15, 2001.

Meeting topics include sub-committee formation (Interoperability,

Implementation and Technology) and Election of Region 24 Committee

Secretary.

Subcommittee Chairpersons elected:

**Technology** – Steve Makky, Sr. St Charles County Emergency Management

**Interoperability** – William Cade, Jasper County 911 (Ron Shook, Greene

County Emergency Management)

**Implementation** – Stephen T. Devine, Missouri State Highway Patrol

Email sent to FCC Wireless Bureau and Radio Resource, MRT and APCO

Magazine with meeting announcement including date, location and time of

meeting.

FCC issues Public Notice (DA 01-343) on Region 24 meeting set for March

29, 2001 on February 13, 2001.

April 16, 2001 Region 24 Chairperson Stephen T. Devine attends the Missouri State

Emergency Management Agency Annual Conference at Lake Ozark and

attends Region 24 display table providing information on the 700 MHz

planning committee that is formed within Missouri. A banner is used to

advertise the Committee and questions from conference attendees are

answered. The hours of the display table are 8 am through 2 pm.

June 28, 2001 Region 24 700 MHz Regional Planning Committee meeting is announced for

June 28, 2001 at the Missouri State Highway Patrol Headquarters located at

1510 East Elm, Jefferson City, Missouri 65101. Attendee list is on file.

Meeting convened at 12:39 PM. Meeting topics included discussed were

several documents initiated by the NCC that are before the FCC, particularly

the NPSTC request to not allow commercial wireless providers to use high

powered base stations in areas of commercial spectrum adjacent to public

safety mobile users.

Missouri State Highway Patrol issues a news release announcing date, time

and location June 28, 2001 Region 24 700 MHz meeting.

FCC Wireless Bureau issues Public Notice (DA 01-1043) for meeting.

Radio Resource, MRT magazine and APCO magazine post meeting

information for June 28 meeting after receiving E-mail from Chairperson.

Other meeting topics include:

NCC standing documents,

Progress reports on NCC status

Region 24 planned use of the NPSTC pre-coordination database

Interference issues

Coordination licensing

Regional funding

July 27, 2001 The list-serve for Region 24 is rpc24@yahoogroups.com

It is a forum for members and other interested parties to exchange 700 MHz

public safety information along with updated NCC information. The National

Public safety Telecommunications Council created the website for the

Region.

September 18, 2001 NPSPAC Region 24 held meetings at the Chateau on the Lake Resort in

Branson, Missouri, which is the site of the Missouri APCO Chapter’s annual

conference. 700 MHz meeting topics included NCC progress updates,

information from APCO Intl. National Conference in Salt Lake City which

introduced a packing plan for General Use spectrum to be implemented on

The NPSTC CAPRAD database.

The packing program establishes an average terrain within a county (or any

geographic area) and then determines predicted coverage based on the 40-

dBu contours. For co co-channel use, the 40-dBu contours can touch, but not

overlap the 5-dBu contour of the co channel “victim” site. County

boundaries will be used for coverage determination and terrain will be used

for interference contours. This new packing technology is estimated to have

a channel gain of five times that of the packing method employed for 800

MHz NPSPAC.

The topic of Canada’s movement onto 700 MHz and its effect on states near

Line A was discussed as well. The State of New York is leading an effort to

intervene and negotiate with the Canadian government. Other issues

discussed.

The Missouri State Highway Patrol issued a press release throughout

Missouri on this 700 MHz Regional Planning Committee meeting on August

2, 2001

They also issued an announcement on the State Law Enforcement Teletype

Network announcing the meeting and inviting all interested parties. Notices

regarding this meeting were also posted in Radio Resource magazine, MRT

magazine and the APCO Intl. magazine.

The Federal Communications Commissions Wireless Telecommunications

Bureau issued a Public Notice (DA 01-1608) on July 6, 2001 announcing this

meeting.

Minutes of meeting are on file

Next meeting set for January 10, 2002

January 10, 2002 Region 24 700 MHz Regional Planning Committee meeting was held at the

Missouri State Highway Patrol General Headquarters in Jefferson City,

Missouri on January 10, 2002 and was called to order at 0927 hrs.

An E mail message announcing the meeting for January 10, 2002 was sent to

the FCC’s WTB on 092701 to the Wireless Telecommunications Bureau

(WTB), along with the previously mentioned trade publications, however

there was no Public Notice issued by the WTB. This could have been due to

the September 11 attacks. Topics of the Region 24 700 MHz meeting are as

follows:

Acceptance of Bylaws of the Region 24 700 MHz Regional Plan

Final Decisions on content of the Regional Plan

Development of criteria needed for applicant eligibility

Update on NCC progress and current status of 700 MHz in Missouri along

with Broadcaster issues.

Updates on CAPRAD database being developed by National Public Safety

Telecommunications Council. Minutes of meeting are on file.

Next meeting set for April 11, 2002 in Kansas City, Missouri

April 11, 2002 Region 24 700 MHz Committee meeting was held in Kansas City, Missouri

at the Kansas City Police Department Communications Office. FCC Public

Notice DA 02-278 issued February 7, 2002. The Meeting minutes are on file.

A press release was issued by the State of Missouri indicating the date, time

and location of the meeting on January 31, 2002. All major industry

periodicals (Radio Resource Magazine, MFT Magazine and APCO-Public

Safety Bulletin) were notified and posted the meeting announcement in their

publications. Plan updates were discussed, as were anticipated channel

allotment parameters for the CAPRAD database general Use channels. Also

discussed were FCC designated Interoperability channels and how they

would be implemented in the region.

The uncertainty of use for the interoperability data channels was a topic of

discussion as was the future use of the 150 KHz channel aggregated data

channels. Training for the CAPRAD database will be in June and Steve

Makky of St Charles County Emergency Management, Chairman of

Technical Region 24 Subcommittee and Stephen Devine, Region 24

Chairperson will attend.

A discussion on the band plan and the location of the reserve channels

adjacent to the designated interoperability channels needed for 25 KHz

implementation ensued.

A short discussion of the Motorola Greenhouse project and adjacent TV

channel 62 provided committee members an update on DTV transition.

Meeting adjourned with next meeting scheduled for

September 24, 2002 700 MHz Regional Committee meeting held at the State Emergency

Management Agency at 10 am. Announcements were sent to Radio

Resource Magazine, APCO Public Safety Magazine and MRT Magazine as

well as the FCC’s Wireless Bureau, announcing the meeting. The Missouri

State Highway Patrol issued a news release to all the major news media in

Missouri with details of the meeting including location, time and content.

There was a discussion on the 700 MHz allotment process and how it would

allot channels to each individual county area. It was also decided that the

Regional Planning Committee Writing Group would create an allotment for

the committee to review while waiting for the NPSTC CAPRAD channel

packing plan was completed.

Wideband data standards were also discussed and several committee

members commented on NCC preliminary channel loading figures that would

require 180 users per 50 KHz wideband data channel. These figures are

preliminary and will probably be revised when better information is

available.

A meeting was called for January 10, 2003 at 10 am in the State Emergency

Management Agency. This meeting will be to review the Region 24 channel

allotment from the CAPRAD/NPSTC packing plan and the packing plan

created in by Region 24. A discussion on the benefits of each packing plan

will be encouraged.

It is anticipated Regional Planning Committee members will take both plans

to their respective regions for review and a second meeting, at the State

Emergency Management Agency’s Annual Communications Conference at

the Tan Tara Resort on February 14, will be held. At this meeting, the

Regional Plan will be reviewed in its entirety and the Regional Planning

Committee will approve one of the channel allotment plans for Region 24.

January 14, 2003 The Region 24 Regional Planning Committee held a meeting on January 10,

2003 at 10 AM to review two potential channel packing plans for Region 24.

The NYSTEC channel packing plan sponsored by the National Public Safety

Telecommunications Council (NPSTC) was reviewed as was the packing

plan created by members of the Region 24 Writing Group. A vote of the

members present indicated the Regional Planning Committee

overwhelmingly supported the packing plan developed by the Regional

Planning Committee as it provided a greater number of channels in the

metropolitan areas located within Region 24. The committee decided to vote

on the plan they preferred to use in the Region 24 Plan, and voted

(unanimously) to implement the Region 24 packing plan and the number of

channels indicated on the internally developed plan. The members in

attendance also voted in favor of including technical material, in accordance

with NCC guidelines, in the final version of the Plan so applicants could

review the Region’s expectations with regard to expected service area

coverage, system contours etc. It was decided at the January 10, 2003

meeting that the Region, under the direction of the Chairperson, should file

the Region 24 700 MHz plan with the FCC under Docket 02-378, per the

FCC’s Public Notice DA 02-3497 dated 12-31-2002.

The FCC issued a public notice on this meeting, DA 02-3195 dated

November 19, 2002.

The meeting was adjourned

April 22, 2003 Region 24 700 MHz Regional Planning Committee is again represented at the

Missouri State Emergency Management Agency Annual Conference at the

Lake of the Ozarks April 21-23, 2003. The Regional Chairperson was

provided a table in the exhibit area and displayed channel plans, information

regarding channel allotments and pamphlets supporting the 700 MHz process

in Missouri.

July 1, 2003 Region 24 held a 700 MHz meeting at the State Emergency Management

Agency facility in Jefferson City, Missouri on July 1, 2003. Items discussed

were:

The approval process for acceptance of the regional plan by the FCC and

what was the time frame involved. Chairperson Devine advised the

committee on the process of approval, adjacent region concurrence and a

time frame to expect before being able to file. The inter-regional dispute

resolution form and the purpose for obtaining adjacent state concurrence was

discussed and several questions were answered.

Chairperson Devine and Vice Chair Steve Makky discussed the CAPRAD

database and its function in assisting regional planning committees in the 700

MHz process. The committee members in attendance had questions

regarding the licensing process and channel allotments for their respective

county. All information was provided to the satisfaction of the committee.

Chairperson Devine announced that he would make the Committee aware via

the rpc24@yahoogroups.com list-serve when the plan has been filed with the

FCC.

February 4, 2004 Region 24 Chairperson Steve Devine traveled to Little Rock Arkansas to

attend the initial Region 4 (Arkansas) Regional Planning meeting. He

provided information on Missouri’s pending plan and how border issues with

Region 4, as well as other bordering regions, will be worked out through the

use of the CAPRAD channel packing sort. He also provided Region 4

attendees information on Missouri’s wideband data sort of indicated that the

sort offered a significant number of channels along Missouri’s adjacent

borders.

March 29, 2004 FCC Wireless Telecommunications Bureau returns Region 24’s plan for

several reasons and require adjacent region concurrence to be obtained from

all eight (8) adjacent states.

April 8, 2004 Region 24 files a Petition for Reconsideration with the Wireless

Telecommunications Bureau to reconsider the return of the Region 24

application. The main concern of Region 24 is the requirement of the

adjacent region coordination with the six (6) adjacent regions Region24

submitted previously.

October 2004 Region 24 Chairperson Stephen Devine speaks with FCC Wireless

Telecommunications Bureau and clarifies what Region 24 needs to

accomplish regarding its plan prior to re-filing.

December 8 2004 Region 24 700 MHz meeting held at St Louis City Police Department 1 PM.

The 700 MHz regional planning committee meeting was called to order at 1

PM. In the absence of RPC Secretary Steve Makky, Chairperson Steve

Devine took meeting minutes. Discussions on the 700 MHz regional plan

and the Missouri SIEC’s role in the administration of the 700 MHz

narrowband interoperability channels took place with the committee voting to

support the Chairperson modifying and re-submitting the 700 MHz regional

plan to the FCC. Discussions also took place on 4.9 GHz and the

Chairperson asked the RPC members in attendance what they felt was the

most appropriate was for the RPC to address 4.9 GHz regional planning. The

group was brought up to date with the FCC’s most recent document

accepting both the DSRC “A” mask and the DSRC “C” for 4.9 GHz public

safety use. They were also made aware of the FCC’s decision to not require

regional planning in the administration of 4.9 GHz public safety spectrum

and that while the FCC thinks the RPC approach might benefit the

implementation across the country, they would not mandate that users adhere

to a regional plan.

Chairperson Devine suggested a plan be filed that explained the 4.9 GHz

band, its anticipated use and benefits to the Region 24 public safety

community, the geographic licenses issued based on jurisdictional boundaries

and how those differ from previous licenses and how the RPC would be a

“clearinghouse” to the users community and assist those that wanted to

implement 4.9 GHz. The RPC is planning on utilizing the CAPRAD

database to document the use within the region, but will need the help of the

users to accomplish this.

The RPC members in attendance supported this approach and recommended

the Chairperson DRAFT a 4.9 GHz plan that included guidelines for use and

explained how the RPC would not develop a plan, but rather assist in the

development in the band while documenting its use across Region 24.

**Meeting adjourned at 250 PM CST**

March 7, 2005 Region 24 re-files 700 MHz plan with FCC WTB

**Appendix E**

**Table of Interoperability Channels**

NOTE: The interoperability nomenclature identified below is for reference only

pending finalization of channel labeling recommendations currently before the FCC.

These recommendations originated from the National Coordination Committee

(NCC) Interoperability Subcommittee asking for standardized channel nomenclature

and labeling. The Federal Communications Commission’s decisions on channel

labeling can alter these values accordingly. The FCC designated 700 MHz

interoperability channels will be administered by the Missouri Statewide

Interoperability Executive Committee with Federal Communications Commission

rules. The FCC’s final ruling on interoperability channel labeling and interoperability

channel designations and the Missouri Statewide Interoperability Executive

Committee interpretation of those rules take precedence over any Region 24

recommendation in this plan.

**For Specific Uses/Services**

**16 CHANNEL**

**SETS**

**DESCRIPTION LABEL**

*Channel 23 & 24 General Public Safety Services (secondary*

*trunked)*

*7TAC58*

*Channel 103 & 104 General Public Safety Services (secondary*

*trunked)*

*7TAC62*

*Channel 183 & 184 General Public Safety Services (secondary*

*trunked)*

*7TAC66*

*Channel 263 & 264 General Public Safety Services (secondary*

*trunked)*

*7TAC70*

Channel 39 &40 Calling Channel 7CALL1

Channel 119 & 120 General Public Safety Service 7TAC63

Channel 199 & 200 General Public Safety Service 7TAC67

Channel 279 & 280 Mobile Data 7DAT71

Channel 63 & 64 Emergency Medical Service 7EMS60

Channel 143 & 144 Fire Service 7FIR64

Channel 223 & 224 Law Enforcement Service 7LAW68

Channel 303 & 304 Mobile Repeater 7MOB68

Channel 79 & 80 Emergency Medical Service 7EMS61

Channel 159 & 160 Fire Service 7FIR65

Channel 239 & 240 Law Enforcement Service 7LAW69

Channel 319 & 320 Other Public Service 7TAC73

*Channel 657 & 658 General Public Safety Services (secondary*

*trunked)*

*7TAC74*

*Channel 737 & 738 General Public Safety Services (secondary*

*trunked)*

*7TAC78*

*Channel 817 & 818 General Public Safety Services (secondary*

*trunked)*

*7TAC82*

*Channel 897 & 898 General Public Safety Services (secondary*

*trunked)*

*7TAC86*

Channel 681 & 682 Calling Channel 7CALL2

Channel 761 & 762 General Public Safety Service 7TAC79

Channel 841 & 842 General Public Safety Service 7TAC83

Channel 921 & 922 Mobile Data 7DAT87

Channel 641 & 642 Emergency Medical Service 7EMS76

Channel 721 & 742 Fire Service 7FIR80

Channel 801 & 802 Law Enforcement Service 7LAW84

Channel 881 & 882 Mobile Data 7MOB88

Channel 697 & 698 Emergency Medical Service 7EMS77

Channel 777 & 778 Fire Services 7FIR81

Channel 857 & 858 Law Enforcement Service 7LAW85

Channel 937 & 938 Other Public Services 7TAC89

*Trunking is permitted on the 10 channel sets indicated in italic*

**Project 25 Common Air Interface**

**Interoperability channel parameters**

Certain common P25 parameters need to be defined to ensure digital radios operating on the 700

MHz Interoperability Channels can communicate. This is analogous to defining the common

CTCSS tone used on NPSPAC analog Interoperability channels.

**Network Access Code**

In the Project 25 Common Air Interface definition, the Network Access Code is analogous

to the use of CTCSS and CDCSS signals in analog radio systems. It is a code transmitted in the

pre-amble of the P25 signal and repeated periodically throughout the transmission. Its purpose is to

provide selective access to and maintain access to a receiver. It is also used to block nuisance and

other co-channel signals. There are up to 4096 of these NAC codes. For ease of migration in other

frequency bands, a NAC code table was developed which shows a mapping of CTCSS and CDCSS

signals into corresponding NAC codes. Document TIA/EIA TSB102.BAAC contains NAC code

table and other Project 25 Common Air Interface Reserve Values.

Use of corresponding NAC code $293 is required for the 700 MHz Interoperability Channel NAC

code.

**Talk group ID**

In the Project 25 Common Air Interface definition, the Talk group ID on conventional

channels is analogous to the use of talk groups in trunking. In order to ensure that all users can

communicate, all units should use a common Talk group ID.

Recommendation: Use P25 default value for Talk group ID = $0001

**Manufacturer's ID**

The Project 25 Common Air Interface allows the ability to define manufacturer specific

functions. In order to ensure that all users can communicate, all units should not use a specific

Manufacturer's ID, but should use the default value of $00.

**Message ID**

The Project 25 Common Air Interface allows the ability to define specific message

functions. In order to ensure that all users can communicate, all units should use the default

Message ID for unencrypted messages of $00000000000000000000.

**Encryption Algorithm ID and Key ID**

The Project 25 Common Air Interface allows the ability to define specific encryption

algorithms and encryption keys. In order to ensure that all users can communicate, encryption

should not be used on the Interoperability Calling Channels, all units should use the default

Algorithm ID for unencrypted messages of $80 and default Key ID for unencrypted messages 0000.

These same defaults may be used for the other Interoperability channels when encryption is not

used.

Use of encryption is allowed on the other Interoperability channels. Regional Planning

Committees need to define appropriate Message ID, Encryption Algorithm ID, and Encryption Key

ID to be used in the encrypted mode on Interoperability channels.

**Appendix F**

**NCC 700 MHz Pre-Assignment Rules/Recommendations**

**Introduction**

A process for doing the initial block assignments of 700 MHz channels before details of actual

system deployments is required. In this initial phase, there is little actual knowledge of what

specific equipment is to be deployed and where the sites will be. As a result, a high level simplified

method is proposed to establish guidelines for frequency coordination. When actual systems are

deployed, additional details will be known and the system designers will be required to select

specific sites and supporting hardware to control interference.

Overview

Assignments will be based on a defined service area of each applicant. For Public Safety entities

this will normally be a geographically defined area such as city, county or by a data file consisting

of line segments creating a polygon that encloses the defined area. TIA/EIA TSB88-A (or latest

version) will be used to determine harmful interference assuming 40 dBμ, or greater, signal in all

systems coverage areas.

For co-channel assignments, the 40dBμ contour will be allowed to extend beyond the defined

service area by 3 to 5 miles, depending on the type of environment, urban, suburban or low density.

The interfering co-channel 15 dBμ contour will be allowed to touch but not overlap the 40 dBμ

contour of the system being evaluated. All contours are (50,50). TIA/EIA TSB88-A (or latest

version) will be used to determine harmful interference assuming 40 dBμ, or greater, signal in all

systems coverage areas.

For adjacent and alternate channels, the interfering channels 60 dBμ will be allowed to touch but

not overlap the 40 dBμ contour of the system being evaluated. All contours are (50,50). TIA/EIA

TSB88-A (or latest version) will be used to determine harmful interference assuming 40 dBμ, or

greater, signal in all systems coverage areas.

**7.4.1.1 Discussion**

The FCC limits the maximum field strength to 40 dB relative to 1μV/m (customarily denoted as 40

dBμ). It is assumed that this limitation will be applied similarly to the way it is applied in the 821-

824/866/869 MHz band. That is, a 40 dBμ field strength can be deployed up to a defined distance

from the edge of the service area, based on the size of the service area or type of applicant, i.e. city,

county or statewide system. This is important as the potential for interference from CMRS

infrastructure demands that public safety systems have adequate margins for reliability in the

presence of interference. The value of 40 dBμ corresponds to a signal of -92.7 dBm, received by a

half-wavelength dipole (λ/2) antenna. The thermal noise floor for a 6.25 kHz receiver would be in

the range of -126 dBm, so there is a margin of approximately 33 dB available for “noise limited”

reliability. Figure 1 shows show the various interfering sources and how they accumulate to form a

composite noise floor that can be used to determine the “reliability” or probability of achieving the

desired performance in the presence of various interfering sources with differing characteristics.

Allowing for a 3 dB reduction in the available margin due to CMRS OOBE noise lowers the

reliability and/or the channel performance of Public Safety systems. TIA TR8 made this allowance

during the meetings in Mesa, AZ, January 2001. In addition, there are various channel bandwidths

with different performance criteria and unknown adjacent and alternate channel assignments need to

be accounted for. The co-channel and adjacent/alternate sources are shown in the right hand side

of Figure 1. There would be a single co-channel source, but potentially several adjacent or alternate

channel sources involved.

Desired Signal Level

C/I, 1%

Multiple Sources

Multiple bandwidths

Receiver kTb + NF (dB)

-126 dBm (6.25 kHz)

CMRS Site Noise)

C/N

Determines

performance &

reliability

C/N - 3 dB

Joint Probability

Determines

ultimate

performance &

reliability

Figure 1 - Interfering Sources Create A “Noise” Level Influencing Reliability

It is recommended that co-channel assignments limit the C/I at the edge (worst case mile) be

sufficient to limit that interference to <1%. A C/I ratio of 26.4 dB plus the required capture value

required to achieve this goal.. A 17 - 20 dB C/N is required to achieve channel performance. Table

1 shows estimated performance considering the 3 dB noise floor rise at the 40 dBμ signal level.

Performance varies due to the different Cf/N requirements of the different modulations and channel

bandwidths. These values are appropriate for a mobile on the street, but are considerably short to

provide reliable communications to portables inside buildings.

Channel Bandwidth 6.25 kHz 12.5 kHz 12.5 kHz 25.0 kHz

Receiver ENBW (kHz) 6 6 9 18

Noise Figure(10 dB) 10 10 10 10

Receiver Noise Floor (dBm) -126.22 -126.22 -124.46 -121.45

Rise in Noise Floor (dB) 3.00 3.00 3.00 3.00

New Receiver Noise Floor (dB) -123.22 -123.22 -121.46 -118.45

40 dBu = -92.7 dBm -92.7 -92.7 -92.7 -92.7

Receiver Capture (dB) 10.0 10.0 10.0 10.0

Noise Margin (dB) 30.52 30.52 28.76 25.75

C/N Required for DAQ = 3 17.0 17.0 18.0 20.0

C/N Margin (dB) **13.52 13.52 10.76 5.75**

Standard deviation (8 dB) 8.0 8.0 8.0 8.0

Z 1.690 1.690 1.345 0.718

Noise Reliability (%) **95.45% 95.45% 91.06% 76.37%**

C/I for <1% prob of capture 36.4 36.4 36.4 36.4

I (dBu) 3.7 3.7 3.7 3.7

I (dBm) -129.0 -129.0 -129.0 -129.0

Joint Probability (C & I) **94.2% 94.2% 90.4% 75.8%**

40 dBu = -92.7 dBm @ 770 MHz

**Comparison of Joint Reliability for various configurations**

Table 1 Joint Probability For Project 25, 700 MHz Equipment Configurations.

To analyze the impact of requiring portable in building coverage, several scenarios are presented.

The different scenarios involve a given separation from the desired sites. Then the impact of

simulcast is included to show that the 40 dBμ must be able to fall outside the edge of the service

area. From the analysis, recommendations of how far the 40 dBμ extensions should be allowed to

occur are made.

Table 2 Estimates urban coverage where simulcast is required to achieve the desired portable in

building coverage. Several assumptions are required to use this estimate.

• Distance from the location to each site. Equal distance is assumed.

• CMRS noise is reduced when entering buildings. This is not a guarantee as the type of

deployments is unknown. It is possible that CMRS units may have transmitters inside

buildings. This could be potentially a large contributor unless the CMRS OOBE is suppressed

to TIA’s most recent recommendation and the “site isolation” is maintained at 65 dB minimum.

• The 40 dBμ is allowed to extend beyond the edge of the service area boundary.

• Other configurations may be deployed utilizing additional sites, lower tower heights, lower ERP

and shorter site separations.

Estimated Performance at 2.5 miles from each site

Channel Bandwidth 6.25 kHz 12.5 kHz 12.5 kHz 25.0 kHz

Receiver Noise Floor (dBm) -126.20 -126.20 -124.50 -118.50

Signal at 2.5 miles (dBm) -72.7 -72.7 -72.7 -72.7

Margin (dB) 53.50 53.50 51.80 45.80

C/N Required for DAQ = 3 17.0 17.0 18.0 20.0

Building Loss (dB) 20 20 20 20

Antenna Loss (dBd) 8 8 8 8

Reliability Margin 8.50 8.50 5.80 -2.20

Z 1.0625 1.0625 0.725 -0.275

Single Site Noise Reliability

(%)

**85.60% 85.60% 76.58% 39.17%**

Simulcast with 2 sites 97.93% 97.93% 94.51% 62.99%

Simulcast with 3 sites 99.70% 99.70% 98.71% 77.49%

Simulcast with 4 sites 99.96% 99.96% 99.70% 86.30%

Table 2, Estimated Performance From Site(s) 2.5 Miles From Typical Urban Buildings.

Table 2 shows for the example case of 2.5 miles that simulcast is required to achieve public safety

levels of reliability. The difference in performance margin requirements would require more sites

and closer site-to-site separation for wider bandwidth channels.

Figures 2 and 3 show how the configurations would potentially be deployed for a typical site with

240 Watts ERP. This is based on:

• 75 Watt transmitter, 18.75 dBW

• 200 foot tower

• 10 dBd 180 degree sector antenna +10.0 dBd

• 5 dB of cable/filter loss. - 5.0 dB

23.75 dBW ≈ 240 Watts (ERPd)

Jurisdiction

5 miles wide

30.1 dBμ

21.6 dBμ

23.6 dBμ

40.1 dBμ

41.6 dBμ

43.3 dBμ

-72.7 dBm

60.1 dBμ

Figure 2 - Field Strength From Left Most Site.

Figure 3 - Antenna Configuration Required To Limit Field Strength Off “Backside”

Figure 2 is for an urbanized area with a jurisdiction of a 5-mile circle. To provide the necessary

coverage to portables in buildings at the center of the jurisdiction requires that the sites be placed

along the edge of the service area utilizing direction antennas oriented toward the center of the

service area (Figure 3). In this case, at 5 miles beyond the edge of the service area, the sites would

produce composite field strength of approximately 40 dBμ. Since one site is over 10 dB dominant,

the contribution from the other site is not considered. The control of the field strength behind the

site relies on a 20 dB antenna with a Front to Back Ratio (F/B) specification as shown in Figure 3.

This performance may be optimistic due to backscatter off local obstructions in urbanized areas.

However, use of antennas on the sides of buildings can assist in achieving better F/B ratios and the

initial planning is not precise enough to prohibit using the full 20 dB.

The use of a single site at the center of the service area is not normally practical. To provide the

necessary signal strength at the edge of the service area would produce field strength 5 miles

beyond in excess of 44 dBμ. However, if the high loss buildings were concentrated at the service

area’s center, then potentially a single site could be deployed, assuming that the building loss

sufficiently decreases near the edge of the service area allowing a reduction in ERP to achieve the

desired reliability.

The down tilting of antennas to control the 40 dBμ is not practical as the difference in angular

discrimination from a 200-foot tall tower at 2.5 miles and 10 miles is approximately 0.6 degrees.

Tables 3 and 4 represent the same configuration, but for less dense buildings. In these cases, the

distance to extend the 40 dBm can be determined from Table Z. Recommendations are made in

Table 6.

Channel Bandwidth 6.25 kHz 12.5 kHz 12.5 kHz 25.0 kHz

Receiver Noise Floor (dBm) -126.20 -126.20 -124.50 -118.50

Signal at 2.5 miles (dBm) -77.7 -77.7 -77.7 -77.7

Margin (dB) 48.50 48.50 46.80 40.80

C/N Required for DAQ = 3 17.0 17.0 18.0 20.0

Building Loss (dB) 15 15 15 15

Antenna Loss (dBd) 8 8 8 8

Reliability Margin 8.50 8.50 5.80 -2.20

Z 1.0625 1.0625 0.725 -0.275

Single Site Noise Reliability (%) **85.60% 85.60% 76.58% 39.17%**

Simulcast with 2 sites 97.93% 97.93% 94.51% 62.99%

Simulcast with 3 sites 99.70% 99.70% 98.71% 77.49%

Simulcast with 4 sites 99.96% 99.96% 99.70% 86.30%

Estimated Performance at 3.5 miles from each site

Table 3 - Lower Loss Buildings, 3.5 Mile From Site(s)

Channel Bandwidth 6.25 kHz 12.5 kHz 12.5 kHz 25.0 kHz

Receiver Noise Floor (dBm) -126.20 -126.20 -124.50 -118.50

Signal at 2.5 miles (dBm) -82.7 -82.7 -82.7 -82.7

Margin (dB) 43.50 43.50 41.80 35.80

C/N Required for DAQ = 3 17.0 17.0 18.0 20.0

Building Loss (dB) 10 10 10 10

Antenna Loss (dBd) 8 8 8 8

Reliability Margin 8.50 8.50 5.80 -2.20

Z 1.0625 1.0625 0.725 -0.275

Single Site Noise Reliability (%) **85.60% 85.60% 76.58% 39.17%**

Simulcast with 2 sites 97.93% 97.93% 94.51% 62.99%

Simulcast with 3 sites 99.70% 99.70% 98.71% 77.49%

Simulcast with 4 sites 99.96% 99.96% 99.70% 86.30%

Estimated Performance at 5.0 miles from each site

Table 4 - Low Loss Buildings, 5.0 Miles From Site(s)

Note that the receive signals were adjusted to offset the lowered building penetration loss. This

produces the same numerical reliability results, but allows increasing the site to building separation

and this in turn lowers the magnitude of the “overshoot” across the service area.

Table 5 shows the field strength for a direct path and for a path reduced by a 20 dB F/B antenna.

This allows the analysis to be simplified for the specific example being discussed.

Overshoot Distance (mi) Field Strength

(dBμ)

20 dB F/B

(dBμ)

1 73.3 53.3

2 63.3 43.3

2.5 60.1 40.1

3 57.5 37.5

4 53.3 33.5

5 50.1 30.1

**… …**

10 40.1

11 38.4

12 37.5

13 36.0

14 34.5

15 33.0

Table 5 - Field Strength Vs. Distance From Site

This allows the overshoot to be 11 miles so the extension of the 40 dbm can be 4 miles for

suburbanized territory. For the more rural territory, the limit is the signal strength off the back of

the antenna. So the result is that for various types of urbanized areas the offset of the 40 dbm

should be:

Type of Area Extension (mi.)

Urban (20 dB Buildings) 5

Suburban (15 dB

Buildings)

4

Rural (10 dB Buildings) 3

Table 6 - Recommended Extension Distance Of 40 Dbμ Field Strength

The 40 dBμ can then be constructed based on the defined service area without having to perform an

actual prediction. Since the 40 dBμ is beyond the edge of the service area, some relaxation in the

level of I is reasonable. Therefore a 35 dB ration is recommended and is consistent with what is

currently being licensed in the 821-824/866-869 MHz Public Safety band.

Region 24 700 MHz Plan Amended Dec 28, 2007

Main Section Page 69

Co-Channel Recommendation

• Allow the constructed 40 dBμ (50,50) to extend beyond the edge of the defined service area by

the distance indicated in Table 6.

• Allow the Interfering 15 dBμ (50,50) to intercept but not overlap the 40 dBμ contour.

Figure 4 - Co-Channel Reuse Criterion

**Adjacent and alternate Channel Considerations**

Adjacent and alternate channels are treated as being noise sources that alter the composite noise

floor of a victim receiver. Using the 47 CFR § 90.543 values of ACCP can facilitate the

coordination of adjacent and alternate channels. The C/I requirements for <1% interference can be

reduced by the value of ACCPR. For example to achieve an X dB C/I for the adjacent channel that

is -40 dBc a C/I of [X-40] dB is required. Where the alternate channel ACP value is -60 dBc, then

the C/I = [X-60] dB is the goal for assignment(s). There is a compounding of interference energy,

as there are numerous sources, i.e. co channel, adjacent channels and alternate channels plus the

noise from CMRS OOBE.

There is insufficient information in 47 CFR § 90.543 to include the actual receiver performance.

Receivers typically have “skirts” that allow energy outside the bandwidth of interest to be received.

In addition, the FCC defines ACCP differently than does the TIA. The term used by the FCC is the

same as the TIA definition of ACP. The subtle difference is that ACCP defines the energy

intercepted by a defined receiver filter. ACP defines the energy in a measured bandwidth that is

typically wider than the receiver. As a result, the FCC values are optimistic at very close spacing

and somewhat pessimistic at wider spacing, as the typical receiver filter is less than the channel

bandwidth.

**Site**

**Separation**

**5 dBu(50,50)**

**Interference Contour**

Service Area

40 dBu (50,50)

Service Area + 3/5 miles

700 MHz Co- Channel Reuse

In addition, as a channel bandwidth is increased, the total noise is allowed to rise, as it is initially

defined in a 6.25 kHz channel bandwidth. However, the effect is diminished at very close spacing

as the noise is rapidly falling off. At greater spacing, the noise is essentially flat and the receiver’s

filter limits the noise to the specified 3 dB rise in the thermal noise floor.

Digital receivers tend to be less tolerant to interference than analog. Therefore a 3 dB reduction in

the C/(I+N) can reduce a DAQ = 3 to a DAQ = 2 which is threshold to complete receiver muting.

Therefore at least 17 dB plus the margin for keeping the interference below 1% probability requires

a total margin of 43.4 dB. However, this margin would be at the edge of the service area and the 40

dBμ is allowed to extend past the edge of the service area.

Frequency drift is controlled by the FCC requirement for 0.4-ppm stability when locked. This

equates to approximately a 1 dB standard deviation, which is negligible when associated with the

recommended initial lognormal standard deviation of 8 dB and can be ignored.

Project 25 requires that a transceiver receiver have an ACIPR of 60 dB. This implies that an

ACCPR ≥ 65 dB will exist for a “companion receiver”. A companion receiver is one that is

designed for the specific modulation. At this time the highest likelihood is that receivers will be

deploying the following receiver bandwidths at the following channel bandwidths.

Estimated Receiver Parameters

Channel Bandwidth Receiver Bandwidth

6.25 kHz 5.5 kHz

12.5 kHz 5.5 or 9 kHz

25 kHz 18.0 kHz

Table 7 - Estimated Receiver Parameters

Based on 47 CFR ¶ 90.543 and the P25 requirement for an ACCPR ≥ 65 dB into a 6.0 kHz channel

bandwidth and leaving room for a migration from Phase 1 to Phase 2, allows for making the

simplifying assumption that 65 dB ACCPR is available for both adjacent 25 kHz block.

Figure 5, Potential Frequency Separations

Base initial (presorts) on 25 kHz channels. This provides the maximum flexibility by using 65 dB

ACCPR for all but one possible combination of 6.25 kHz channels within the 25 kHz allotment.

Case ACCPR

25 kHz 65 dB

18.725 kHz 65 dB

15.625 kHz >40 dB

12.5 kHz 65 dB

9.375 kHz >40 dB

6.25 kHz 65 dB

Table 8 - ACCPR Values For Potential Frequency Separations

All cases meet or exceed the FCC requirement. The most troublesome cases occur where the wider

bandwidths are working against a Phase 2 narrowband 6.25 kHz channel. If system designers keep this

consideration in mind and move the edge 6.25 kHz channels inward on their own systems, then a constant

value of 65 dB ACCPR can be applied across all 25 kHz channels regardless of what is eventually deployed.

For other blocks, it must be assumed that transmitter filtering in addition to transmitter performance

improvements with greater frequency separation will further reduce the ACCPR.

Therefore it is recommended that a consistent value of 65 dB ACCPR be used for coordinating adjacent 25

kHz channel blocks. Rounding to be conservative due to the possibility of multiple sources allows the “I”

contour to be approximately 20 dB above the 40 dBμ contour, 60 dBμ.

A B

1 2 3 4 1 2 3 4

**25.0**

**12.5**

**9.375**

**6.25**

**15.625**

**18.725**

Desired Signal [C]

40 dBμ

Interfering Signal [I]

Requirement for <1%

26.4 + 17 = 43.4 dB

Allowable I

40 dBμ - 43.4 + 65 ≈ **60 dB**μ

ACCPR = 65 dB

Figure 6 - Adjusted Adjacent 25 kHz Channel Interfering Contour Value

An adjacent Interfering (25 kHz) channel shall be allowed to have its 60 dBμ (50,50) contour touch

but not overlap the 40 dBμ (50,50) contour of a system being evaluated. Evaluations should be

made in both directions.

Figure 7 - Example Of Adjacent/Alternate Overlap Criterion

65 dB ACCPR, Based on P25 Requirements of 60 dB ACIPR

Site Separation (D)

60 dBμ= 0.23 D

38.5 Log(0.77/0.23)≈ 20 dB

C/I = -20 dB

40 dBμ= 0.77 D

This simple method is only adequate for presorting large blocks to potential entities. A more

detailed analysis should be executed in the actual design phase to take all the issues into

consideration. Additional factors that should be considered include:

• Degree of Service Area Overlap

• Different size of Service Areas

• Different ERP’s and HAAT’s

• Actual Terrain and Land Usage

• Differing User Reliability Requirements

• Migration from Project 25 Phase 1 to Phase 2

• Actual ACCP

• Balanced Systems

• Mobiles vs. Portables

• Use of voting

• Use of simulcast

• Radio specifications

• Simplex Operation

• Future unidentified requirements.

Special attention needs to be paid to the use of simplex operation. In this case, an interferer can be

on an offset adjacent channel and in extremely close proximity to the victim receiver. This is

especially critical in public safety where simplex operations are frequently used at a fire scene or

during police operation. This type operation is also quite common in the lower frequency bands. In

those cases, evaluation of base-to-base as well as mobile-to-mobile interference should be

considered and evaluated.

Carrier to Interference Requirements

There are two different ways that interference is considered.

• Co Channel

• Adjacent and Alternate Channels

Both involve using a C/I ratio. The C/I ratio requires a probability be assigned. For example, a

10% Interference is specified; the C/I implies 90% probability of successfully achieving the desired

ratio. At 1% interference, means that there is a 99% probability of achieving the desired C/I.

*C*

*I*

% = • *erfc*

⎛

⎝

⎜⎜⎜

⎞

⎠

⎟⎟⎟

1

2

C

I

margin

2σ

(1)

This can also be written in a form using the standard deviate unit (*Z*). In this case the *Z* for the

desired probability of achieving the C/I is entered. For example, for a 90% probability of achieving

the necessary C/I, *Z* = 1.28.

*C*

*I*

% = *Z* ⋅ 2 ⋅σ (2)

The most common requirements for several typical lognormal standard deviations (σ) are included

in the following table based on Equation (2).

Location Standard Deviation (σ)

dB 5.6 6.5 8 10

Probability %

10% 10.14 dB 11.77 dB 14.48 dB 18.10 dB

5% 13.07 dB 15.17 dB 18.67 dB 23.33 dB

4% 13.86 dB 16.09 dB 19.81 dB 24.76 dB

3% 14.90 dB 17.29 dB 21.28 dB 26.20 dB

2% 16.27 dB 18.88 dB 23.24 dB 29.04 dB

1% 18.45 dB 21.42 dB 26.36 dB 32.95 dB

Table A1 - Probability Of Not Achieving C/I For Various Location Lognormal Standard Deviations

**Probability of Achieving Required C/I verses Mean C/I as a Funcation of**

**Location Lognormal Standard deviation (does not include C/N requirement)**

0.1

1

10

100

0 5 10 15 20 25 30 35 40

**C/I (dB)**

**Interference Probability (%)**

10

8

6.5

5.6

5

Figure A1, Probability Of Achieving Required C/I As A Function Of Location Standard Deviation

For co-channel the margin needs to include the “capture” requirement. When this is done, then a 1%

probability of co channel interference can be rephrased to mean, there is a 99% probability that the “capture

ratio” will be achieved. The capture ratio varies with the type of modulation. Older analog equipment has a

capture ratio of approximately 7 dB. Project 25 FDMA is specified at 9 dB. Figure A1 shows the C/I

requirement without including the capture requirement.

The 8 dB values for lognormal location standard deviation is reasonable when little information is

available. Later when a detailed design is required, additional details and high-resolution terrain

and land usage databases will allow a lower value to be used. The TIA recommended value is 5.6

dB. This provides the additional flexibility necessary to complete the design

To determine the desired probability that both the C/N and C/I will be achieved requires that a joint

probability be determined. Figure A2 shows the effects of a family of various levels of C/N

reliability and the joint probability (Y-axis) in the presence of various probabilities of Interference.

Note that at 99% reliability with 1% interference (X-axis) that the reduction is nearly the difference.

This is because the very high noise reliability is degraded by the interference, as there is little

probability that the noise criterion will not be satisfied. At 90%, the 1% interference has a greater

likelihood that it will occur simultaneously when the noise criterion not being met, resulting is a less

degradation of the 90%

**Joint Probability [8 dB Standard Deviation]**

84

85

86

87

88

89

90

91

92

93

94

95

96

97

98

99

100

0 1 2 3 4 5 6 7 8 9 10

**Probability of Interference [%]**

**Joint Probability [%]**

90%

91%

92%

93%

94%

95%

96%

97%

98%

99%

Figure A2 - Effect Of Joint Probability On The Composite Probability

For adjacent and alternate channels, the channel performance requirement must be added to the C/I

ratio. When this is applied, then a 1% probability of adjacent/alternate channel interference can be

rephrased to mean, there is a 99% probability that the “channel performance ratio” will be achieved.

**Appendix G**

**The Region 24 Channel allocations have been established by the National Public Safety**

**Telecommunications Council’s channel packing program. Region 24 anticipates an open**

**filing window where applicants can apply for available channels in their county area, until all**

**channels are depleted. A “County Area” is defined as an area consisting of the area within**

**the county as well as a distance of up to 10 miles outside of the county. It is anticipated this**

**extended county area will enable Region 24 to maximize channel re-use of any “orphan”**

**remainders.**

12/16/2007 Region 24

Channel Allotments

-----------------------------------------------------------------------------------------------------------

General Use

-----------------------------------------------------------------------------------------------------------

FCC Channel Base New New

County Band Number Frequency Base Mobile

Adair Voice 25KHz 17-20 769.1125 799.1125

Voice 25KHz 57-60 769.3625 799.3625

Voice 25KHz 125-128 769.7875 799.7875

Voice 25KHz 177-180 770.1125 800.1125

Voice 25KHz 281-284 770.7625 800.7625

Voice 25KHz 329-332 771.0625 801.0625

Voice 25KHz 385-388 771.4125 801.4125

Voice 25KHz 437-440 771.7375 801.7375

Voice 25KHz 477-480 771.9875 801.9875

Voice 25KHz 501-504 772.1375 802.1375

Voice 25KHz 577-580 772.6125 802.6125

Voice 25KHz 617-620 772.8625 802.8625

Voice 25KHz 709-712 773.4375 803.4375

Voice 25KHz 793-796 773.9625 803.9625

Voice 25KHz 861-864 774.3875 804.3875

Voice 25KHz 913-916 774.7125 804.7125

Andrew Voice 25KHz 93-96 769.5875 799.5875

Voice 25KHz 173-176 770.0875 800.0875

Voice 25KHz 281-284 770.7625 800.7625

Voice 25KHz 353-356 771.2125 801.2125

Voice 25KHz 397-400 771.4875 801.4875

Voice 25KHz 437-440 771.7375 801.7375

Voice 25KHz 597-600 772.7375 802.7375

Voice 25KHz 673-676 773.2125 803.2125

Voice 25KHz 797-800 773.9875 803.9875

Voice 25KHz 861-864 774.3875 804.3875

Voice 25KHz 945-948 774.9125 804.9125

Atchison Voice 25KHz 341-344 771.1375 801.1375

Voice 25KHz 385-388 771.4125 801.4125

Voice 25KHz 509-512 772.1875 802.1875

Voice 25KHz 589-592 772.6875 802.6875

Voice 25KHz 717-720 773.4875 803.4875

Voice 25KHz 825-828 774.1625 804.1625

Audrain Voice 25KHz 97-100 769.6125 799.6125

Voice 25KHz 245-248 770.5375 800.5375

Voice 25KHz 329-332 771.0625 801.0625

Voice 25KHz 421-424 771.6375 801.6375

Voice 25KHz 465-468 771.9125 801.9125

Voice 25KHz 513-516 772.2125 802.2125

Voice 25KHz 617-620 772.8625 802.8625

Voice 25KHz 705-708 773.4125 803.4125

Voice 25KHz 821-824 774.1375 804.1375

Voice 25KHz 901-904 774.6375 804.6375

Barry Voice 25KHz 49-52 769.3125 799.3125

Voice 25KHz 169-172 770.0625 800.0625

Voice 25KHz 289-292 770.8125 800.8125

Voice 25KHz 357-360 771.2375 801.2375

Voice 25KHz 473-476 771.9625 801.9625

Voice 25KHz 481-484 772.0125 802.0125

Voice 25KHz 537-540 772.3625 802.3625

Voice 25KHz 625-628 772.9125 802.9125

Voice 25KHz 901-904 774.6375 804.6375

Voice 25KHz 941-944 774.8875 804.8875

Barton Voice 25KHz 125-128 769.7875 799.7875

Voice 25KHz 321-324 771.0125 801.0125

Voice 25KHz 369-372 771.3125 801.3125

Voice 25KHz 513-516 772.2125 802.2125

Voice 25KHz 569-572 772.5625 802.5625 Campus

Voice 25KHz 701-704 773.3875 803.3875

Voice 25KHz 705-708 773.4125 803.4125 Campus

Voice 25KHz 789-792 773.9375 803.9375

Bates Voice 25KHz 89-92 769.5625 799.5625

Voice 25KHz 325-328 771.0375 801.0375 Campus

Voice 25KHz 333-336 771.0875 801.0875

Voice 25KHz 377-380 771.3625 801.3625 Campus

Voice 25KHz 417-420 771.6125 801.6125

Voice 25KHz 465-468 771.9125 801.9125 Campus

Voice 25KHz 473-476 771.9625 801.9625

Voice 25KHz 509-512 772.1875 802.1875

Voice 25KHz 521-524 772.2625 802.2625 Campus

Voice 25KHz 633-636 772.9625 802.9625 Campus

Voice 25KHz 677-680 773.2375 803.2375

Voice 25KHz 717-720 773.4875 803.4875 Campus

Voice 25KHz 741-744 773.6375 803.6375

Voice 25KHz 821-824 774.1375 804.1375 Campus

Voice 25KHz 833-836 774.2125 804.2125 Campus

Voice 25KHz 869-872 774.4375 804.4375

Voice 25KHz 909-912 774.6875 804.6875

Benton Voice 25KHz 81-84 769.5125 799.5125

Voice 25KHz 257-260 770.6125 800.6125

Voice 25KHz 297-300 770.8625 800.8625

Voice 25KHz 341-344 771.1375 801.1375

Voice 25KHz 345-348 771.1625 801.1625 Campus

Voice 25KHz 369-372 771.3125 801.3125 Campus

Voice 25KHz 381-384 771.3875 801.3875

Voice 25KHz 425-428 771.6625 801.6625

Voice 25KHz 477-480 771.9875 801.9875 Campus

Voice 25KHz 497-500 772.1125 802.1125

Voice 25KHz 501-504 772.1375 802.1375 Campus

Voice 25KHz 541-544 772.3875 802.3875 Campus

Voice 25KHz 565-568 772.5375 802.5375 Campus

Voice 25KHz 569-572 772.5625 802.5625

Voice 25KHz 785-788 773.9125 803.9125 Campus

Bollinger Voice 25KHz 41-44 769.2625 799.2625

Voice 25KHz 177-180 770.1125 800.1125

Voice 25KHz 357-360 771.2375 801.2375

Voice 25KHz 517-520 772.2375 802.2375

Voice 25KHz 829-832 774.1875 804.1875

Boone Voice 25KHz 41-44 769.2625 799.2625

Voice 25KHz 81-84 769.5125 799.5125

Voice 25KHz 137-140 769.8625 799.8625

Voice 25KHz 177-180 770.1125 800.1125

Voice 25KHz 217-220 770.3625 800.3625

Voice 25KHz 257-260 770.6125 800.6125

Voice 25KHz 297-300 770.8625 800.8625

Voice 25KHz 349-352 771.1875 801.1875

Voice 25KHz 389-392 771.4375 801.4375

Voice 25KHz 437-440 771.7375 801.7375

Voice 25KHz 477-480 771.9875 801.9875

Voice 25KHz 501-504 772.1375 802.1375

Voice 25KHz 549-552 772.4375 802.4375

Voice 25KHz 625-628 772.9125 802.9125

Voice 25KHz 665-668 773.1625 803.1625

Voice 25KHz 713-716 773.4625 803.4625

Voice 25KHz 785-788 773.9125 803.9125

Voice 25KHz 833-836 774.2125 804.2125

Voice 25KHz 873-876 774.4625 804.4625

Voice 25KHz 913-916 774.7125 804.7125

Buchanan Voice 25KHz 121-124 769.7625 799.7625

Voice 25KHz 161-164 770.0125 800.0125

Voice 25KHz 201-204 770.2625 800.2625

Voice 25KHz 253-256 770.5875 800.5875

Voice 25KHz 333-336 771.0875 801.0875

Voice 25KHz 389-392 771.4375 801.4375

Voice 25KHz 473-476 771.9625 801.9625

Voice 25KHz 497-500 772.1125 802.1125

Voice 25KHz 537-540 772.3625 802.3625

Voice 25KHz 577-580 772.6125 802.6125

Voice 25KHz 633-636 772.9625 802.9625

Voice 25KHz 749-752 773.6875 803.6875

Voice 25KHz 789-792 773.9375 803.9375

Voice 25KHz 913-916 774.7125 804.7125

Butler Voice 25KHz 45-48 769.2875 799.2875

Voice 25KHz 133-136 769.8375 799.8375

Voice 25KHz 201-204 770.2625 800.2625

Voice 25KHz 249-252 770.5625 800.5625

Voice 25KHz 345-348 771.1625 801.1625

Voice 25KHz 445-448 771.7875 801.7875

Voice 25KHz 501-504 772.1375 802.1375

Voice 25KHz 545-548 772.4125 802.4125

Voice 25KHz 609-612 772.8125 802.8125

Voice 25KHz 713-716 773.4625 803.4625

Voice 25KHz 785-788 773.9125 803.9125

Voice 25KHz 833-836 774.2125 804.2125

Voice 25KHz 905-908 774.6625 804.6625

Caldwell Voice 25KHz 89-92 769.5625 799.5625

Voice 25KHz 349-352 771.1875 801.1875 Campus

Voice 25KHz 393-396 771.4625 801.4625

Voice 25KHz 465-468 771.9125 801.9125

Voice 25KHz 489-492 772.0625 802.0625

Voice 25KHz 553-556 772.4625 802.4625

Voice 25KHz 557-560 772.4875 802.4875 Campus

Voice 25KHz 613-616 772.8375 802.8375 Campus

Voice 25KHz 781-784 773.8875 803.8875

Voice 25KHz 909-912 774.6875 804.6875

Voice 25KHz 941-944 774.8875 804.8875 Campus

Callaway Voice 25KHz 17-20 769.1125 799.1125

Voice 25KHz 89-92 769.5625 799.5625

Voice 25KHz 165-168 770.0375 800.0375

Voice 25KHz 209-212 770.3125 800.3125

Voice 25KHz 321-324 771.0125 801.0125

Voice 25KHz 369-372 771.3125 801.3125

Voice 25KHz 457-460 771.8625 801.8625

Voice 25KHz 481-484 772.0125 802.0125

Voice 25KHz 521-524 772.2625 802.2625

Voice 25KHz 565-568 772.5375 802.5375

Voice 25KHz 609-612 772.8125 802.8125

Voice 25KHz 677-680 773.2375 803.2375

Voice 25KHz 753-756 773.7125 803.7125

Voice 25KHz 793-796 773.9625 803.9625

Camden Voice 25KHz 13-16 769.0875 799.0875

Voice 25KHz 177-180 770.1125 800.1125

Voice 25KHz 217-220 770.3625 800.3625

Voice 25KHz 333-336 771.0875 801.0875

Voice 25KHz 389-392 771.4375 801.4375

Voice 25KHz 441-444 771.7625 801.7625

Voice 25KHz 489-492 772.0625 802.0625

Voice 25KHz 549-552 772.4375 802.4375

Voice 25KHz 601-604 772.7625 802.7625

Voice 25KHz 661-664 773.1375 803.1375

Voice 25KHz 821-824 774.1375 804.1375

Voice 25KHz 861-864 774.3875 804.3875

Voice 25KHz 909-912 774.6875 804.6875

Cape

Girardeau Voice 25KHz 81-84 769.5125 799.5125

Voice 25KHz 121-124 769.7625 799.7625

Voice 25KHz 165-168 770.0375 800.0375

Voice 25KHz 205-208 770.2875 800.2875

Voice 25KHz 253-256 770.5875 800.5875

Voice 25KHz 321-324 771.0125 801.0125

Voice 25KHz 369-372 771.3125 801.3125

Voice 25KHz 409-412 771.5625 801.5625

Voice 25KHz 449-452 771.8125 801.8125

Voice 25KHz 489-492 772.0625 802.0625

Voice 25KHz 529-532 772.3125 802.3125

Voice 25KHz 569-572 772.5625 802.5625

Voice 25KHz 621-624 772.8875 802.8875

Voice 25KHz 717-720 773.4875 803.4875

Voice 25KHz 757-760 773.7375 803.7375

Voice 25KHz 821-824 774.1375 804.1375

Voice 25KHz 869-872 774.4375 804.4375

Voice 25KHz 917-920 774.7375 804.7375

Carroll Voice 25KHz 165-168 770.0375 800.0375

Voice 25KHz 213-216 770.3375 800.3375

Voice 25KHz 353-356 771.2125 801.2125

Voice 25KHz 409-412 771.5625 801.5625

Voice 25KHz 521-524 772.2625 802.2625

Voice 25KHz 569-572 772.5625 802.5625

Voice 25KHz 625-628 772.9125 802.9125

Voice 25KHz 713-716 773.4625 803.4625

Voice 25KHz 869-872 774.4375 804.4375

Carter Voice 25KHz 93-96 769.5875 799.5875

Voice 25KHz 369-372 771.3125 801.3125

Voice 25KHz 409-412 771.5625 801.5625

Voice 25KHz 529-532 772.3125 802.3125

Voice 25KHz 629-632 772.9375 802.9375

Voice 25KHz 705-708 773.4125 803.4125

Voice 25KHz 873-876 774.4625 804.4625

Cass Voice 25KHz 137-140 769.8625 799.8625

Voice 25KHz 245-248 770.5375 800.5375

Voice 25KHz 349-352 771.1875 801.1875

Voice 25KHz 389-392 771.4375 801.4375

Voice 25KHz 393-396 771.4625 801.4625 Campus

Voice 25KHz 441-444 771.7625 801.7625

Voice 25KHz 489-492 772.0625 802.0625

Voice 25KHz 553-556 772.4625 802.4625 Campus

Voice 25KHz 565-568 772.5375 802.5375

Voice 25KHz 597-600 772.7375 802.7375 Campus

Voice 25KHz 605-608 772.7875 802.7875

Voice 25KHz 661-664 773.1375 803.1375

Voice 25KHz 861-864 774.3875 804.3875 Campus

Cedar Voice 25KHz 249-252 770.5625 800.5625

Voice 25KHz 293-296 770.8375 800.8375

Voice 25KHz 421-424 771.6375 801.6375

Voice 25KHz 461-464 771.8875 801.8875

Voice 25KHz 625-628 772.9125 802.9125

Voice 25KHz 749-752 773.6875 803.6875

Voice 25KHz 917-920 774.7375 804.7375

Chariton Voice 25KHz 333-336 771.0875 801.0875

Voice 25KHz 377-380 771.3625 801.3625

Voice 25KHz 441-444 771.7625 801.7625

Voice 25KHz 585-588 772.6625 802.6625

Voice 25KHz 661-664 773.1375 803.1375

Voice 25KHz 701-704 773.3875 803.3875

Voice 25KHz 789-792 773.9375 803.9375

Voice 25KHz 905-908 774.6625 804.6625

Christian Voice 25KHz 57-60 769.3625 799.3625

Voice 25KHz 209-212 770.3125 800.3125

Voice 25KHz 345-348 771.1625 801.1625

Voice 25KHz 385-388 771.4125 801.4125

Voice 25KHz 425-428 771.6625 801.6625

Voice 25KHz 493-496 772.0875 802.0875

Voice 25KHz 553-556 772.4625 802.4625

Voice 25KHz 593-596 772.7125 802.7125

Voice 25KHz 673-676 773.2125 803.2125

Voice 25KHz 757-760 773.7375 803.7375

Voice 25KHz 837-840 774.2375 804.2375

Voice 25KHz 877-880 774.4875 804.4875

Clark Voice 25KHz 205-208 770.2875 800.2875

Voice 25KHz 389-392 771.4375 801.4375

Voice 25KHz 441-444 771.7625 801.7625

Voice 25KHz 545-548 772.4125 802.4125

Voice 25KHz 585-588 772.6625 802.6625

Voice 25KHz 665-668 773.1625 803.1625

Voice 25KHz 745-748 773.6625 803.6625

Clay Voice 25KHz 129-132 769.8125 799.8125 Campus

Voice 25KHz 133-136 769.8375 799.8375

Voice 25KHz 241-244 770.5125 800.5125

Voice 25KHz 289-292 770.8125 800.8125

Voice 25KHz 345-348 771.1625 801.1625

Voice 25KHz 405-408 771.5375 801.5375

Voice 25KHz 445-448 771.7875 801.7875

Voice 25KHz 517-520 772.2375 802.2375

Voice 25KHz 561-564 772.5125 802.5125

Voice 25KHz 593-596 772.7125 802.7125 Campus

Voice 25KHz 601-604 772.7625 802.7625

Voice 25KHz 665-668 773.1625 803.1625

Clinton Voice 25KHz 41-44 769.2625 799.2625

Voice 25KHz 81-84 769.5125 799.5125

Voice 25KHz 377-380 771.3625 801.3625

Voice 25KHz 509-512 772.1875 802.1875

Voice 25KHz 585-588 772.6625 802.6625

Voice 25KHz 709-712 773.4375 803.4375

Voice 25KHz 821-824 774.1375 804.1375

Voice 25KHz 901-904 774.6375 804.6375

Cole Voice 25KHz 49-52 769.3125 799.3125

Voice 25KHz 125-128 769.7875 799.7875

Voice 25KHz 201-204 770.2625 800.2625

Voice 25KHz 249-252 770.5625 800.5625

Voice 25KHz 289-292 770.8125 800.8125

Voice 25KHz 361-364 771.2625 801.2625

Voice 25KHz 409-412 771.5625 801.5625

Voice 25KHz 449-452 771.8125 801.8125

Voice 25KHz 493-496 772.0875 802.0875

Voice 25KHz 541-544 772.3875 802.3875

Voice 25KHz 585-588 772.6625 802.6625

Voice 25KHz 637-640 772.9875 802.9875

Voice 25KHz 701-704 773.3875 803.3875

Voice 25KHz 745-748 773.6625 803.6625

Voice 25KHz 825-828 774.1625 804.1625

Voice 25KHz 865-868 774.4125 804.4125

Voice 25KHz 905-908 774.6625 804.6625

Voice 25KHz 945-948 774.9125 804.9125

Cooper Voice 25KHz 205-208 770.2875 800.2875

Voice 25KHz 281-284 770.7625 800.7625

Voice 25KHz 405-408 771.5375 801.5375

Voice 25KHz 445-448 771.7875 801.7875

Voice 25KHz 517-520 772.2375 802.2375

Voice 25KHz 589-592 772.6875 802.6875

Voice 25KHz 673-676 773.2125 803.2125

Voice 25KHz 749-752 773.6875 803.6875

Crawford Voice 25KHz 85-88 769.5375 799.5375

Voice 25KHz 205-208 770.2875 800.2875

Voice 25KHz 297-300 770.8625 800.8625

Voice 25KHz 385-388 771.4125 801.4125

Voice 25KHz 441-444 771.7625 801.7625

Voice 25KHz 497-500 772.1125 802.1125

Voice 25KHz 545-548 772.4125 802.4125

Voice 25KHz 601-604 772.7625 802.7625

Voice 25KHz 821-824 774.1375 804.1375

Voice 25KHz 869-872 774.4375 804.4375

Voice 25KHz 909-912 774.6875 804.6875

Dade Voice 25KHz 13-16 769.0875 799.0875

Voice 25KHz 381-384 771.3875 801.3875

Voice 25KHz 429-432 771.6875 801.6875

Voice 25KHz 489-492 772.0625 802.0625

Voice 25KHz 525-528 772.2875 802.2875 Campus

Voice 25KHz 561-564 772.5125 802.5125

Voice 25KHz 613-616 772.8375 802.8375 Campus

Voice 25KHz 709-712 773.4375 803.4375 Campus

Dallas Voice 25KHz 357-360 771.2375 801.2375

Voice 25KHz 405-408 771.5375 801.5375

Voice 25KHz 465-468 771.9125 801.9125

Voice 25KHz 589-592 772.6875 802.6875

Voice 25KHz 677-680 773.2375 803.2375

Voice 25KHz 753-756 773.7125 803.7125

Voice 25KHz 833-836 774.2125 804.2125

Daviess Voice 25KHz 125-128 769.7875 799.7875

Voice 25KHz 209-212 770.3125 800.3125

Voice 25KHz 285-288 770.7875 800.7875

Voice 25KHz 341-344 771.1375 801.1375

Voice 25KHz 385-388 771.4125 801.4125

Voice 25KHz 449-452 771.8125 801.8125

Voice 25KHz 501-504 772.1375 802.1375

Voice 25KHz 573-576 772.5875 802.5875

Voice 25KHz 617-620 772.8625 802.8625

Voice 25KHz 741-744 773.6375 803.6375

De Kalb Voice 25KHz 13-16 769.0875 799.0875

Voice 25KHz 53-56 769.3375 799.3375

Voice 25KHz 369-372 771.3125 801.3125

Voice 25KHz 421-424 771.6375 801.6375

Voice 25KHz 565-568 772.5375 802.5375

Voice 25KHz 605-608 772.7875 802.7875

Voice 25KHz 757-760 773.7375 803.7375

Voice 25KHz 837-840 774.2375 804.2375

Voice 25KHz 877-880 774.4875 804.4875

Dent Voice 25KHz 121-124 769.7625 799.7625

Voice 25KHz 289-292 770.8125 800.8125

Voice 25KHz 337-340 771.1125 801.1125

Voice 25KHz 341-344 771.1375 801.1375 Campus

Voice 25KHz 401-404 771.5125 801.5125

Voice 25KHz 465-468 771.9125 801.9125

Voice 25KHz 481-484 772.0125 802.0125 Campus

Voice 25KHz 525-528 772.2875 802.2875 Campus

Voice 25KHz 573-576 772.5875 802.5875 Campus

Voice 25KHz 581-584 772.6375 802.6375

Voice 25KHz 677-680 773.2375 803.2375

Voice 25KHz 749-752 773.6875 803.6875 Campus

Voice 25KHz 753-756 773.7125 803.7125 Campus

Voice 25KHz 825-828 774.1625 804.1625 Campus

Voice 25KHz 833-836 774.2125 804.2125

Voice 25KHz 913-916 774.7125 804.7125 Campus

Voice 25KHz 945-948 774.9125 804.9125

Douglas Voice 25KHz 45-48 769.2875 799.2875

Voice 25KHz 353-356 771.2125 801.2125

Voice 25KHz 409-412 771.5625 801.5625

Voice 25KHz 469-472 771.9375 801.9375

Voice 25KHz 525-528 772.2875 802.2875

Voice 25KHz 629-632 772.9375 802.9375

Voice 25KHz 829-832 774.1875 804.1875

Dunklin Voice 25KHz 173-176 770.0875 800.0875

Voice 25KHz 365-368 771.2875 801.2875

Voice 25KHz 405-408 771.5375 801.5375

Voice 25KHz 513-516 772.2125 802.2125

Voice 25KHz 553-556 772.4625 802.4625

Voice 25KHz 593-596 772.7125 802.7125

Voice 25KHz 741-744 773.6375 803.6375

Voice 25KHz 797-800 773.9875 803.9875

Voice 25KHz 865-868 774.4125 804.4125

Voice 25KHz 913-916 774.7125 804.7125

Franklin Voice 25KHz 129-132 769.8125 799.8125

Voice 25KHz 349-352 771.1875 801.1875

Voice 25KHz 397-400 771.4875 801.4875

Voice 25KHz 461-464 771.8875 801.8875

Voice 25KHz 529-532 772.3125 802.3125

Voice 25KHz 577-580 772.6125 802.6125

Voice 25KHz 621-624 772.8875 802.8875

Voice 25KHz 669-672 773.1875 803.1875

Voice 25KHz 837-840 774.2375 804.2375

Gasconade Voice 25KHz 285-288 770.7875 800.7875

Voice 25KHz 357-360 771.2375 801.2375

Voice 25KHz 405-408 771.5375 801.5375

Voice 25KHz 469-472 771.9375 801.9375

Voice 25KHz 589-592 772.6875 802.6875

Voice 25KHz 717-720 773.4875 803.4875

Voice 25KHz 941-944 774.8875 804.8875

Gentry Voice 25KHz 165-168 770.0375 800.0375

Voice 25KHz 329-332 771.0625 801.0625

Voice 25KHz 477-480 771.9875 801.9875

Voice 25KHz 493-496 772.0875 802.0875

Voice 25KHz 561-564 772.5125 802.5125 Campus

Voice 25KHz 581-584 772.6375 802.6375

Voice 25KHz 829-832 774.1875 804.1875

Voice 25KHz 905-908 774.6625 804.6625

Greene Voice 25KHz 41-44 769.2625 799.2625

Voice 25KHz 81-84 769.5125 799.5125

Voice 25KHz 121-124 769.7625 799.7625

Voice 25KHz 161-164 770.0125 800.0125

Voice 25KHz 201-204 770.2625 800.2625

Voice 25KHz 241-244 770.5125 800.5125

Voice 25KHz 281-284 770.7625 800.7625

Voice 25KHz 325-328 771.0375 801.0375

Voice 25KHz 365-368 771.2875 801.2875

Voice 25KHz 413-416 771.5875 801.5875

Voice 25KHz 477-480 771.9875 801.9875

Voice 25KHz 501-504 772.1375 802.1375

Voice 25KHz 541-544 772.3875 802.3875

Voice 25KHz 581-584 772.6375 802.6375

Voice 25KHz 633-636 772.9625 802.9625

Voice 25KHz 705-708 773.4125 803.4125

Voice 25KHz 745-748 773.6625 803.6625

Voice 25KHz 785-788 773.9125 803.9125

Voice 25KHz 825-828 774.1625 804.1625

Voice 25KHz 865-868 774.4125 804.4125

Voice 25KHz 905-908 774.6625 804.6625

Voice 25KHz 945-948 774.9125 804.9125

Grundy Voice 25KHz 85-88 769.5375 799.5375

Voice 25KHz 161-164 770.0125 800.0125

Voice 25KHz 217-220 770.3625 800.3625

Voice 25KHz 357-360 771.2375 801.2375

Voice 25KHz 413-416 771.5875 801.5875

Voice 25KHz 525-528 772.2875 802.2875

Voice 25KHz 589-592 772.6875 802.6875

Voice 25KHz 629-632 772.9375 802.9375

Voice 25KHz 669-672 773.1875 803.1875

Voice 25KHz 797-800 773.9875 803.9875

Harrison Voice 25KHz 57-60 769.3625 799.3625

Voice 25KHz 133-136 769.8375 799.8375

Voice 25KHz 241-244 770.5125 800.5125

Voice 25KHz 321-324 771.0125 801.0125

Voice 25KHz 365-368 771.2875 801.2875

Voice 25KHz 425-428 771.6625 801.6625

Voice 25KHz 517-520 772.2375 802.2375

Voice 25KHz 637-640 772.9875 802.9875

Voice 25KHz 717-720 773.4875 803.4875

Voice 25KHz 873-876 774.4625 804.4625

Henry Voice 25KHz 41-44 769.2625 799.2625

Voice 25KHz 321-324 771.0125 801.0125

Voice 25KHz 365-368 771.2875 801.2875

Voice 25KHz 457-460 771.8625 801.8625

Voice 25KHz 529-532 772.3125 802.3125

Voice 25KHz 585-588 772.6625 802.6625

Voice 25KHz 637-640 772.9875 802.9875

Voice 25KHz 701-704 773.3875 803.3875

Voice 25KHz 829-832 774.1875 804.1875

Voice 25KHz 941-944 774.8875 804.8875

Hickory Voice 25KHz 137-140 769.8625 799.8625

Voice 25KHz 205-208 770.2875 800.2875

Voice 25KHz 505-508 772.1625 802.1625

Voice 25KHz 557-560 772.4875 802.4875

Voice 25KHz 617-620 772.8625 802.8625

Holt Voice 25KHz 297-300 770.8625 800.8625

Voice 25KHz 405-408 771.5375 801.5375

Voice 25KHz 469-472 771.9375 801.9375

Voice 25KHz 517-520 772.2375 802.2375

Voice 25KHz 573-576 772.5875 802.5875

Voice 25KHz 629-632 772.9375 802.9375

Howard Voice 25KHz 129-132 769.8125 799.8125

Voice 25KHz 169-172 770.0625 800.0625

Voice 25KHz 365-368 771.2875 801.2875

Voice 25KHz 485-488 772.0375 802.0375

Voice 25KHz 525-528 772.2875 802.2875

Voice 25KHz 573-576 772.5875 802.5875

Voice 25KHz 757-760 773.7375 803.7375

Howell Voice 25KHz 53-56 769.3375 799.3375

Voice 25KHz 97-100 769.6125 799.6125

Voice 25KHz 169-172 770.0625 800.0625

Voice 25KHz 217-220 770.3625 800.3625

Voice 25KHz 285-288 770.7875 800.7875

Voice 25KHz 333-336 771.0875 801.0875

Voice 25KHz 381-384 771.3875 801.3875

Voice 25KHz 457-460 771.8625 801.8625

Voice 25KHz 505-508 772.1625 802.1625

Voice 25KHz 545-548 772.4125 802.4125

Voice 25KHz 589-592 772.6875 802.6875

Voice 25KHz 661-664 773.1375 803.1375

Voice 25KHz 717-720 773.4875 803.4875

Voice 25KHz 785-788 773.9125 803.9125

Voice 25KHz 905-908 774.6625 804.6625

Iron Voice 25KHz 217-220 770.3625 800.3625

Voice 25KHz 353-356 771.2125 801.2125

Voice 25KHz 417-420 771.6125 801.6125

Voice 25KHz 553-556 772.4625 802.4625

Voice 25KHz 557-560 772.4875 802.4875 Campus

Voice 25KHz 625-628 772.9125 802.9125 Campus

Voice 25KHz 633-636 772.9625 802.9625

Voice 25KHz 789-792 773.9375 803.9375

Voice 25KHz 877-880 774.4875 804.4875 Campus

Voice 25KHz 905-908 774.6625 804.6625 Campus

Voice 25KHz 917-920 774.7375 804.7375 Campus

Jackson Voice 25KHz 45-48 769.2875 799.2875

Voice 25KHz 85-88 769.5375 799.5375

Voice 25KHz 125-128 769.7875 799.7875

Voice 25KHz 177-180 770.1125 800.1125

Voice 25KHz 217-220 770.3625 800.3625

Voice 25KHz 257-260 770.6125 800.6125

Voice 25KHz 297-300 770.8625 800.8625

Voice 25KHz 337-340 771.1125 801.1125

Voice 25KHz 381-384 771.3875 801.3875

Voice 25KHz 429-432 771.6875 801.6875

Voice 25KHz 469-472 771.9375 801.9375

Voice 12.5KHz 501-502 772.1313 802.1313

Voice 12.5KHz 503-504 772.1438 802.1438

Voice 25KHz 549-552 772.4375 802.4375

Voice 12.5KHz 589-590 772.6813 802.6813

Voice 12.5KHz 591-592 772.6938 802.6938

Voice 25KHz 629-632 772.9375 802.9375

Voice 12.5KHz 705-706 773.4063 803.4063

Voice 12.5KHz 707-708 773.4188 803.4188

Voice 25KHz 745-748 773.6625 803.6625

Voice 25KHz 785-788 773.9125 803.9125

Voice 12.5KHz 825-826 774.1563 804.1563

Voice 12.5KHz 827-828 774.1688 804.1688

Voice 25KHz 865-868 774.4125 804.4125

Voice 25KHz 905-908 774.6625 804.6625

Voice 12.5KHz 945-946 774.9063 804.9063

Voice 12.5KHz 947-948 774.9188 804.9188

Jasper Voice 25KHz 45-48 769.2875 799.2875

Voice 25KHz 89-92 769.5625 799.5625

Voice 25KHz 137-140 769.8625 799.8625

Voice 25KHz 177-180 770.1125 800.1125

Voice 25KHz 217-220 770.3625 800.3625

Voice 25KHz 297-300 770.8625 800.8625

Voice 25KHz 341-344 771.1375 801.1375

Voice 25KHz 405-408 771.5375 801.5375

Voice 25KHz 469-472 771.9375 801.9375

Voice 25KHz 505-508 772.1625 802.1625

Voice 25KHz 545-548 772.4125 802.4125

Voice 25KHz 585-588 772.6625 802.6625

Voice 25KHz 629-632 772.9375 802.9375

Voice 25KHz 677-680 773.2375 803.2375

Voice 25KHz 741-744 773.6375 803.6375

Voice 25KHz 781-784 773.8875 803.8875

Voice 25KHz 833-836 774.2125 804.2125

Voice 25KHz 873-876 774.4625 804.4625

Voice 25KHz 913-916 774.7125 804.7125

Jefferson Voice 25KHz 137-140 769.8625 799.8625

Voice 25KHz 341-344 771.1375 801.1375

Voice 25KHz 389-392 771.4375 801.4375

Voice 25KHz 437-440 771.7375 801.7375

Voice 25KHz 501-504 772.1375 802.1375

Voice 25KHz 549-552 772.4375 802.4375

Voice 25KHz 593-596 772.7125 802.7125

Voice 25KHz 637-640 772.9875 802.9875

Voice 25KHz 709-712 773.4375 803.4375

Voice 25KHz 825-828 774.1625 804.1625

Voice 25KHz 873-876 774.4625 804.4625

Voice 25KHz 913-916 774.7125 804.7125

Johnson Voice 25KHz 161-164 770.0125 800.0125

Voice 25KHz 209-212 770.3125 800.3125

Voice 25KHz 285-288 770.7875 800.7875

Voice 25KHz 357-360 771.2375 801.2375

Voice 25KHz 401-404 771.5125 801.5125

Voice 25KHz 449-452 771.8125 801.8125

Voice 25KHz 513-516 772.2125 802.2125

Voice 25KHz 577-580 772.6125 802.6125

Voice 25KHz 669-672 773.1875 803.1875

Voice 25KHz 753-756 773.7125 803.7125

Voice 25KHz 793-796 773.9625 803.9625

Voice 25KHz 873-876 774.4625 804.4625

Knox Voice 25KHz 361-364 771.2625 801.2625

Voice 25KHz 417-420 771.6125 801.6125

Voice 25KHz 465-468 771.9125 801.9125

Voice 25KHz 485-488 772.0375 802.0375

Voice 25KHz 673-676 773.2125 803.2125

Laclede Voice 25KHz 89-92 769.5625 799.5625

Voice 25KHz 165-168 770.0375 800.0375

Voice 25KHz 293-296 770.8375 800.8375

Voice 25KHz 429-432 771.6875 801.6875

Voice 25KHz 481-484 772.0125 802.0125

Voice 25KHz 529-532 772.3125 802.3125

Voice 25KHz 577-580 772.6125 802.6125

Voice 25KHz 625-628 772.9125 802.9125

Voice 25KHz 741-744 773.6375 803.6375

Voice 25KHz 789-792 773.9375 803.9375

Voice 25KHz 901-904 774.6375 804.6375

Voice 25KHz 941-944 774.8875 804.8875

Lafayette Voice 25KHz 13-16 769.0875 799.0875 Campus

Voice 25KHz 53-56 769.3375 799.3375 Campus

Voice 25KHz 93-96 769.5875 799.5875

Voice 25KHz 121-124 769.7625 799.7625 Campus

Voice 25KHz 201-204 770.2625 800.2625

Voice 25KHz 373-376 771.3375 801.3375

Voice 25KHz 421-424 771.6375 801.6375

Voice 25KHz 461-464 771.8875 801.8875

Voice 25KHz 537-540 772.3625 802.3625

Voice 25KHz 581-584 772.6375 802.6375 Campus

Voice 25KHz 617-620 772.8625 802.8625

Voice 25KHz 913-916 774.7125 804.7125

Lawrence Voice 25KHz 97-100 769.6125 799.6125

Voice 25KHz 253-256 770.5875 800.5875

Voice 25KHz 393-396 771.4625 801.4625

Voice 25KHz 441-444 771.7625 801.7625

Voice 25KHz 529-532 772.3125 802.3125

Voice 25KHz 573-576 772.5875 802.5875

Voice 25KHz 613-616 772.8375 802.8375

Voice 25KHz 661-664 773.1375 803.1375

Voice 25KHz 717-720 773.4875 803.4875

Lewis Voice 25KHz 97-100 769.6125 799.6125

Voice 25KHz 381-384 771.3875 801.3875

Voice 25KHz 509-512 772.1875 802.1875

Voice 25KHz 565-568 772.5375 802.5375

Voice 25KHz 609-612 772.8125 802.8125

Voice 25KHz 821-824 774.1375 804.1375

Voice 25KHz 873-876 774.4625 804.4625

Voice 25KHz 917-920 774.7375 804.7375

Lincoln Voice 25KHz 57-60 769.3625 799.3625

Voice 25KHz 253-256 770.5875 800.5875

Voice 25KHz 293-296 770.8375 800.8375

Voice 25KHz 401-404 771.5125 801.5125

Voice 25KHz 473-476 771.9625 801.9625

Voice 25KHz 485-488 772.0375 802.0375

Voice 25KHz 561-564 772.5125 802.5125

Voice 25KHz 605-608 772.7875 802.7875

Voice 25KHz 673-676 773.2125 803.2125

Voice 25KHz 785-788 773.9125 803.9125

Voice 25KHz 869-872 774.4375 804.4375

Voice 25KHz 909-912 774.6875 804.6875

Linn Voice 25KHz 45-48 769.2875 799.2875

Voice 25KHz 205-208 770.2875 800.2875

Voice 25KHz 249-252 770.5625 800.5625

Voice 25KHz 289-292 770.8125 800.8125

Voice 25KHz 345-348 771.1625 801.1625

Voice 25KHz 457-460 771.8625 801.8625

Voice 25KHz 509-512 772.1875 802.1875

Voice 25KHz 561-564 772.5125 802.5125

Voice 25KHz 605-608 772.7875 802.7875

Voice 25KHz 745-748 773.6625 803.6625

Voice 25KHz 945-948 774.9125 804.9125

Livingston Voice 25KHz 97-100 769.6125 799.6125

Voice 25KHz 173-176 770.0875 800.0875

Voice 25KHz 257-260 770.6125 800.6125

Voice 25KHz 297-300 770.8625 800.8625

Voice 25KHz 401-404 771.5125 801.5125

Voice 25KHz 481-484 772.0125 802.0125

Voice 25KHz 541-544 772.3875 802.3875

Voice 25KHz 597-600 772.7375 802.7375

Voice 25KHz 677-680 773.2375 803.2375

Voice 25KHz 753-756 773.7125 803.7125

Voice 25KHz 917-920 774.7375 804.7375

Macon Voice 25KHz 93-96 769.5875 799.5875

Voice 25KHz 133-136 769.8375 799.8375

Voice 25KHz 241-244 770.5125 800.5125

Voice 25KHz 321-324 771.0125 801.0125

Voice 25KHz 369-372 771.3125 801.3125

Voice 25KHz 429-432 771.6875 801.6875

Voice 25KHz 529-532 772.3125 802.3125

Voice 25KHz 593-596 772.7125 802.7125

Voice 25KHz 637-640 772.9875 802.9875

Voice 25KHz 717-720 773.4875 803.4875

Voice 25KHz 825-828 774.1625 804.1625

Voice 25KHz 877-880 774.4875 804.4875

Madison Voice 25KHz 169-172 770.0625 800.0625

Voice 25KHz 281-284 770.7625 800.7625

Voice 25KHz 393-396 771.4625 801.4625

Voice 25KHz 505-508 772.1625 802.1625

Voice 25KHz 573-576 772.5875 802.5875

Voice 25KHz 617-620 772.8625 802.8625

Voice 25KHz 865-868 774.4125 804.4125

Maries Voice 25KHz 169-172 770.0625 800.0625

Voice 25KHz 241-244 770.5125 800.5125

Voice 25KHz 345-348 771.1625 801.1625

Voice 25KHz 473-476 771.9625 801.9625 Campus

Voice 25KHz 485-488 772.0375 802.0375

Voice 25KHz 513-516 772.2125 802.2125 Campus

Voice 25KHz 533-536 772.3375 802.3375

Voice 25KHz 617-620 772.8625 802.8625 Campus

Voice 25KHz 829-832 774.1875 804.1875 Campus

Marion Voice 25KHz 45-48 769.2875 799.2875

Voice 25KHz 201-204 770.2625 800.2625

Voice 25KHz 249-252 770.5625 800.5625

Voice 25KHz 289-292 770.8125 800.8125

Voice 25KHz 345-348 771.1625 801.1625

Voice 25KHz 393-396 771.4625 801.4625

Voice 25KHz 445-448 771.7875 801.7875

Voice 25KHz 517-520 772.2375 802.2375

Voice 25KHz 581-584 772.6375 802.6375

Voice 25KHz 629-632 772.9375 802.9375

Voice 25KHz 701-704 773.3875 803.3875

Voice 25KHz 749-752 773.6875 803.6875

Voice 25KHz 789-792 773.9375 803.9375

Voice 25KHz 905-908 774.6625 804.6625

McDonald Voice 25KHz 249-252 770.5625 800.5625

Voice 25KHz 397-400 771.4875 801.4875

Voice 25KHz 465-468 771.9125 801.9125

Voice 25KHz 517-520 772.2375 802.2375

Voice 25KHz 565-568 772.5375 802.5375

Voice 25KHz 829-832 774.1875 804.1875

Mercer Voice 25KHz 201-204 770.2625 800.2625

Voice 25KHz 405-408 771.5375 801.5375

Voice 25KHz 497-500 772.1125 802.1125

Voice 25KHz 621-624 772.8875 802.8875

Voice 25KHz 749-752 773.6875 803.6875

Voice 25KHz 865-868 774.4125 804.4125

Miller Voice 25KHz 97-100 769.6125 799.6125

Voice 25KHz 325-328 771.0375 801.0375

Voice 25KHz 373-376 771.3375 801.3375

Voice 25KHz 421-424 771.6375 801.6375

Voice 25KHz 461-464 771.8875 801.8875

Voice 25KHz 525-528 772.2875 802.2875

Voice 25KHz 573-576 772.5875 802.5875

Voice 25KHz 621-624 772.8875 802.8875

Voice 25KHz 797-800 773.9875 803.9875

Mississippi Voice 25KHz 169-172 770.0625 800.0625

Voice 25KHz 345-348 771.1625 801.1625

Voice 25KHz 465-468 771.9125 801.9125

Voice 25KHz 533-536 772.3375 802.3375

Voice 25KHz 625-628 772.9125 802.9125

Voice 25KHz 793-796 773.9625 803.9625

Moniteau Voice 25KHz 337-340 771.1125 801.1125

Voice 25KHz 429-432 771.6875 801.6875

Voice 25KHz 469-472 771.9375 801.9375

Voice 25KHz 509-512 772.1875 802.1875

Voice 25KHz 561-564 772.5125 802.5125

Voice 25KHz 613-616 772.8375 802.8375

Monroe Voice 25KHz 85-88 769.5375 799.5375

Voice 25KHz 213-216 770.3375 800.3375

Voice 25KHz 409-412 771.5625 801.5625

Voice 25KHz 505-508 772.1625 802.1625

Voice 25KHz 569-572 772.5625 802.5625

Voice 25KHz 669-672 773.1875 803.1875

Voice 25KHz 781-784 773.8875 803.8875

Voice 25KHz 865-868 774.4125 804.4125

Montgomery Voice 25KHz 341-344 771.1375 801.1375

Voice 25KHz 413-416 771.5875 801.5875

Voice 25KHz 633-636 772.9625 802.9625

Voice 25KHz 741-744 773.6375 803.6375

Voice 25KHz 861-864 774.3875 804.3875

Voice 25KHz 917-920 774.7375 804.7375

Morgan Voice 25KHz 45-48 769.2875 799.2875

Voice 25KHz 121-124 769.7625 799.7625

Voice 25KHz 353-356 771.2125 801.2125

Voice 25KHz 453-456 771.8375 801.8375

Voice 25KHz 581-584 772.6375 802.6375

Voice 25KHz 629-632 772.9375 802.9375

Voice 25KHz 717-720 773.4875 803.4875

Voice 25KHz 869-872 774.4375 804.4375

Voice 25KHz 917-920 774.7375 804.7375

New Madrid Voice 25KHz 209-212 770.3125 800.3125

Voice 25KHz 325-328 771.0375 801.0375

Voice 25KHz 377-380 771.3625 801.3625

Voice 25KHz 441-444 771.7625 801.7625

Voice 25KHz 541-544 772.3875 802.3875

Voice 25KHz 581-584 772.6375 802.6375

Voice 25KHz 633-636 772.9625 802.9625

Voice 25KHz 701-704 773.3875 803.3875

Newton Voice 25KHz 17-20 769.1125 799.1125

Voice 25KHz 129-132 769.8125 799.8125

Voice 25KHz 205-208 770.2875 800.2875

Voice 25KHz 333-336 771.0875 801.0875

Voice 25KHz 377-380 771.3625 801.3625

Voice 25KHz 433-436 771.7125 801.7125

Voice 25KHz 497-500 772.1125 802.1125

Voice 25KHz 557-560 772.4875 802.4875

Voice 25KHz 597-600 772.7375 802.7375

Voice 25KHz 637-640 772.9875 802.9875

Voice 25KHz 753-756 773.7125 803.7125

Voice 25KHz 797-800 773.9875 803.9875

Voice 25KHz 861-864 774.3875 804.3875

Nodaway Voice 25KHz 45-48 769.2875 799.2875

Voice 25KHz 85-88 769.5375 799.5375

Voice 25KHz 137-140 769.8625 799.8625

Voice 25KHz 205-208 770.2875 800.2875

Voice 25KHz 249-252 770.5625 800.5625

Voice 25KHz 361-364 771.2625 801.2625

Voice 25KHz 413-416 771.5875 801.5875

Voice 25KHz 461-464 771.8875 801.8875

Voice 25KHz 481-484 772.0125 802.0125

Voice 25KHz 529-532 772.3125 802.3125

Voice 25KHz 621-624 772.8875 802.8875

Voice 25KHz 661-664 773.1375 803.1375

Voice 25KHz 701-704 773.3875 803.3875

Voice 25KHz 745-748 773.6625 803.6625

Voice 25KHz 785-788 773.9125 803.9125

Voice 25KHz 869-872 774.4375 804.4375

Voice 25KHz 917-920 774.7375 804.7375

Oregon Voice 25KHz 41-44 769.2625 799.2625

Voice 25KHz 161-164 770.0125 800.0125

Voice 25KHz 325-328 771.0375 801.0375

Voice 25KHz 401-404 771.5125 801.5125

Voice 25KHz 441-444 771.7625 801.7625

Voice 25KHz 557-560 772.4875 802.4875

Voice 25KHz 741-744 773.6375 803.6375

Voice 25KHz 861-864 774.3875 804.3875

Osage Voice 25KHz 133-136 769.8375 799.8375

Voice 25KHz 381-384 771.3875 801.3875

Voice 25KHz 553-556 772.4625 802.4625

Voice 25KHz 597-600 772.7375 802.7375

Voice 25KHz 709-712 773.4375 803.4375

Voice 25KHz 781-784 773.8875 803.8875

Ozark Voice 25KHz 89-92 769.5625 799.5625

Voice 25KHz 369-372 771.3125 801.3125

Voice 25KHz 417-420 771.6125 801.6125

Voice 25KHz 561-564 772.5125 802.5125

Voice 25KHz 609-612 772.8125 802.8125

Pemiscot Voice 25KHz 57-60 769.3625 799.3625

Voice 25KHz 217-220 770.3625 800.3625

Voice 25KHz 393-396 771.4625 801.4625

Voice 25KHz 433-436 771.7125 801.7125

Voice 25KHz 529-532 772.3125 802.3125

Voice 25KHz 573-576 772.5875 802.5875

Voice 25KHz 757-760 773.7375 803.7375

Perry Voice 25KHz 345-348 771.1625 801.1625

Voice 25KHz 441-444 771.7625 801.7625

Voice 25KHz 597-600 772.7375 802.7375

Voice 25KHz 705-708 773.4125 803.4125

Voice 25KHz 793-796 773.9625 803.9625

Voice 25KHz 945-948 774.9125 804.9125

Pettis Voice 25KHz 17-20 769.1125 799.1125

Voice 25KHz 57-60 769.3625 799.3625

Voice 25KHz 133-136 769.8375 799.8375

Voice 25KHz 173-176 770.0875 800.0875

Voice 25KHz 241-244 770.5125 800.5125

Voice 25KHz 329-332 771.0625 801.0625

Voice 25KHz 413-416 771.5875 801.5875

Voice 25KHz 481-484 772.0125 802.0125

Voice 25KHz 553-556 772.4625 802.4625

Voice 25KHz 597-600 772.7375 802.7375

Voice 25KHz 709-712 773.4375 803.4375

Voice 25KHz 781-784 773.8875 803.8875

Voice 25KHz 837-840 774.2375 804.2375

Voice 25KHz 901-904 774.6375 804.6375

Phelps Voice 25KHz 41-44 769.2625 799.2625

Voice 25KHz 93-96 769.5875 799.5875

Voice 25KHz 161-164 770.0125 800.0125

Voice 25KHz 213-216 770.3375 800.3375

Voice 25KHz 253-256 770.5875 800.5875

Voice 25KHz 329-332 771.0625 801.0625

Voice 25KHz 377-380 771.3625 801.3625

Voice 25KHz 433-436 771.7125 801.7125

Voice 25KHz 509-512 772.1875 802.1875

Voice 25KHz 565-568 772.5375 802.5375

Voice 25KHz 609-612 772.8125 802.8125

Voice 25KHz 665-668 773.1625 803.1625

Voice 25KHz 705-708 773.4125 803.4125

Voice 25KHz 793-796 773.9625 803.9625

Pike Voice 25KHz 49-52 769.3125 799.3125

Voice 25KHz 173-176 770.0875 800.0875

Voice 25KHz 373-376 771.3375 801.3375

Voice 25KHz 441-444 771.7625 801.7625

Voice 25KHz 497-500 772.1125 802.1125

Voice 25KHz 545-548 772.4125 802.4125

Voice 25KHz 585-588 772.6625 802.6625

Voice 25KHz 665-668 773.1625 803.1625

Platte Voice 25KHz 17-20 769.1125 799.1125

Voice 25KHz 57-60 769.3625 799.3625

Voice 25KHz 169-172 770.0625 800.0625

Voice 25KHz 325-328 771.0375 801.0375

Voice 25KHz 365-368 771.2875 801.2875

Voice 25KHz 417-420 771.6125 801.6125

Voice 25KHz 457-460 771.8625 801.8625

Voice 25KHz 485-488 772.0375 802.0375

Voice 25KHz 525-528 772.2875 802.2875

Voice 25KHz 569-572 772.5625 802.5625

Voice 25KHz 609-612 772.8125 802.8125

Voice 25KHz 677-680 773.2375 803.2375

Voice 25KHz 717-720 773.4875 803.4875

Polk Voice 25KHz 53-56 769.3375 799.3375

Voice 25KHz 93-96 769.5875 799.5875

Voice 25KHz 213-216 770.3375 800.3375

Voice 25KHz 349-352 771.1875 801.1875

Voice 25KHz 397-400 771.4875 801.4875

Voice 25KHz 445-448 771.7875 801.7875

Voice 25KHz 533-536 772.3375 802.3375

Voice 25KHz 597-600 772.7375 802.7375

Voice 25KHz 665-668 773.1625 803.1625

Voice 25KHz 713-716 773.4625 803.4625

Pulaski Voice 25KHz 57-60 769.3625 799.3625

Voice 25KHz 137-140 769.8625 799.8625

Voice 25KHz 281-284 770.7625 800.7625

Voice 25KHz 365-368 771.2875 801.2875

Voice 25KHz 413-416 771.5875 801.5875

Voice 25KHz 477-480 771.9875 801.9875

Voice 25KHz 501-504 772.1375 802.1375

Voice 25KHz 593-596 772.7125 802.7125

Voice 25KHz 633-636 772.9625 802.9625

Voice 25KHz 673-676 773.2125 803.2125

Voice 25KHz 713-716 773.4625 803.4625

Voice 25KHz 757-760 773.7375 803.7375

Voice 25KHz 837-840 774.2375 804.2375

Voice 25KHz 877-880 774.4875 804.4875

Putnam Voice 25KHz 165-168 770.0375 800.0375

Voice 25KHz 353-356 771.2125 801.2125

Voice 25KHz 397-400 771.4875 801.4875

Voice 25KHz 461-464 771.8875 801.8875

Voice 25KHz 565-568 772.5375 802.5375

Voice 25KHz 609-612 772.8125 802.8125

Voice 25KHz 821-824 774.1375 804.1375

Ralls Voice 25KHz 281-284 770.7625 800.7625

Voice 25KHz 337-340 771.1125 801.1125

Voice 25KHz 385-388 771.4125 801.4125

Voice 25KHz 489-492 772.0625 802.0625

Voice 25KHz 553-556 772.4625 802.4625

Voice 25KHz 757-760 773.7375 803.7375

Randolph Voice 25KHz 13-16 769.0875 799.0875

Voice 25KHz 53-56 769.3375 799.3375

Voice 25KHz 121-124 769.7625 799.7625

Voice 25KHz 161-164 770.0125 800.0125

Voice 25KHz 285-288 770.7875 800.7875

Voice 25KHz 357-360 771.2375 801.2375

Voice 25KHz 397-400 771.4875 801.4875

Voice 25KHz 453-456 771.8375 801.8375

Voice 25KHz 557-560 772.4875 802.4875

Voice 25KHz 601-604 772.7625 802.7625

Voice 25KHz 797-800 773.9875 803.9875

Voice 25KHz 941-944 774.8875 804.8875

Ray Voice 25KHz 321-324 771.0125 801.0125

Voice 25KHz 361-364 771.2625 801.2625

Voice 25KHz 453-456 771.8375 801.8375

Voice 25KHz 505-508 772.1625 802.1625 Campus

Voice 25KHz 529-532 772.3125 802.3125

Voice 25KHz 637-640 772.9875 802.9875

Voice 25KHz 833-836 774.2125 804.2125

Reynolds Voice 25KHz 13-16 769.0875 799.0875

Voice 25KHz 57-60 769.3625 799.3625

Voice 25KHz 165-168 770.0375 800.0375

Voice 25KHz 449-452 771.8125 801.8125

Voice 25KHz 521-524 772.2625 802.2625

Voice 25KHz 569-572 772.5625 802.5625

Voice 25KHz 613-616 772.8375 802.8375

Voice 25KHz 781-784 773.8875 803.8875

Ripley Voice 25KHz 293-296 770.8375 800.8375

Voice 25KHz 361-364 771.2625 801.2625

Voice 25KHz 433-436 771.7125 801.7125

Voice 25KHz 473-476 771.9625 801.9625

Voice 25KHz 509-512 772.1875 802.1875

Voice 25KHz 573-576 772.5875 802.5875

Voice 25KHz 621-624 772.8875 802.8875

Voice 25KHz 757-760 773.7375 803.7375

Voice 25KHz 825-828 774.1625 804.1625

Saline Voice 25KHz 49-52 769.3125 799.3125

Voice 25KHz 253-256 770.5875 800.5875

Voice 25KHz 293-296 770.8375 800.8375

Voice 25KHz 385-388 771.4125 801.4125

Voice 25KHz 433-436 771.7125 801.7125

Voice 25KHz 473-476 771.9625 801.9625

Voice 25KHz 493-496 772.0875 802.0875

Voice 25KHz 545-548 772.4125 802.4125

Voice 25KHz 633-636 772.9625 802.9625

Voice 25KHz 741-744 773.6375 803.6375

Voice 25KHz 861-864 774.3875 804.3875

Schuyler Voice 25KHz 293-296 770.8375 800.8375

Voice 25KHz 377-380 771.3625 801.3625

Voice 25KHz 445-448 771.7875 801.7875

Voice 25KHz 541-544 772.3875 802.3875

Voice 25KHz 781-784 773.8875 803.8875

Scotland Voice 25KHz 49-52 769.3125 799.3125

Voice 25KHz 453-456 771.8375 801.8375

Voice 25KHz 525-528 772.2875 802.2875

Voice 25KHz 601-604 772.7625 802.7625

Voice 25KHz 753-756 773.7125 803.7125

Voice 25KHz 829-832 774.1875 804.1875

Voice 25KHz 941-944 774.8875 804.8875

Scott Voice 25KHz 13-16 769.0875 799.0875

Voice 25KHz 53-56 769.3375 799.3375

Voice 25KHz 129-132 769.8125 799.8125

Voice 25KHz 245-248 770.5375 800.5375

Voice 25KHz 285-288 770.7875 800.7875

Voice 25KHz 333-336 771.0875 801.0875

Voice 25KHz 421-424 771.6375 801.6375

Voice 25KHz 509-512 772.1875 802.1875

Voice 25KHz 549-552 772.4375 802.4375

Voice 25KHz 665-668 773.1625 803.1625

Voice 25KHz 781-784 773.8875 803.8875

Voice 25KHz 861-864 774.3875 804.3875

Voice 25KHz 909-912 774.6875 804.6875

Shannon Voice 25KHz 209-212 770.3125 800.3125

Voice 25KHz 357-360 771.2375 801.2375

Voice 25KHz 421-424 771.6375 801.6375

Voice 25KHz 489-492 772.0625 802.0625

Voice 25KHz 537-540 772.3625 802.3625

Voice 25KHz 597-600 772.7375 802.7375

Voice 25KHz 637-640 772.9875 802.9875

Shelby Voice 25KHz 473-476 771.9625 801.9625

Voice 25KHz 493-496 772.0875 802.0875

Voice 25KHz 537-540 772.3625 802.3625

Voice 25KHz 573-576 772.5875 802.5875 Campus

Voice 25KHz 621-624 772.8875 802.8875

Voice 25KHz 741-744 773.6375 803.6375

Voice 25KHz 837-840 774.2375 804.2375

Voice 25KHz 869-872 774.4375 804.4375 Campus

St. Charles Voice 25KHz 45-48 769.2875 799.2875

Voice 25KHz 121-124 769.7625 799.7625

Voice 25KHz 161-164 770.0125 800.0125

Voice 25KHz 165-168 770.0375 800.0375 Campus

Voice 25KHz 241-244 770.5125 800.5125

Voice 25KHz 281-284 770.7625 800.7625

Voice 25KHz 337-340 771.1125 801.1125

Voice 25KHz 377-380 771.3625 801.3625

Voice 25KHz 381-384 771.3875 801.3875 Campus

Voice 25KHz 417-420 771.6125 801.6125

Voice 25KHz 505-508 772.1625 802.1625

Voice 25KHz 521-524 772.2625 802.2625 Campus

Voice 25KHz 557-560 772.4875 802.4875 Campus

Voice 25KHz 569-572 772.5625 802.5625

Voice 25KHz 573-576 772.5875 802.5875 Campus

Voice 25KHz 629-632 772.9375 802.9375

Voice 25KHz 713-716 773.4625 803.4625

Voice 25KHz 753-756 773.7125 803.7125 Campus

Voice 25KHz 757-760 773.7375 803.7375

Voice 25KHz 829-832 774.1875 804.1875

St. Clair Voice 25KHz 97-100 769.6125 799.6125 Campus

Voice 25KHz 129-132 769.8125 799.8125

Voice 25KHz 289-292 770.8125 800.8125 Campus

Voice 25KHz 373-376 771.3375 801.3375

Voice 25KHz 433-436 771.7125 801.7125

Voice 25KHz 437-440 771.7375 801.7375 Campus

Voice 25KHz 485-488 772.0375 802.0375 Campus

Voice 25KHz 493-496 772.0875 802.0875 Campus

Voice 25KHz 517-520 772.2375 802.2375 Campus

Voice 25KHz 537-540 772.3625 802.3625 Campus

Voice 25KHz 545-548 772.4125 802.4125

Voice 25KHz 573-576 772.5875 802.5875 Campus

Voice 25KHz 609-612 772.8125 802.8125

Voice 25KHz 673-676 773.2125 803.2125 Campus

Voice 25KHz 757-760 773.7375 803.7375 Campus

Voice 25KHz 877-880 774.4875 804.4875

St. Francois Voice 25KHz 49-52 769.3125 799.3125

Voice 25KHz 97-100 769.6125 799.6125

Voice 25KHz 201-204 770.2625 800.2625

Voice 25KHz 245-248 770.5375 800.5375

Voice 25KHz 293-296 770.8375 800.8375

Voice 25KHz 333-336 771.0875 801.0875

Voice 25KHz 405-408 771.5375 801.5375

Voice 25KHz 453-456 771.8375 801.8375

Voice 25KHz 485-488 772.0375 802.0375

Voice 25KHz 533-536 772.3375 802.3375

Voice 25KHz 585-588 772.6625 802.6625

Voice 25KHz 673-676 773.2125 803.2125

Voice 25KHz 753-756 773.7125 803.7125

Voice 25KHz 901-904 774.6375 804.6375

St. Louis

(City) Voice 25KHz 17-20 769.1125 799.1125 Campus

Voice 25KHz 89-92 769.5625 799.5625 Campus

Voice 25KHz 205-208 770.2875 800.2875 Campus

Voice 25KHz 353-356 771.2125 801.2125

Voice 25KHz 393-396 771.4625 801.4625

Voice 25KHz 457-460 771.8625 801.8625

Voice 25KHz 497-500 772.1125 802.1125

Voice 25KHz 553-556 772.4625 802.4625

Voice 25KHz 617-620 772.8625 802.8625

Voice 25KHz 665-668 773.1625 803.1625

Voice 25KHz 705-708 773.4125 803.4125

Voice 25KHz 797-800 773.9875 803.9875

Voice 25KHz 877-880 774.4875 804.4875

St. Louis

County Voice 25KHz 13-16 769.0875 799.0875

Voice 25KHz 53-56 769.3375 799.3375

Voice 25KHz 93-96 769.5875 799.5875

Voice 25KHz 169-172 770.0625 800.0625

Voice 25KHz 209-212 770.3125 800.3125

Voice 25KHz 249-252 770.5625 800.5625

Voice 25KHz 289-292 770.8125 800.8125

Voice 25KHz 329-332 771.0625 801.0625

Voice 25KHz 369-372 771.3125 801.3125

Voice 25KHz 409-412 771.5625 801.5625

Voice 25KHz 477-480 771.9875 801.9875

Voice 25KHz 481-484 772.0125 802.0125

Voice 25KHz 541-544 772.3875 802.3875

Voice 25KHz 545-548 772.4125 802.4125 Campus

Voice 25KHz 609-612 772.8125 802.8125

Voice 25KHz 677-680 773.2375 803.2375

Voice 25KHz 749-752 773.6875 803.6875

Voice 25KHz 789-792 773.9375 803.9375

Voice 25KHz 865-868 774.4125 804.4125

Voice 25KHz 905-908 774.6625 804.6625

Voice 25KHz 945-948 774.9125 804.9125

Ste.

Genevieve Voice 25KHz 325-328 771.0375 801.0375

Voice 25KHz 365-368 771.2875 801.2875

Voice 25KHz 413-416 771.5875 801.5875

Voice 25KHz 465-468 771.9125 801.9125

Voice 25KHz 525-528 772.2875 802.2875

Voice 25KHz 605-608 772.7875 802.7875

Voice 25KHz 741-744 773.6375 803.6375

Voice 25KHz 785-788 773.9125 803.9125

Stoddard Voice 25KHz 89-92 769.5625 799.5625

Voice 25KHz 297-300 770.8625 800.8625

Voice 25KHz 389-392 771.4375 801.4375

Voice 25KHz 429-432 771.6875 801.6875

Voice 25KHz 469-472 771.9375 801.9375

Voice 25KHz 481-484 772.0125 802.0125

Voice 25KHz 561-564 772.5125 802.5125

Voice 25KHz 601-604 772.7625 802.7625

Voice 25KHz 673-676 773.2125 803.2125

Voice 25KHz 749-752 773.6875 803.6875

Voice 25KHz 877-880 774.4875 804.4875

Voice 25KHz 941-944 774.8875 804.8875

Stone Voice 25KHz 85-88 769.5375 799.5375

Voice 25KHz 329-332 771.0625 801.0625

Voice 25KHz 401-404 771.5125 801.5125

Voice 25KHz 457-460 771.8625 801.8625

Voice 25KHz 521-524 772.2625 802.2625

Voice 25KHz 601-604 772.7625 802.7625

Voice 25KHz 793-796 773.9625 803.9625

Voice 25KHz 869-872 774.4375 804.4375

Voice 25KHz 909-912 774.6875 804.6875

Sullivan Voice 25KHz 337-340 771.1125 801.1125

Voice 25KHz 421-424 771.6375 801.6375

Voice 25KHz 469-472 771.9375 801.9375

Voice 25KHz 549-552 772.4375 802.4375

Voice 25KHz 785-788 773.9125 803.9125

Voice 25KHz 833-836 774.2125 804.2125

Voice 25KHz 901-904 774.6375 804.6375

Taney Voice 25KHz 125-128 769.7875 799.7875

Voice 25KHz 165-168 770.0375 800.0375

Voice 25KHz 249-252 770.5625 800.5625

Voice 25KHz 361-364 771.2625 801.2625

Voice 25KHz 433-436 771.7125 801.7125

Voice 25KHz 485-488 772.0375 802.0375

Voice 25KHz 637-640 772.9875 802.9875

Voice 25KHz 701-704 773.3875 803.3875

Voice 25KHz 741-744 773.6375 803.6375

Voice 25KHz 781-784 773.8875 803.8875

Voice 25KHz 821-824 774.1375 804.1375

Voice 25KHz 861-864 774.3875 804.3875

Texas Voice 25KHz 17-20 769.1125 799.1125

Voice 25KHz 81-84 769.5125 799.5125

Voice 25KHz 129-132 769.8125 799.8125

Voice 25KHz 201-204 770.2625 800.2625

Voice 25KHz 245-248 770.5375 800.5375

Voice 25KHz 321-324 771.0125 801.0125

Voice 25KHz 393-396 771.4625 801.4625

Voice 25KHz 445-448 771.7875 801.7875

Voice 25KHz 517-520 772.2375 802.2375

Voice 25KHz 865-868 774.4125 804.4125

Voice 25KHz 917-920 774.7375 804.7375

Vernon Voice 25KHz 169-172 770.0625 800.0625

Voice 25KHz 209-212 770.3125 800.3125

Voice 25KHz 361-364 771.2625 801.2625

Voice 25KHz 409-412 771.5625 801.5625

Voice 25KHz 449-452 771.8125 801.8125

Voice 25KHz 481-484 772.0125 802.0125

Voice 25KHz 521-524 772.2625 802.2625

Voice 25KHz 589-592 772.6875 802.6875

Voice 25KHz 837-840 774.2375 804.2375

Voice 25KHz 901-904 774.6375 804.6375

Warren Voice 25KHz 81-84 769.5125 799.5125

Voice 25KHz 177-180 770.1125 800.1125

Voice 25KHz 217-220 770.3625 800.3625

Voice 25KHz 325-328 771.0375 801.0375

Voice 25KHz 365-368 771.2875 801.2875

Voice 25KHz 429-432 771.6875 801.6875

Voice 25KHz 517-520 772.2375 802.2375

Voice 25KHz 613-616 772.8375 802.8375

Washington Voice 25KHz 17-20 769.1125 799.1125

Voice 25KHz 173-176 770.0875 800.0875

Voice 25KHz 257-260 770.6125 800.6125

Voice 25KHz 373-376 771.3375 801.3375

Voice 25KHz 425-428 771.6625 801.6625

Voice 25KHz 473-476 771.9625 801.9625

Voice 25KHz 513-516 772.2125 802.2125

Voice 25KHz 561-564 772.5125 802.5125

Voice 25KHz 701-704 773.3875 803.3875

Voice 25KHz 745-748 773.6625 803.6625

Voice 25KHz 797-800 773.9875 803.9875

Wayne Voice 25KHz 125-128 769.7875 799.7875

Voice 25KHz 241-244 770.5125 800.5125

Voice 25KHz 329-332 771.0625 801.0625

Voice 25KHz 381-384 771.3875 801.3875

Voice 25KHz 457-460 771.8625 801.8625

Voice 25KHz 493-496 772.0875 802.0875

Voice 25KHz 589-592 772.6875 802.6875

Voice 25KHz 661-664 773.1375 803.1375

Webster Voice 25KHz 133-136 769.8375 799.8375

Voice 25KHz 173-176 770.0875 800.0875

Voice 25KHz 257-260 770.6125 800.6125

Voice 25KHz 337-340 771.1125 801.1125

Voice 25KHz 377-380 771.3625 801.3625

Voice 25KHz 437-440 771.7375 801.7375

Voice 25KHz 513-516 772.2125 802.2125

Voice 25KHz 565-568 772.5375 802.5375

Voice 25KHz 605-608 772.7875 802.7875

Voice 25KHz 797-800 773.9875 803.9875

Voice 25KHz 913-916 774.7125 804.7125

Worth Voice 25KHz 213-216 770.3375 800.3375

Voice 25KHz 289-292 770.8125 800.8125

Voice 25KHz 337-340 771.1125 801.1125

Voice 25KHz 389-392 771.4375 801.4375

Voice 25KHz 549-552 772.4375 802.4375

Voice 25KHz 677-680 773.2375 803.2375

Wright Voice 25KHz 453-456 771.8375 801.8375

Voice 25KHz 497-500 772.1125 802.1125

Voice 25KHz 557-560 772.4875 802.4875

Voice 25KHz 613-616 772.8375 802.8375

Voice 25KHz 669-672 773.1875 803.1875

Voice 25KHz 709-712 773.4375 803.4375

Voice 25KHz 749-752 773.6875 803.6875

Voice 25KHz 873-876 774.4625 804.4625

Channels labeled “Campus” are subject to ERP and Service Area limitations. See

section 3.12, Paragraph “F” for additional information.

**PROCESS FOR HANDLING UNFORMED REGIONS**

The Implementation Subcommittee recommends that all Regions use the following pre-planning

methodology to facilitate coordination with adjacent Regions. This procedure will provide a

spectrum allotment for adjacent Regions that do not immediately form a Committee.

Counties or other geographic subdivisions within 70 miles of the Regional border need to share

spectrum with the adjacent Region(s). The appropriate ratio of channels shall be allotted to counties

in adjacent Regions based upon each county’s population. A 25 kHz building block will be used to

distribute spectrum between the Regions. A description of the demographics of the affected border

areas shall be included.

*The requirements for adjacent Region concurrence will require a waiver if the adjacent Region has*

*not yet formed. The Region filing the Plan must use the pre-planning procedure outlined above.*

*The waiver request must be filed concurrently with the Plan and contained in the cover letter.*

**The following form is an electronic copy of the signed PFD versions**

**from Region 24’s adjacent regions accompanying this document.**

**Appendix H**

**Sample Form**

**Inter-Regional Coordination Procedures**

**And**

**Procedures for Resolution of Disputes**

**That May Arise Under FCC Approved Plans**

**I.**

**II. INTRODUCTION**

1. This is a mutually agreed upon Inter-Regional Coordination Procedures

Agreement (Agreement) by and between the following 700 MHz Regional Planning Committees,

**Region XX**

**Region XX**

**II. INTER-REGIONAL COORDINATION AGREEMENT**

2. The following is the specific procedure for inter-Regional coordination which has

been agreed upon by Regions 24, X, XX, XX, XX, XX, XX, XX and XX and which will be used by

the Regions to coordinate with adjacent Regional Planning Committees.

a. An application-filing window is opened or the Region announces that it

is prepared to begin accepting applications on a first-come/first-served basis.

b. Applications by eligible entities are accepted.

c. An application-filing window (if this procedure is being used) is closed

after appropriate time interval.

d. Intra-Regional review and coordination takes place, including a technical

review resulting in assignment of channels.

e. After intra-Regional review, a copy of those frequency-specific

applications requiring adjacent Region approval, including a definition statement of proposed

service area, shall then be forwarded to the adjacent Region(s) for review. 2 This information will

be sent to the adjacent Regional chairperson(s) using the CAPRAD database.

f. The adjacent Region reviews the application. If the application is

approved, a letter of concurrence shall be sent, via the CAPRAD database, to the initiating Regional

chairperson within thirty (30) calendar days.

*II. Dispute Resolution*

(1) If the adjacent Region(s) cannot approve the request, the adjacent Region shall

document the reasons for partial or non-concurrence, and respond within 10 (Ten)-calendar

days via email. If the applying Region cannot modify the application to satisfy the

objections of the adjacent Region then, a working group comprised of representatives of the

two Regions shall be convened within thirty (30) calendar days to attempt to resolve the

dispute. The working group shall then report its findings within thirty (30) calendar days to

the Regional chairpersons email (CAPRAD database). Findings may include, but not be

limited to:

(i) Unconditional concurrence;

(ii) Conditional concurrence contingent upon modification of

Applicant’s technical parameters; or

2 If an applicant’s proposed service area extends into an adjacent Public Safety Region (s), the affected Region(s) must

approve the application. Service area shall normally be defined as the area included within the geographical boundary of

the applicant, plus three (3) miles. Other definitions of service area shall be justified with an accompanying

*Memorandum of Understanding (MOU)* or other application documentation between agencies, i.e. mutual aid

agreements.

 (iii) Partial or total denial of proposed frequencies due to inability to

meet co-channel/adjacent channel interference free protection to

existing licensees within the adjacent Region.

(2) If the Inter-Regional Working Group cannot resolve the dispute, then the matter shall be

forwarded for evaluation to the National Plan Oversight Committee (NPOC), of the National

Public Safety Telecommunications Council (NPSTC). Each Region involved in the dispute

shall include a detailed explanation of its position, including engineering studies and any other

technical information deemed relevant. The NPOC will, within thirty (30) calendar days,

report its recommendation(s) to the Regional chairpersons via the CAPRAD database. The

NPOC’s decision may support either of the disputing Regions or it may develop a proposal that

it deems mutually advantageous to each disputing Region.

g. Where adjacent Region concurrence has been secured, and the channel

assignments would result in no change to the Region’s currently Commission approved channel

assignment matrix. The initiating Region may then advise the applicant(s) that their application

may be forwarded to a frequency coordinator for processing and filing with the Commission.

h. Where adjacent Region concurrence has been secured, and the channel

assignments would result in a change to the Region’s currently Commission approved channel

assignment matrix, then the initiating Region shall file with the Commission a *Petition to Amend*

their current Regional plan’s frequency matrix, reflecting the new channel assignments, with a copy

of the *Petition* sent to the adjacent Regional chairperson(s).

i. Upon Commission issuance of an *Order* adopting the amended channel

assignment matrix, the initiating Regional chairperson will send a courtesy copy of the *Order* to the

adjacent Regional chairperson(s) and may then advise the applicant(s) that they may forward their

applications to the frequency coordinator for processing and filing with the Commission.

**III. CONCLUSION**

3. IN AGREEMENT HERETO, Regions 4,13,15,16,17,24,26,34 and 39 do hereunto

set their signatures the day and year first above written.

Respectfully,

 [all signatories to agreement]

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Appendix I**

**DTV transition**

**Frequency Availability through the DTV Transition**

**(NOTE: DTV transition continues to be a topic discussed across the country. Region 24 is**

**fortunate to be relatively unencumbered with regard to primary 700 MHz licensee**

**broadcasters operating high power analog TV stations on channels 63-64 or 68-69. KSMOTV**

**Channel 62 operates in the Kansas City area and will encumbered some of the 63-68**

**channel pair in the Kansas City operating area. Region 24 will continue to distribute DTV**

**transition information to its members.**

***4.1.1.1.1 On August 14, 1996, the FCC released a* Sixth Further Notice of Proposed Rule**

**Making *in the digital television (DTV) proceeding. A portion of the spectrum recovered from TV***

***channels 60-69 when DTV is fully deployed "could be used to meet public safety needs."3 By***

***Congressional direction in the Balanced Budget Act of 1997, the FCC reallocated 24 MHz of spectrum to***

***Public Safety services in the 769-775 MHz and 794-806 MHz bands. The statute required the FCC to***

***establish service rules, by September 30, 1998, in order to start the process of assigning licenses. The rules***

***that the FCC established by September 30, 1998, "provided the minimum technical framework necessary to***

***standardize operations in this spectrum band, including, but not limited to: (a) establishing interference***

***limits at the boundaries of the spectrum block and service areas; (b) establishing technical restrictions***

***necessary to protect full-service analog and digital television service during the transition to digital***

***television services; (c) permitting public safety licensees the flexibility to aggregate multiple licenses to***

***create larger spectrum blocks and service areas, and to disaggregate or partition licenses to create smaller***

***spectrum blocks or service areas; and (d) ensuring that the new spectrum will not be subject to harmful***

***interference from television broadcast licensees" 4.***

In April 1997, the FCC assigned a second 6 MHz block of spectrum to each license (or

permit to construct) holders of full power, analog, television broadcast station (NTSC) in order to

3 Advanced Television Systems and Their Impact Upon the Existing Television Broadcast Service*,*

MM Docket No. 87-268, *Sixth Further Notice of Proposed Rule Making*, 11 FCC Rcd 10,968, 10,980

(1996) (*DTV Sixth Notice*).

4

FCC 98-191, 1st R&O and 3rd NPRM on WT Docket No. 96-86 Operational & Technical Requirements or the 700 MHz Public Safety Band,

para.4.

construct a digital television station (DTV). Secondary low power television stations (LPTV),

secondary translators and boosters (TX), mutually exclusive applications for new stations, and

application filed after a cut-off date did not receive a second 6 MHz allotment for DTV. The FCC

established about a 10 year timeline for those stations with a DTV assignment to construct a DTV

station, cease NTSC transmissions, and return one of the two 6 MHz blocks of spectrum to the

FCC. Target date for the end of analog television (NTSC) transmission was set for December 31,

2006.

Congress provided several market penetration loopholes (>85% households served, all 4

major networks converted, etc) allowing NTSC operations to continue past the December 31, 2006

date. While there are over 100 NTSC full power stations in this band, there are also about 12 DTV

assignments. The DTV assignments might continue operations past the December 31, 2006 date for

two reasons. 1) They must find a suitable channel below channel 60 to move to, which may be their

own NTSC assignment. They may not be able to find another allocation until other NTSC stations

have ceased operations and returned a channel below 60 to the FCC. Or, 2) their license does not

expire until after 2006 (most are licensed into 2007 or 2008).

**Protection of Public Safety from future TV/DTV Stations**

Public safety base and mobile operations must have a safe distance between the co-channel or

adjacent TV and DTV systems. This typically means that a co-channel and adjacent channel base and

mobile system cannot operate in areas where TV stations already exist. The public safety systems that

will operate in the 700 MHz band for some locations in the U.S. and its possessions must wait until

the transition period is over and the TV/DTV stations have moved to other channels before beginning

operations. In other areas, channels will be available for public safety operations. During the

transition period, public safety stations must be acutely aware of the TV allocations for both TV and

DTV stations. The FCC wants the number of situations where the public safety licensee has to

coordinate its station with the existing TV stations kept to a minimum. The Commission's decisions

in the reallocation of spectrum to DTV implemented two requirements, which will help public safety

systems to protect TV/DTV stations and reduce the number of coordination’s. The first requirement

is that full power UHF-TV stations can no longer apply for channels 60-69 or modifications in

channels 60-69, which would increase the stations' service areas, which creates a known environment

for public safety licensees. The second requirement is that since only existing TV station licensees can

apply for DTV channels, the applicants and their proposed locations are already known.

Also, the low power TV stations and translators already on channels 60-69 are secondary and

must cease operations if they cause harmful interference when a primary service, like land mobile,

comes into operation. The secondary Low Power TV stations already on channels 60-69 cannot apply

for the new Class A protection status.

**Spectrum Overview**

**700 MHz Public Safety Band**

The FCC designated 769-775 MHz for base-to-mobile transmissions and 799-805 MHz for mobileto-

base communications. In addition, base transmit channels in TV Channel 63 are paired with

mobile channels in TV Channel 68 and likewise that base channels in TV Channel 64 are paired

with mobile channels in TV Channel 69. This provides 30 MHz separations between base and

mobile transmit channel center frequencies. This band plan was suggested because of the close

proximity of TV Channels 68 and 69 to the 806-824 MHz band, which already contains the transmit

channels for mobile and portable radios (base receive).

Mobile transmissions are allowed on any part of the 700 MHz band, not just the upper 12 MHz.

This will facilitate direct mobile-to-mobile communications (*i.e.*, not through a repeater) that are

often employed at the site of an incident, where wide area communications facilities are not

available or desired. Allowing mobile transmissions on both halves of a paired channel is generally

consistent with FCC rules governing use of other public safety bands.

Non-uniform TV Channel Pairing

There are currently geographical areas where, either licensed or otherwise protected fullservice

analog or new digital, television stations are currently authorized to operate on TV

Channels 62, 63, 64, 65, 67, 68, and 69.5 During the DTV transition period, an incumbent TV station

occupying one or more of the four Public Safety channels (63, 64, 68, 69) or the three adjacent

channels (62, 65, 67) may preclude pairing of the channels in accordance with the band plan defined

above. Therefore, to provide for cases where standard pairing is not practicable during the DTV

transition period, the FCC will allow the RPCs to consider pairing base-to-mobile channels in

TV Channel 63 with mobile-to-base channels in TV Channel 69 and/or base-to-mobile channels in

TV Channel 64 with mobile-to-base channels in TV Channel 68. Because such non-standard channel

pairing may cause problems when the band becomes more fully occupied, the FCC expects the RPCs

to permit such non-standard channel pairing only when absolutely necessary, and the FCC may

require stations to return to standard channel pairing after the DTV transition period is over.

However, the FCC will not permit non-standard channel pairing on the nationwide interoperability

channels in the 700 MHz band because of the need for nationwide uniformity of these channels.

5 *See Reallocation, Notice of Proposed Rule Making,* 12 FCC Rcd at 14,141, 14,177-78 and

14,182-83.

At least three issues must be considered before deciding upon non-uniform channel pairing:

1) Preliminary analysis, looking at current incumbent TV stations, shows few geographic areas

where non-uniform pairing allows early implementation of 700 MHz systems. As DTV Transition

progresses, and TV stations vacate the band, this situation might change.

2) If interoperability channels must be uniform, operation on I/O channels will be blocked until all

incumbent TV stations are cleared, even though General Use channels may be implemented earlier.

3) If I/O channels must follow uniform pairing, and general use & reserve channels can be

implemented using non-uniform pairing, narrowband voice subscriber equipment must operate on 3

different channel pairings - 39 MHz (764-767 paired with 803-806 MHz), 30 MHz, and 21 MHz

(773-776 paired with 794-797 MHz). Likewise, there will be 3 different channel pairing for

wideband channels. No vendors have volunteered to build equipment & systems for non-uniform

pairing, yet.

**TV/DTV Protection**

During the DTV Transition period, public safety must consider all co-channel and adjacent

channel TV and DTV stations within about a 160 mile radius.

For public safety channel pair 63/68, public safety must consider six TV/DTV channels - cochannels

63 and 68, as well as, adjacent channels 62, 64, 67, and 69.

-100

-90

-80

-70

-60

-50

-40

-30

-20

-10

-6 -3 0 0 +3 +6

Measured NTSC Signal

-100

-90

-80

-70

-60

-50

-40

-30

-20

-10

-6 -3 0 0 +3 +6

Measured NTSC Signal

**CH-62 CH-63 CH-64**

**Fixed Transmit,**

**Mobile Talk-around Transmit,**

**&**

**Control Station & Mobile Receive**

**CH-67 CH-68 CH-69**

**Fixed Receive**

**&**

**Control Station & Mobile Transmit**

**NB**

**Voice**

**WB**

**Data**

**NB**

**Voice**

**WB**

**Data**

**NB**

**Voice**

**WB**

**Data**

**NB**

**Voice**

**WB**

**Data**

**Measured (off-the-air) Analog TV Signal**

**vs**

**700 MHz Public Safety Assignments**

**HAVE 2 CO-CHANNEL AND 4 ADJACENT CHANNELS**

**TO CONSIDER FOR EACH 700 MHz PAIRED BLOCKS OF SPECTRUM**

**CH-62 CH-63 CH-64**

-6 -3 0 Fd, MHz 0 +3 +6

**Lower Adjacent Co-Channel Upper Adjacent**

**Fixed Transmit,**

**Mobile Talk-around Transmit,**

**&**

**Control Station & Mobile Receive**

-6 -3 0 Fd, MHz 0 +3 +6

**Lower Adjacent Co-Channel Upper Adjacent**

**CH-67 CH-68 CH-69**

**Fixed Receive**

**&**

**Control Station & Mobile Transmit**

**DTV Emission Mask**

**vs**

**700 MHz Public Safety Assignments**

**HAVE 2 CO-CHANNEL AND 4 ADJACENT CHANNELS**

**TO CONSIDER FOR EACH 700 MHz PAIRED BLOCKS OF SPECTRUM**

**NB**

**Voice**

**WB**

**Data**

**NB**

**Voice**

**WB**

**Data**

**NB**

**Voice**

**WB**

**Data**

**NB**

**Voice**

**WB**

**Data**

For public safety channel pair 64/69, public safety must consider five TV/DTV channels;

co-channels 64 and 69, as well as, adjacent channels 63, 65, and 68.

It may only take one TV/DTV station to block operations on one, the other, or both public

safety channel pairs. For a public safety system at 500 watts ERP and 500 ft HAAT, co-channel TV

stations can block a 120 mile radius and adjacent channel TV/DTV stations can block a 90 mile

radius.

Since base stations transmitters are located only on channels 63 and 64, LMR mobile only

TV/DTV protection spacing on channels 68 and 69 may be shorter than LMR base TV/DTV

protection on channels 63 & 64.

**TV/DTV Protection Criteria**

Public safety applicants can select one of three ways to meet the TV/DTV protection

requirements: (1) utilize the geographic separation specified in the 40 dB Tables of 90.309;

(2) submit an engineering study to justify other separations which the Commission approves; or

(3) obtain concurrence from the applicable TV/DTV station(s).

**90.309 40 dB D/U Tables**

The FCC adopted a 40 dB desired (TV/DTV) to undesired (LMR) signal ratio for co-channel

operations and a 0 dB desired/undesired (D/U) signal ratio for adjacent channel operations. The

D/U ratio is used to determine the geographic separation needed between public safety base stations

and the Grade B service contours of co-channel and adjacent channel TV/DTV stations. The D/U

signal ratio is used to determine the level of land mobile signals that can be permitted at protected

fringe area TV receiver locations without degrading the TV picture to less than a defined picture

quality. In other words, the D/U signal ratio indicates what relative levels of TV and land mobile

signals can be tolerated without causing excessive interference to TV reception at the fringe of the

TV service area.

Desired and undesired contours are not quite the same thing. Desired analog TV contours

are defined as F(50,50), meaning coverage is 50% of the places and 50% of the time. Undesired

land mobile or interference contours are defined as F(50,10). For Digital TV, the desired contours

are defined as F(50,90), while the undesired land mobile contour are still F(50,10).

Land mobile and analog TV services have successfully shared the 470-512 MHz band

(TV Channels 14-20) within a 50 mile radius of eleven major cities since the early 1970's based

upon providing a signal ratio of at least 50 dB between the desired TV signal and undesired cochannel

land mobile signal (D/U signal ratio) at a hypothetical 88.5 km (55 mi) Grade B service

contour and an adjacent channel D/U signal ratio of 0 dB at the same hypothetical Grade B service

contour. These separation distances also protected the land mobile systems from interference from

the TV stations. In 1985, recognizing that 50 dB D/U was too conservative, the FCC proposed to

expand land mobile/TV sharing to other TV channels and proposed that the geographic separation

requirements for co-channel operations be based on a D/U signal ratio of 40 dB rather than 50 dB.

That proceeding was put on hold pending completion of the DTV proceeding, which has now been

completed. In the 470-512 MHz band, the FCC also relied on minimum separation distances based

on the various heights and powers of the land mobile stations (HAAT/ERP separation tables) to

prevent harmful interference.

Since this simple, yet conservative, method was successful, the FCC decided to use this same

method, the 90.309 HAAT/ERP Separation Tables, to administer LMR to TV/DTV receiver

protection criteria for the services in the 700 MHz band.

Co-channel land mobile base station transmitters are limited to a maximum signal strength at the

hypothetical TV Grade B contour 40 dB D/U below desired 64 dBu F(50,50) analog TV signal

level, or 24 dBu F(50,10). The FCC adopted a 0 dB D/U signal ratio for adjacent channel

operations*.* Adjacent channel land mobile transmitters will be limited to a maximum signal of 64

dBu F(50,10) which is 0 dB D/U below the TV Grade B signal of 64 dBu F(50,50) at the TV station

Grade B contour of 88.5 km (55 miles). A typical TV receiver's adjacent channel rejection is at

least 10-20 dB greater than this level, which will further safeguards TV receivers from land mobile

interference.

***4.2***

**T**

**R**

**T**

**R**

**LMR to Analog TV Co-channel Interference**

**LMR**

**Repeater**

**LMR Repeater**

**Antenna w/**

**500 watt ERP,**

**< 500 ft HAAT,**

**& Vertical**

**Polarization**

**Portable Radio**

**<3 watts**

**Mobile Radio**

**< 30 watts**

**LMR Control Station**

**Antenna w/ HAAT & AGL,**

**Directional Gain, &**

**Vertical Polarization**

**NTSC**

**TV 62-69**

**RCVR**

**TV Rcvr at Grade B Contour**

**w/**

**9.1 meter Antenna AGL,**

**IGNORING**

**Horizontal Polarization,**

**Directional Yagi Antenna**

**w/ Gain = 10 dB &**

**Front/Back Ratio = 14 dB,**

**& Line Loss = 4 dB**

**TV 62-69**

**XMTR**

**TV antenna w/**

**up to 5000 watt ERP,**

**> 500 ft HAAT,**

**& Horizontal**

**Polarization**

**64 dBu F(50,50)**

**horizontally polarized**

**TV Signal**

**24 dBu F(50,10)**

**[~10 dBu F(50,50)]**

**vertically polarized**

**co-channel LMR Signal**

**T**

**R**

**T**

**R**

**LMR to Analog TV Adj-channel Interference**

**LMR**

**Repeater**

**LMR Repeater**

**Antenna w/**

**500 watt ERP,**

**< 500 ft HAAT,**

**& Vertical**

**Polarization**

**Portable Radio**

**<3 watts**

**Mobile Radio**

**< 30 watts**

**LMR Control Station**

**Antenna w/ HAAT & AGL,**

**Directional Gain, &**

**Vertical Polarization**

**NTSC**

**TV 62-69**

**RCVR**

**TV Rcvr at Grade B Contour w/**

**9.1 meter Antenna AGL,**

**IGNORING**

**Horizontal Polarization,**

**Directional Yagi Antenna**

**w/ Gain = 10 dB &**

**Front/Back Ratio = 14 dB,**

**& Line Loss = 4 dB**

**TV 62-69**

**XMTR**

**TV antenna w/**

**up to 5000 watt ERP,**

**> 500 ft HAAT,**

**& Horizontal**

**Polarization**

**64 dBu F(50,50)**

**horizontally polarized**

**TV Signal**

**64 dBu F(50,10)**

**vertically polarized**

**adj-channel LMR Signal**

The equivalent ratios for a DTV station's 41 dB F(50,90) desired field strength contour are land

mobile 17 dB F(50,10) contour for co-channel and land mobile - 23 dB F(50,10) contour for

adjacent channel.

The Tables to protect TV/DTV stations are found in Section 90.309 of the Commission's rules.

These existing Tables cover co-channel protection based on a 40 dB D/U ratio using the separation

methods described in Section 73.611 of the Commission's rules for base, control, and mobile

stations, and for adjacent channel stations for base stations based on a 0 dB D/U ratio.

However, the original considerations in 470-512 MHz band under Section 90.309 were different in

that mobiles were limited in their roaming distance from the base station (less than 30 miles) and

mobiles were on the same TV channel as the base station.

Control and mobile stations (including portables) are limited in height (200 ft for control stations,

20 ft for mobiles/portables) and power (200 watts ERP for control stations, 30 watts for mobiles, 3

watts for portables). Mobiles and control stations shall afford protection to co-channel and adjacent

channel TV/DTV stations in accordance with the values specified in Table D (co-channel

frequencies based on 40 dB protection for TV and 17 dB for DTV) in § 90.309.

Control stations and mobiles/portables shall keep a minimum distance of 8 kilometers (5 miles)

from all adjacent channel TV/DTV station hypothetical or equivalent Grade B contours (adjacent

channel frequencies based on 0 dB protection for TV and -23 dB for DTV). This means that control

and mobile stations shall keep a minimum distance of 96.5 kilometers (60 miles) from all adjacent

channel TV/DTV stations.

Since operators of mobiles and portables are able to move and communicate with each other,

licensees or coordinators must determine the areas where the mobiles can and cannot roam in order

to protect the TV/DTV stations, and advise the mobile operators of these areas and their restrictions.

**Engineering Analysis**

Limiting TV/land mobile separation to distances specified in the 40 dB HAAT/ERP Separation

Tables found in 90.309 may prevent public safety entities from fully utilizing this spectrum in a

number of major metropolitan areas until after the DTV transition period ends. Public safety

applicants will be allowed to submit engineering studies showing how they propose to meet the

appropriate D/U signal ratio at the existing TV station's authorized or applied for Grade B service

contour or equivalent contour for DTV stations instead of the hypothetical contour at 88.5 km.

This would permit public safety applicants to take into account intervening terrain and engineering

techniques such as directional and down-tilt antennas in determining the necessary separation to

provide the required protection. Public safety applicants who use the engineering techniques must

consider the actual TV/DTV parameters and not base their study on the 88.5 km hypothetical or

equivalent Grade B contour. If land mobile interference contour does not overlap the TV Grade B

contour (or DTV equivalent), then engineering analysis may be submitted to the FCC with the

application.

**55 miles**

**~45 miles**

**55 mile**

**hypothetical**

**Grade B Contour**

**TV Licensed**

**64 dBu F(50,50)**

**Contour**

**Public Safety**

**Service Area**

**<63 miles**

**<30 miles**

**TV LMR**

**LMR**

**24 dBu F(50,10)**

**Contour**

**500 watts ERP**

**500 feet HAAT**

**700 MHz Band - LMR to Co-Channel TV Spacing using 40 dBu Table**

**Many Channel 60-69 TV stations do not have 55 mile radius Grade B contours.**

**Average calculated for NE corridor is less than 45 miles.**

**Area not usuable**

**by Public Safety**

**Per 90.545 (c)(1)(i)**

**use 90.309 Table B (40 dBu)**

**based upon hypothetical 55 mile Grade B contour**

**which results in greater than 120 miles separation for**

**LMR @ 500 watts ERP & 500 feet HAAT**

**(~45 miles)**

This method is most useful with lower power TV stations whose Grade B contours are much smaller than the hypothetical

55 mile (88.5 km) Grade B contour or have directional patterns

**55 miles**

**~45 miles**

**55 mile**

**hypothetical**

**Grade B Contour**

**TV Licensed**

**64 dBu F(50,50)**

**Contour**

**Public Safety**

**Service Area**

**<63 miles**

**<30 miles**

**TV LMR**

**LMR**

**24 dBu F(50,10)**

**Contour**

**500 watts ERP**

**500 feet HAAT**

**Area not**

**usuable by**

**Public Safety**

**reduced >45 miles**

**separation to**

**<35 miles**

**Less than 110 miles**

**700 MHz Band - Public Safety to Co-Channel TV Spacing**

**using Engineering Analysis per 90.545(c)(1)(ii)**

**Actual LMR 24 dBu contour just touches Licensed TV/DTV 64 dBu contour**

***Note that 200 ft AGL limitations on 700 MHz control stations is much higher than the 100 ft AGL limitation***

***used at UHF. Limiting control station antenna height and/or ERP may greatly reduce land mobile to TV***

***contour spacing.***

Also, note that analysis for TV/DTV receivers uses 30 ft (10 m) antenna height whereas,

analysis for land mobile subscribers uses about a 6 ft (2m) antenna height.

**TV/DTV Short-spacing**

***4.3 Public safety applicants will also be allowed to "short-space" even closer if they get the (written)***

***approval of the TV stations they are required to protect. Public safety applicants need to determine the station's***

***intended market area vs its hypothetical Grade B contour area. Alternately, the TV/DTV station may be shortspaced***

***against another TV/DTV station, limiting their area of operation, but does not affect LMR operations.***

***4.4 Instead of each agency negotiating with a TV/DTV station individually, they may want to combine***

***into a single group or committee and negotiate together.***

**55 miles**

**Offset Antenna Pattern**

**TV Licensed**

**TV 64 dBu F(50,50)**

**Contour**

**LMR**

**24 dBu F(50,10)**

**Contour**

**Public Safety**

**Service Area**

**<30 miles**

**35 miles**

**LMR**

**55 miles**

**55 mile**

**hypothetical**

**Grade B Contour**

**TV 500 watts ERP**

**500 feet HAAT**

**Less than**

**minimum 90 miles**

**700 MHz Band - Public Safety to Co-Channel TV Spacing**

**using Engineering Analysis per 90.545(c)(1)(ii)**

**Actual LMR 24 dBu contour just touches Actual TV/DTV 64 dBu contour**

**Ability to consider the effects of terrain may greatly**

**reduce the separation required between LMR and TV.**

**TV/DTV Height Adjustment Factor**

***4.5 In order to protect certain TV/DTV stations which have extremely large contours due to unusual***

***height situations, such as a television station mounted on top of Mount Wilson near Los Angeles, California, the***

***FCC incorporated an additional height adjustment factor which must be used by all public safety base, control***

***and mobile stations to protect these few TV/DTV stations and afford the land mobile stations the necessary***

***protection from the TV/DTV stations. The equation necessary to calculate the additional distance from the***

***hypothetical or equivalent Grade B contour is found in the rules section 90.545(c)(2)(iii).***

**CANADIAN AND MEXICAN BORDER REGIONS**

The FCC typically takes one of two approaches. They either postpone licensing of land

mobile stations within a certain geographic distance (*e.g.,* 120 km (75 miles)) of Canada and

Mexico, or permit interim authorizations conditioned on the outcome of future agreements.

Because international negotiations can take many months or even years to finalize, the FCC took

the later approach and adopted certain interim requirements for public safety licenses along the

Canada and Mexico borders, providing that the licenses are subject to whatever future agreements

the United States develops with the two countries.

Nevertheless, existing mutual agreements with Canada and Mexico for the use of these

bands for UHF television must be recognized until further negotiations are completed. The US

negotiated an agreement with Mexico of DTV operations near the US/Mexican border in July 1998.

The US just negotiated an agreement with Mexico of DTV operations, and limited non-broadcast

operations on 746-806 MHz, near the US/Canadian border in September 2000. Existing agreements

recognize existing TV and/or DTV allotments and planning factors within a specified distance of

the border. The Canadian Letter of Understanding also acknowledges that US plans to use 746-806

MHz for non-broadcast purposes and provides planning criteria (40 dB D/U) to protect Canadian

TV/DTV receivers.

Additionally, public safety facilities within the United States must accept interference from

authorized channel 60-69 TV transmitters in Canada and Mexico in accordance with the existing

agreements. Since the locations of the Canadian and Mexican analog TV assignments and DTV

allotments are known, the public safety applicants can consider the levels of harmful interference to

expect from Canadian and Mexican TV/DTV stations when applying for a license. Both Canada

and Mexico have been informally notified that the Commission has changed its allocated use of TV

channels 60-69, and the Commission will discuss the possibility of mutually compatible spectrum

use with Canada and Mexico.

**Appendix J Meeting Announcements**

This Region 24 700 MHz Regional Planning Committee report is a documentation of the Region 24

700 MHz process. Every item in this document has been reviewed and is pertinent to public safety

700 MHz implementation in Missouri and in accordance with plans for allowing 700 MHz channels

to be used in Missouri’s adjacent states of Arkansas, Oklahoma, Kentucky, Tennessee, Illinois,

Kansas, Nebraska and Iowa. We look forward to working with the regional planning committees in

these states to better the potential for public safety to have the tools available to complete their

mission of protecting life and property in their respective states.

Regards,

Steven J. Makky, Sr.

Chairperson, Region 24 Regional Planning Committee

St. Charles County Sheriff’s Department

December 28, 2007